{"text_format":"1","workbook":"xlsx","n_sheets":46,"sheets":["Общая","Подробная","КПСР 100,110","КПСР 200","КПСР 210","КССР","РА 100,200","RV 103","RV 111","Серия VFM2","Серия VL2","Серия VFS2","Серия VFG2 ","Серия VFGS2_16","Серия VFGS2_25","Серия VFGS2_40","Серия VM2","Серия VRB2","Серия VRG2","Серия VL3","Серия VF3","Серия VRB3","Серия VRG3","Серия AVP","Серия AVA","Серия AVD","Серия AVDS","Серия AFP-VFG2_16","Серия AFP-VFG2_25","Серия AFA-VFG2","Серия AFD-VFG2","RV 113R","RD 103 (D,V)","RV 210-220","RV 212-222","Подбор RV","Подбор RD","Привода","KVs","Перепад","КПСР серия 100","КПСР серия 110","КПСР серия 200","КПСР серия 210","КССР серия 100","РА серия 100,200"],"not_rendered":{"charts":0,"images":77,"macros":1,"external_links":1,"defined_names":138,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Общая","index":0,"n_rows":18,"n_cols":4,"rows_kept":18,"cut":false,"hidden":false,"merged":[[11,2,13,2],[11,3,13,3],[15,0,15,3],[16,0,16,3],[17,0,17,3],[11,0,13,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[4,0,7,0],[8,1,10,1],[8,0,10,0],[8,2,10,2],[8,3,10,3],[4,1,7,1],[11,1,13,1],[4,3,7,3],[4,2,7,2]]}
[null,"Серия 100","Серия 200","Серия 210"]
[]
[]
[]
["Клапаны проходные седельные регулирующие по типу КПСР"]
[]
[]
[]
["Регуляторы давления прямого действия по типу РА"]
[]
[]
["Клапаны смесительные/ разделительные регулирующие по типу КССР"]
[]
[]
[]
["По вопросам продаж и поддержки обращайтесь:"]
[]
["Сайт: http://kpsr.nt-rt.ru  ||  Эл. почта: krp@nt-rt.ru"]

{"sheet":"Подробная","index":1,"n_rows":129,"n_cols":19,"rows_kept":129,"cut":false,"hidden":true,"merged":[[91,15,96,16],[96,13,96,14],[93,17,96,18],[54,9,54,10],[55,9,55,10],[56,9,56,10],[73,9,73,10],[71,3,72,4],[71,5,72,6],[71,7,72,8],[67,11,72,12],[72,13,72,14],[69,15,72,16],[69,17,72,18],[73,15,73,16],[82,3,87,3],[89,3,90,3],[91,3,92,3],[90,17,92,17],[88,15,89,15],[91,5,92,5],[80,9,80,10],[82,9,89,9],[82,13,86,13],[125,9,125,10],[122,9,122,10],[123,9,123,10],[124,9,124,10],[90,9,92,9],[97,9,100,10],[102,9,102,10],[103,9,103,10],[104,9,104,10],[105,9,105,10],[106,9,106,10],[112,9,120,10],[126,9,126,10],[127,9,127,10],[128,9,128,10],[0,5,0,6],[1,5,1,6],[2,5,2,6],[6,5,6,6],[7,5,7,6],[8,5,8,6],[19,5,20,5],[10,5,13,5],[21,5,22,5],[14,5,18,5],[30,5,30,6],[31,5,31,6],[32,5,32,6],[34,5,37,5],[38,5,42,5],[43,5,44,5],[107,9,107,10],[108,9,108,10],[109,9,109,10],[123,5,123,6],[121,9,121,10],[6,17,6,18],[7,17,7,18],[8,17,8,18],[10,15,15,15],[17,15,18,15],[19,15,20,15],[10,13,15,13],[17,13,20,13],[6,13,6,14],[10,17,17,17],[18,17,20,17],[67,15,68,15],[67,13,69,13],[8,9,8,10],[10,9,17,9],[18,9,20,9],[26,9,26,10],[27,9,27,10],[28,9,28,10],[82,17,89,17],[25,15,25,16],[32,17,32,18],[27,13,27,14],[58,13,62,13],[63,13,64,13],[65,13,66,13],[21,15,24,16],[56,17,56,18],[46,11,48,12],[48,13,48,14],[25,9,25,10],[21,9,24,10],[22,11,24,12],[21,13,24,14],[30,11,30,12],[25,17,25,18],[39,11,39,12],[40,11,40,12],[41,11,41,12],[42,11,42,12],[43,11,43,12],[44,11,44,12],[45,11,45,12],[55,13,55,14],[55,15,55,16],[55,17,55,18],[29,15,29,16],[29,17,29,18],[30,15,30,16],[30,17,30,18],[34,11,34,12],[35,11,35,12],[36,11,36,12],[37,11,37,12],[30,13,30,14],[38,11,38,12],[41,13,42,13],[43,13,45,13],[46,13,47,13],[25,13,25,14],[64,7,67,7],[21,17,24,18],[3,3,3,4],[4,3,4,4],[6,3,6,4],[0,1,0,2],[1,1,1,2],[2,1,2,2],[6,1,6,2],[49,17,49,18],[34,7,39,7],[34,15,39,15],[40,7,41,7],[41,15,42,15],[43,15,44,15],[31,17,31,18],[32,7,32,8],[32,11,32,12],[32,13,32,14],[32,15,32,16],[31,15,31,16],[9,11,9,12],[30,9,30,10],[10,7,15,7],[16,7,17,7],[25,7,25,8],[25,5,25,6],[7,1,7,2],[8,1,8,2],[28,1,28,2],[26,1,26,2],[26,3,26,4],[27,3,27,4],[27,1,27,2],[26,5,26,6],[27,5,28,6],[23,3,24,4],[23,5,24,6],[49,5,49,6],[28,7,28,8],[28,11,28,12],[49,11,49,12],[34,3,39,3],[19,7,24,8],[25,1,25,2],[30,1,30,2],[30,3,30,4],[30,7,30,8],[25,3,25,4],[6,7,6,8],[7,7,7,8],[7,9,7,10],[8,7,8,8],[7,3,7,4],[8,3,8,4],[49,13,49,14],[34,13,38,13],[40,3,42,3],[31,7,31,8],[31,11,31,12],[31,13,31,14],[29,0,29,14],[39,13,40,13],[18,11,18,12],[19,11,19,12],[20,11,20,12],[21,11,21,12],[25,11,25,12],[33,11,33,12],[46,1,48,2],[47,3,48,4],[47,5,48,6],[43,7,48,8],[6,9,6,10],[0,0,4,0],[3,1,3,2],[4,1,4,2],[0,11,0,12],[1,11,1,12],[2,11,2,12],[3,11,3,12],[4,11,4,12],[0,7,0,8],[1,7,1,8],[2,7,2,8],[3,7,3,8],[4,7,4,8],[0,9,0,10],[1,9,1,10],[2,9,2,10],[3,9,3,10],[4,9,4,10],[3,5,3,6],[4,5,4,6],[0,3,0,4],[1,3,1,4],[2,3,2,4],[0,17,0,18],[1,17,1,18],[2,17,2,18],[3,17,3,18],[4,17,4,18],[5,0,5,18],[6,15,6,16],[7,15,7,16],[8,15,8,16],[7,13,7,14],[8,13,8,14],[0,15,0,16],[1,15,1,16],[2,15,2,16],[3,15,3,16],[4,15,4,16],[6,11,6,12],[7,11,7,12],[8,11,8,12],[0,13,0,14],[1,13,1,14],[2,13,2,14],[3,13,3,14],[4,13,4,14],[52,9,52,10],[50,5,50,6],[51,5,52,6],[54,5,54,6],[52,13,52,14],[26,0,28,0],[26,7,26,8],[27,7,27,8],[26,11,26,12],[27,11,27,12],[26,13,26,14],[49,1,49,2],[49,3,49,4],[49,7,49,8],[32,1,32,2],[32,3,32,4],[31,1,31,2],[31,3,31,4],[28,3,28,4],[28,13,28,14],[31,9,31,10],[32,9,32,10],[49,9,49,10],[45,5,46,5],[73,13,73,14],[62,5,66,5],[58,7,63,7],[58,15,63,15],[65,15,66,15],[51,3,51,4],[51,7,51,8],[53,0,53,18],[54,1,54,2],[54,3,54,4],[54,7,54,8],[54,11,54,12],[54,13,54,14],[54,15,54,16],[54,17,54,18],[50,0,52,0],[50,1,50,2],[50,3,50,4],[50,7,50,8],[50,11,50,12],[50,13,50,14],[51,13,51,14],[50,9,50,10],[51,9,51,10],[55,1,55,2],[55,3,55,4],[55,7,55,8],[55,11,55,12],[78,13,78,14],[78,15,78,16],[78,17,78,18],[78,9,78,10],[73,17,73,18],[62,11,62,12],[55,5,55,6],[56,5,56,6],[56,1,56,2],[56,3,56,4],[56,7,56,8],[56,11,56,12],[56,13,56,14],[56,15,56,16],[58,5,61,5],[58,3,63,3],[64,3,66,3],[63,11,63,12],[69,7,70,7],[70,13,71,13],[74,0,76,0],[75,11,75,12],[74,13,74,14],[75,13,75,14],[74,15,74,16],[74,17,74,18],[75,17,75,18],[75,9,75,10],[76,9,76,10],[74,3,74,4],[74,7,74,8],[74,11,74,12],[74,1,74,2],[75,5,75,6],[76,5,76,6],[76,17,76,18],[88,1,89,1],[85,1,86,1],[74,9,74,10],[67,5,68,5],[69,5,70,5],[73,5,73,6],[74,5,74,6],[73,1,73,2],[73,3,73,4],[73,7,73,8],[79,5,79,6],[80,5,80,6],[82,5,87,5],[88,5,90,5],[77,0,77,18],[78,1,78,2],[78,3,78,4],[78,7,78,8],[78,11,78,12],[79,13,79,14],[78,5,78,6],[82,7,87,7],[88,7,89,7],[79,17,79,18],[127,5,127,6],[128,5,128,6],[115,7,116,8],[126,1,126,2],[121,3,121,4],[122,3,122,4],[123,3,123,4],[117,5,120,6],[128,1,128,2],[126,7,126,8],[127,7,127,8],[128,7,128,8],[126,3,126,4],[127,3,127,4],[124,5,124,6],[125,5,125,6],[126,5,126,6],[128,3,128,4],[118,3,118,4],[127,1,127,2],[80,1,80,2],[80,3,80,4],[80,7,80,8],[80,11,80,12],[80,13,80,14],[80,15,80,16],[80,17,80,18],[79,1,79,2],[79,3,79,4],[79,7,79,8],[79,15,79,16],[86,11,86,12],[87,11,87,12],[88,11,88,12],[89,11,89,12],[79,9,79,10],[94,13,95,13],[91,13,93,13],[110,9,110,10],[111,9,111,10],[93,11,93,12],[94,11,94,12],[91,11,91,12],[92,11,92,12],[81,11,81,12],[82,11,82,12],[83,11,83,12],[84,11,84,12],[85,11,85,12],[79,11,79,12],[90,11,90,12],[93,9,96,10],[95,11,95,12],[96,11,96,12],[89,13,90,13],[112,1,112,2],[113,1,113,2],[112,7,113,7],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[102,5,102,6],[103,5,103,6],[104,5,104,6],[121,5,121,6],[122,5,122,6],[119,3,120,4],[105,3,105,4],[106,3,106,4],[107,3,107,4],[110,3,110,4],[111,3,111,4],[112,3,112,4],[113,3,113,4],[109,7,111,7],[106,7,108,7],[108,3,108,4],[91,1,92,1],[121,0,125,0],[125,1,125,2],[121,7,121,8],[122,7,122,8],[123,7,123,8],[124,7,124,8],[125,7,125,8],[114,1,114,2],[115,1,115,2],[116,1,116,2],[117,1,117,2],[124,3,124,4],[125,3,125,4],[118,1,120,2],[117,7,120,8],[116,3,116,4],[117,3,117,4],[114,3,114,4],[115,3,115,4],[92,7,96,8],[98,3,98,4],[99,3,99,4],[109,3,109,4],[10,11,10,12],[11,11,11,12],[12,11,12,12],[13,11,13,12],[14,11,14,12],[15,11,15,12],[16,11,16,12],[17,11,17,12],[73,11,73,12],[57,11,57,12],[58,11,58,12],[59,11,59,12],[60,11,60,12],[61,11,61,12],[64,11,64,12],[65,11,65,12],[66,11,66,12],[97,5,97,6],[98,5,98,6],[99,5,99,6],[100,5,100,6],[93,3,96,4],[93,5,96,6],[98,7,98,8],[99,7,99,8],[100,7,100,8],[93,1,96,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[101,0,101,10],[102,1,102,2],[102,7,102,8],[103,1,103,2],[103,3,103,4],[103,7,103,8],[104,1,104,2],[104,3,104,4],[104,7,104,8],[102,3,102,4],[97,0,100,0],[97,1,97,2],[97,3,97,4],[98,1,98,2],[105,1,105,2],[100,3,100,4],[97,7,97,8]]}
["КПСР ","КПСР Групп",null,"Danfoss",null,"Ari Armaturen",null,"POLNA",null,"LDM",null,"ADL",null,"TA",null,"Belimo",null,"Siemens"]
[null,"Серия 100 ",null,"VB 2",null,"STEVI 440",null,"Тип ZH",null,"RV 122",null,"Гранрег КМ125Ф",null,"CV206/216 GG",null,"H6xxN",null,"VVF42xx"]
[null,"Серия 110",null,"VFM 2",null,"STEVI 470/422",null,null,null,"RV 113 R",null,null,null,"CV216",null,"H6xxS",null,"VVF43xx"]
[null,null,null,"VF 2",null,null,null,null,null,"RV 2xx",null,null,null,null,null,"H6xxSP",null,"VVF53xx"]
[null,null,null,"VFG 2 /VFG 21"]
["Тех.характеристики"]
["ДУ max",400,null,250,null,250,null,100,null,150,null,200,null,150,null,150,null,150]
["Давление, бар","16 - 25",null,40,null,"16-40",null,"16-40",null,"6; 16; 25",null,16,null,"6; 16",null,"16; 25",null,16]
["t, °C, max",150,null,200,null,450,null,260,null,150,null,200,null,150,null,150,null,"150; 220"]
["ход штока/kv","ход штока","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv 0,16..40","kv",null,"ход штока, max","kv","ход штока, max","kv","ход штока, max","kv"]
[15,"5; 10"," 0,16; 0,25; 0,4; 0,63; 1; 1,6; 2,5; 3,2; 4",5,"0,25; 0,4; 0,63; 1; 1,6; 2,5; 4",20,"2,5; 4",20,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4",20,"1,6; 2,5; 4",4,null,14,"0,63; 1,25; 1,6; 2,5; 4",15,"0,4; 0,63; 1; 1,6; 2,5;4",20,"0,16 - 4"]
[20,"5; 10","1,6; 2,5; 4; 6,3",5,6.3,null,"2,5; 4; 6,3",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3",null,6.3,5,null,null,"5; 6,3",null,"4; 6,3",null,6.3]
[25,"7; 20","1,6; 2,5; 4,0; 6,3;10",7,10,null,"6,3; 10",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10",null,10,9,null,null,"8; 10",null,"6,3; 10",null,"5,0 - 10"]
[32,"10; 22","6,3; 10; 16",10,16,null,"16; 10",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16",null,16,15,null,null,"12,5; 16",null,"10; 16",null,16]
[40,"10; 25","10; 16; 25",10,25,30,"16; 25",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16; 25",null,25,22,null,null,"20; 25",null,"16; 25",null,"12,5 - 25"]
[50,"10; 32","10; 16; 25; 32; 40",10,40,null,"25; 40",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16; 25; 40",null,40,40,null,null,"31,5; 40",null,"25; 40",null,"31,5; 40"]
[65,32,"25; 32; 40; 63",20,63,null,"40; 63","20; 38","16; 25; 40; 63",null,63,63,null,"20; 30","50; 63","18; 30","58; 63",null,"50; 63"]
[80,40,"40; 63; 80; 100",30,100,null,"63; 100",null,"25; 40; 63; 94",null,100,90,null,50,"80; 100",30,"90; 100",null,"80; 100"]
[100,50,"63; 80; 100; 125;160",30,160,null,"100; 160",38,"94; 125; 160",40,160,136,null,null,"125;160",null,"125; 145",40,"125; 160"]
[125,80,"100; 125; 160; 250",40,250,50,"160; 250",null,null,null,250,230,null,null,250,40,200,null,"200; 250"]
[150,80,"160; 250; 360",40,400,null,"250; 400",null,null,null,360,316,null,null,315,null,320,null,"315; 360; 400"]
[200,80,"250; 360; 450; 630",24,630,65,630,null,null,null,null,555]
[250,80,"400; 630; 800; 1000",24,900,null,1000]
[300,100,"1000; 1250; 1600"]
[400,100,"1250; 1600; 2000; 2500"]
["Разгрузка","Все диаметры",null,"Все диаметры",null,"Все диаметры",null,"Разгружены ду 25-100",null,"Все диаметры",null,null,null,"Все диаметры",null,"частично разгружены ду 65-100",null,"С компенсацией давления с ду 50"]
["КПСР ","Серия 200",null,"VFS 2",null,"STEVI 440",null,"Тип ZH",null,"RV 21x",null,"Гранрег КМ125Ф",null,"CV225"]
[null,null,null,"VEFS 2",null,"STEVI 470/422"]
[null,null,null,"VFGS 2"]
["Тех.характеристики"]
["ДУ max",200,null,250,null,250,null,100,null,400,null,200,null,300]
["Давление, бар",25,null,25,null,"16-40",null,"16-40",null,"16; 40",null,16,null,"16-40"]
["t, °C, max",220,null,250,null,450,null,260,null,"300…500",null,200,null,200]
["ход штока/kv","ход штока","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv","kv",null,"ход штока, max","kv"]
[15,"5; 10"," 0,16; 0,25; 0,4; 0,63; 1; 1,6; 2,5; 3,2; 4",15,"0,4;0,63; 1; 1,6; 2,5; 4",20,"2,5; 4",20,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4",null,null,4,null,20,"0,16; 0,25; 0,4 ;0,63; 1; 1,25; 1,6; 2,5; 4"]
[20,"5; 10","1,6; 2,5; 4; 6,3",null,"4; 6,3",null,"2,5; 4; 6,3",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3",null,null,5,null,null,"2,5; 4; 5; 6,3"]
[25,"7; 20","1,6; 2,5; 4,0; 6,3;10",null,"6,3; 8; 10",null,"6,3; 10",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10",null,null,9,null,null,"5; 6,3; 8; 10"]
[32,"10; 22","6,3; 10; 16",null,"10; 16",null,"16; 10",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16",null,null,15,null,null,"8; 10; 12,5; 16"]
[40,"10; 25","10; 16; 25",null,"16; 20; 25",30,"16; 25",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16; 25",null,null,22,null,null,"12,5; 16; 20;25"]
[50,"10; 32","10; 16; 25; 32; 40",null,"25; 32; 40",null,"25; 40",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16; 25; 40",null,null,40,null,30,"20; 25; 31,5; 40"]
[65,32,"25; 32; 40; 63",40,"40; 50; 63",null,"40; 63","20; 38","16; 25; 40; 63",null,null,63,null,null,"31,5; 40; 50; 63"]
[80,40,"40; 63; 80; 100",null,"63; 80; 100",null,"63; 100",null,"25; 40; 63; 94",null,null,90,null,50,"50; 63; 80; 100"]
[100,50,"63; 80; 100; 125;160",null,"100; 125; 145",null,"100; 160",38,"94; 125; 160",null,null,136,null,null,"80; 100; 125; 160"]
[125,80,"100; 125; 160; 250",null,"125; 160",50,"160; 250",null,null,null,null,230,null,60,"125; 160; 200; 250"]
[150,80,"160; 250; 360",null,"280; 320",null,"250; 400",null,null,null,null,316,null,null,"200; 250; 315; 400"]
[200,80,"250; 360; 450; 630",null,"320; 450",65,630,null,null,null,null,555,null,null,"315; 400; 500; 630"]
[250,null,null,null,"400; 630",null,1000,null,null,null,null,null,null,80,"400; 500; 630; 800"]
[300,null,null,null,null,null,null,null,null,null,null,null,null,null,"630; 800; 1000; 1250"]
[400]
["Разгрузка","с ду 65",null,"Все диаметры",null,"Все диаметры",null,"Разгружены ду 25-100",null,"Все диаметры",null,null,null,"Все диаметры"]
["КПСР ","Серия 210",null,"VFG 2 /VFG 21",null,"STEVI 440",null,"Тип ZH",null,"RV 21x",null,"Гранрег КМ127Ф",null,"CV225"]
[null,null,null,"VFGS 2",null,"STEVI 470/422",null,"Тип Z",null,null,null,null,null,"CV240S"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"CV240E"]
["Тех.характеристики"]
["ДУ max",400,null,250,null,250,null,250,null,400,null,100,null,300,null,150,null,150]
["Давление, бар",25,null,"16 - 25",null,"16-40",null,"10; 16; 25; 40",null,"16; 40",null,40,null,"16-40",null,"16; 25",null,16]
["t, °C, max",260,null,250,null,450,null,450,null,"300…500",null,300,null,200,null,150,null,"150; 220"]
["ход штока/kv","ход штока","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv",null,null,"kv",null,"ход штока, max","kv","ход штока, max","kv","ход штока, max","kv"]
[15,"5; 10"," 0,16; 0,25; 0,4; 0,63; 1; 1,6; 2,5; 3,2; 4",15,"0,4;0,63; 1; 1,6; 2,5; 4",20,"2,5; 4",20,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; 0,4; 0,63; 1; 1,6; 2,5; 4",null,null,4,null,20,"0,16; 0,25; 0,4 ;0,63; 1; 1,25; 1,6; 2,5; 4",15,"0,4; 0,63; 1; 1,6; 2,5;4",null,"0,16 - 4"]
[20,"5; 10","1,6; 2,5; 4; 6,3",null,"4; 6,3",null,"2,5; 4; 6,3",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3",null,null,5,null,null,"2,5; 4; 5; 6,3",null,"4; 6,3",null,6.3]
[25,"7; 20","1,6; 2,5; 4,0; 6,3;10",null,"6,3; 8; 10",null,"6,3; 10",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10",null,null,9,null,null,"5; 6,3; 8; 10",null,"6,3; 10",null,"5,0 - 10"]
[32,"10; 22","6,3; 10; 16",null,"10; 16",null,"16; 10",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16",null,null,15,null,null,"8; 10; 12,5; 16",null,"10; 16",null,16]
[40,"10; 25","10; 16; 25",null,"16; 20; 25",30,"16; 25",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16; 25",null,null,22,null,null,"12,5; 16; 20;25",null,"16; 25",null,"12,5 - 25"]
[50,"10; 32","10; 16; 25; 32; 40",null,"25; 32; 40",null,"25; 40",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16; 25; 40",null,null,40,null,30,"20; 25; 31,5; 40",null,"25; 40",null,"31,5; 40"]
[65,32,"25; 32; 40; 63",40,"40; 50; 63",null,"40; 63","20; 38","16; 25; 40; 63",null,null,63,null,null,"31,5; 40; 50; 63","18; 30","58; 63",null,"50; 63"]
[80,40,"40; 63; 80; 100",null,"63; 80; 100",null,"63; 100",null,"25; 40; 63; 94",null,null,90,null,50,"50; 63; 80; 100",30,"90; 100",null,"80; 100"]
[100,50,"63; 80; 100; 125;160",null,"100; 125; 145",null,"100; 160",null,"40; 63; 94; 125; 160",null,null,136,null,null,"80; 100; 125; 160",null,"125; 145",null,"125; 160"]
[125,80,"100; 125; 160; 250",null,"125; 160",50,"160; 250",null,"40; 63; 94; 125; 160",null,null,null,null,60,"125; 160; 200; 250",40,200,null,"200; 250"]
[150,80,"160; 250; 360",null,"280; 320",null,"250; 400","38; 50"," 63; 94; 125; 160; 250; 320",null,null,null,null,null,"200; 250; 315; 400",null,320,null,"315; 360; 400"]
[200,80,"250; 360; 450; 630",null,"320; 450",65,630,"38; 50; 63","94; 125; 160; 250; 320; 500",null,null,null,null,null,"315; 400; 500; 630"]
[250,80,"400; 630; 800; 1000",null,"400; 630",null,1000,null,"125; 160; 250; 320; 500; 630",null,null,null,null,80,"400; 500; 630; 800"]
[300,100,"1000; 1250; 1600",null,null,null,null,null,null,null,null,null,null,null,"630; 800; 1000; 1250"]
[400,100,"1250; 1600; 2000; 2500"]
["Разгрузка","с ду 50",null,"Все диаметры",null,"Все диаметры",null,"Разгружены ду 40-250",null,"Все диаметры",null,null,null,"Все диаметры",null,"Частично разгружены ду 65-100",null,"С компенсацией давления с ду 50"]
["КССР","Серия 100",null,"VF3",null,"STEVI 450",null,"Тип Z3",null,"RV 113 M",null,"Гранрег КМ 307Ф",null,"CV306/316 GG",null,"H7xxR",null,"VXF42xx"]
[null,null,null,null,null,null,null,null,null,null,null,"Гранрег КМ317Ф",null,"CV316",null,null,null,"VXF43xx"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VXF53xx"]
["Тех.характеристики"]
["ДУ max",150,null,150,null,300,null,150,null,150,null,300,null,200,null,120,null,220]
["Давление, бар",16,null,16,null,"16-40",null,"16; 25; 40",null,"6; 16",null,16,null,"6; 16",null,6,null,"16; 25"]
["t, °C, max",150,null,200,null,150,null,450,null,150,null,230,null,300,null,100,null,150]
["ход штока/kv","ход штока","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv","kv",null,"ход штока, max","kv","ход штока, max","kv","ход штока, max","kv"]
[15,10," 0,16; 0,25; 0,4; 0,63; 1; 1,6; 2,5;  4",15,"0,63; 1; 1,6; 2,5; 4",20,"2,5; 4",20,"0,63; 1; 1,6; 2,5; 4",20,"1,6; 2,5; 4",4,null,"14; 20","0,63; 1,25; 1,6; 2,5; 4",15,"0,63; 1; 1,6; 2,5;4",20,"1,6; 2,5; 4"]
[20,15,"1,6; 2,5; 4; 6,3",null,6.3,null," 4; 6,3",null,"0,63; 1; 1,6; 2,5; 4; 6,3",null,6.3,6.3,null,null,"2,5; 4; 5; 6,3",null,6.3,null,6.3]
[25,20,"1,6; 2,5; 4,0; 6,3;10",null,10,null,"6,3; 10",null,"0,63; 1; 1,6; 2,5; 4; 6,3; 10",null,10,10,null,null,"5; 6,3; 8; 10",null,10,null,"6,3; 10"]
[32,22,"6,3; 10; 16",null,16,null,"16; 10",null,"6,3; 10; 16",null,16,16,null,null,"8; 10; 12,5; 16",null,16,null,16]
[40,null,"10; 16; 25",null,25,null,"16; 25",null,"10; 16; 25",null,25,25,null,null,"12,5; 16; 20; 25",null,25,null,"16; 25"]
[50,25,"10; 16; 25; 40",null,40,null,"25; 40",null,"16; 25; 40",null,40,40,null,"14; 30","20; 25; 31,5; 40",null,40,null,"31,5; 40"]
[65,32,"25; 32; 40; 63",20,63,30,"40; 63","20; 38","25; 40; 63",null,63,63,null,"20; 30","31,5; 40; 50; 63",18,58,null,"50; 63"]
[80,null,"40; 63;100",30,100,null,"63; 100",null,"40; 63; 94",null,100,"70; 100",null,50,"50; 63; 80; 100",null,90,null,"80; 100"]
[100,null,"63; 80; 100; 125;160",null,145,null,"100; 160",38,"63; 94; 125; 160",40,160,"130; 160",null,null,"80; 100; 125;160",30,145,40,"125; 160"]
[125,null,"100; 125; 160; 250",40,220,50,"160; 250","38; 50","125; 160; 250; 320",null,250,"200; 230",null,60,"125; 160; 200; 250",null,null,null,"200; 250"]
[150,null,"160; 250; 360",null,320,null,"250; 320",null,null,null,360,"270; 340",null,null,"200; 250; 315; 400",null,null,null,"315; 400"]
[200,null,null,null,null,null,null,null,null,null,null,"600; 420",null,null,"315; 400; 500; 630"]
[250,null,null,null,null,null,null,null,null,null,null,"900; 640",null,80,"400; 500; 630; 800"]
[300,null,null,null,null,null,null,null,null,null,null,"1200; 930",null,null,"630; 800; 1000; 1250"]
[]
["РА","Серия 100",null,"VFG2 + AFD",null,"ARI-PREDU",null,"Тип ZSN1",null,"RD 122"]
[null,"Серия 200",null,"VFGS2 + AFD",null,null,null,"Тип ZSN3"]
[null,null,null," AVA",null,null,null,"Тип ZSN5"]
[null,null,null,"AVP",null,null,null,"Тип ZSN7"]
["Тех.характеристики"]
["ДУ max",200,null,250,null,150,null,150,null,50]
["Давление, бар","16 ; 25",null,"16-40",null,"16-40",null,"16; 25; 40",null,25]
["t, °C, max",220,null,350,null,350,null,200,null,150]
["kv","kv",null,"kv",null,"ход штока, max","kv","ход штока, max","kv","kv"]
[15," 0,16; 0,25; 0,4; 0,63; 1; 1,6; 2,5; 3,2; 4",null,"1,6; 4; 2,5",null,4,"0,1; 0,4; 1; 2,5; 3,2",6,"1; 1,6; 2,5; 3,2","2,5; 5"]
[20,"1,6; 2,5; 4; 6,3",null,"6,3: 4",null,5,"0,1; 0,4; 1; 2,5; 4; 5",null,"1,6; 2,5; 3,2; 5",8]
[25,"1,6; 2,5; 4,0; 6,3; 8; 10",null,"8; 6,3",null,6,"0,1; 0,4; 1; 2,5; 4; 6,3; 8",null,"2,5; 3,2; 5; 8",10]
[32,"6,3; 10; 16",null,"12,5; 16; 10",null,8,12.5,8,"12,5; 5",15]
[40,"10; 16; 20; 25",null,"20; 16",null,8,20,null,"8; 20",21]
[50,"10; 16; 25; 32; 40",null,"32;25",null,10,32,null,"12,5; 32",32]
[65,"25; 40; 50; 63",null,"50; 40",null,11,50,12,"20; 50"]
[80,"40; 63; 80; 100",null,"80; 63",null,13,80,null,"32; 80"]
[100,"63; 100; 125",null,"125; 100",null,16,125,14,"50; 125"]
[125,"100; 125; 160",null,"160; 125",null,19,190,"спец. Исполнение, по индивид согласованию"]
[150,"160; 280",null,"280; 200",null,22,280]
[200,"250; 360; 450; 630",null,"320; 225"]
[250,null,null,"400; 280"]
[300]
[400]
[" Диапазон настройки, Мпа","0 - (0,01…0,1)",null,"(0,8…1,6)",null,"(0,2…0,6)",null,"(0,01…0,04)",null,"ду 15-25"]
[null,"1 - (0,04...0,16)",null,"(0,3…1,2)",null,"(0,5…1,2)",null,"(0,02…0,08)",null,"(0,015…0,06)"]
[null,"2 - (0,1…0,4)",null,"(0,1…0,6)",null,"(0,8…2,5)",null,"(0,04…0,16)",null,"(0,03…0,21)"]
[null,"3  - (0,3…0,7)",null,"(0,05…0,3)",null,"(2…5)",null,"(0,04…0,16)",null,"(0,06…0,4)"]
[null,"4 - (0,6…1,2)",null,"(0,01…0,07)",null,"(4,5…10)",null,"(0,08…0,32)",null,"ду 32-50"]
[null,null,null,"(0,015…0,15)",null,"(8…16)",null,"(0,1…0,4)",null,"(0,025…0,07)"]
[null,null,null,"(0,005…0,035)",null,null,null,"(0,2…0,8)",null,"(0,04…0,22)"]
[null,null,null,null,null,null,null,"(0,28…1,12)",null,"(0,07…0,41)"]

{"sheet":"КПСР 100,110","index":2,"n_rows":27,"n_cols":19,"rows_kept":27,"cut":false,"hidden":true,"merged":[[22,15,25,16],[22,17,25,18],[0,0,0,18],[26,13,26,14],[26,15,26,16],[26,17,26,18],[26,9,26,10],[24,3,25,4],[24,5,25,6],[20,7,25,8],[22,9,25,10],[23,11,25,12],[22,13,25,14],[22,5,23,5],[22,11,22,12],[26,1,26,2],[26,3,26,4],[26,5,26,6],[26,7,26,8],[26,11,26,12],[18,13,21,13],[18,15,19,15],[19,9,21,9],[19,11,19,12],[10,11,10,12],[11,5,14,5],[11,7,16,7],[11,9,18,9],[11,11,11,12],[11,13,16,13],[11,15,16,15],[11,17,18,17],[19,17,21,17],[20,5,21,5],[20,11,20,12],[20,15,21,15],[21,11,21,12],[12,11,12,12],[13,11,13,12],[14,11,14,12],[15,5,19,5],[15,11,15,12],[16,11,16,12],[17,7,18,7],[17,11,17,12],[18,11,18,12],[8,13,8,14],[8,15,8,16],[8,17,8,18],[9,1,9,2],[9,3,9,4],[9,5,9,6],[9,7,9,8],[9,9,9,10],[9,11,9,12],[9,13,9,14],[8,1,8,2],[8,3,8,4],[8,5,8,6],[8,7,8,8],[8,9,8,10],[8,11,8,12],[9,15,9,16],[9,17,9,18],[5,15,5,16],[5,17,5,18],[6,0,6,18],[7,1,7,2],[7,3,7,4],[7,5,7,6],[7,7,7,8],[7,9,7,10],[7,11,7,12],[7,13,7,14],[7,15,7,16],[7,17,7,18],[1,0,5,0],[5,1,5,2],[5,3,5,4],[5,5,5,6],[5,7,5,8],[5,9,5,10],[5,11,5,12],[5,13,5,14],[3,17,3,18],[4,1,4,2],[4,3,4,4],[4,5,4,6],[4,7,4,8],[4,9,4,10],[4,11,4,12],[4,13,4,14],[4,15,4,16],[4,17,4,18],[3,1,3,2],[3,3,3,4],[3,5,3,6],[3,7,3,8],[3,9,3,10],[3,11,3,12],[3,13,3,14],[3,15,3,16],[1,17,1,18],[2,1,2,2],[2,3,2,4],[2,5,2,6],[2,7,2,8],[2,9,2,10],[2,11,2,12],[2,13,2,14],[2,15,2,16],[2,17,2,18],[1,1,1,2],[1,3,1,4],[1,5,1,6],[1,7,1,8],[1,9,1,10],[1,11,1,12],[1,13,1,14],[1,15,1,16]]}
["Клапаны запорно-регулирующие двухходовые, серия 100,110"]
["КПСР ","КПСР Групп",null,"Danfoss",null,"Ari Armaturen",null,"POLNA",null,"LDM",null,"ADL",null,"TA",null,"Belimo",null,"Siemens"]
[null,"Серия 100 ",null,"VB 2",null,"STEVI 440",null,"Тип ZH",null,"RV 122",null,"Гранрег КМ125Ф",null,"CV206/216 GG",null,"H6xxN",null,"VVF42xx"]
[null,"Серия 110",null,"VFM 2",null,"STEVI 470/422",null,null,null,"RV 113 R",null,null,null,"CV216",null,"H6xxS",null,"VVF43xx"]
[null,null,null,"VF 2",null,null,null,null,null,"RV 2xx",null,null,null,null,null,"H6xxSP",null,"VVF53xx"]
[null,null,null,"VFG 2 /VFG 21"]
["Тех.характеристики"]
["ДУ max",400,null,250,null,250,null,100,null,150,null,200,null,150,null,150,null,150]
["Давление, бар","16 - 25",null,40,null,"16-40",null,"16-40",null,"6; 16; 25",null,16,null,"6; 16",null,"16; 25",null,16]
["t, °C, max",150,null,200,null,450,null,260,null,150,null,200,null,150,null,150,null,"150; 220"]
["ход штока/kv","ход штока","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv 0,16..40","kv",null,"ход штока, max","kv","ход штока, max","kv","ход штока, max","kv"]
[15,"5; 10"," 0,16; 0,25; 0,4; 0,63; 1; 1,6; 2,5; 3,2; 4",5,"0,25; 0,4; 0,63; 1; 1,6; 2,5; 4",20,"2,5; 4",20,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4",20,"1,6; 2,5; 4",4,null,14,"0,63; 1,25; 1,6; 2,5; 4",15,"0,4; 0,63; 1; 1,6; 2,5;4",20,"0,16 - 4"]
[20,"5; 10","1,6; 2,5; 4; 6,3",5,6.3,null,"2,5; 4; 6,3",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3",null,6.3,5,null,null,"5; 6,3",null,"4; 6,3",null,6.3]
[25,"7; 20","1,6; 2,5; 4,0; 6,3;10",7,10,null,"6,3; 10",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10",null,10,9,null,null,"8; 10",null,"6,3; 10",null,"5,0 - 10"]
[32,"10; 22","6,3; 10; 16",10,16,null,"16; 10",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16",null,16,15,null,null,"12,5; 16",null,"10; 16",null,16]
[40,"10; 25","10; 16; 25",10,25,30,"16; 25",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16; 25",null,25,22,null,null,"20; 25",null,"16; 25",null,"12,5 - 25"]
[50,"10; 32","10; 16; 25; 32; 40",10,40,null,"25; 40",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16; 25; 40",null,40,40,null,null,"31,5; 40",null,"25; 40",null,"31,5; 40"]
[65,32,"25; 32; 40; 63",20,63,null,"40; 63","20; 38","16; 25; 40; 63",null,63,63,null,"20; 30","50; 63","18; 30","58; 63",null,"50; 63"]
[80,40,"40; 63; 80; 100",30,100,null,"63; 100",null,"25; 40; 63; 94",null,100,90,null,50,"80; 100",30,"90; 100",null,"80; 100"]
[100,50,"63; 80; 100; 125;160",30,160,null,"100; 160",38,"94; 125; 160",40,160,136,null,null,"125;160",null,"125; 145",40,"125; 160"]
[125,80,"100; 125; 160; 250",40,250,50,"160; 250",null,null,null,250,230,null,null,250,40,200,null,"200; 250"]
[150,80,"160; 250; 360",40,400,null,"250; 400",null,null,null,360,316,null,null,315,null,320,null,"315; 360; 400"]
[200,80,"250; 360; 450; 630",24,630,65,630,null,null,null,null,555]
[250,80,"400; 630; 800; 1000",24,900,null,1000]
[300,100,"1000; 1250; 1600"]
[400,100,"1250; 1600; 2000; 2500"]
["Разгрузка","Все диаметры",null,"Все диаметры",null,"Все диаметры",null,"Разгружены ду 25-100",null,"Все диаметры",null,null,null,"Все диаметры",null,"Частично разгружены ду 65-100",null,"С компенсацией давления с ду 50"]

{"sheet":"КПСР 200","index":3,"n_rows":26,"n_cols":15,"rows_kept":26,"cut":false,"hidden":true,"merged":[[0,0,0,14],[25,13,25,14],[24,17,24,18],[1,0,4,0],[22,1,24,2],[23,3,24,4],[23,5,24,6],[19,7,24,8],[22,11,24,12],[24,13,24,14],[25,1,25,2],[25,3,25,4],[25,5,25,6],[25,7,25,8],[25,9,25,10],[25,11,25,12],[19,5,20,5],[19,11,19,12],[19,13,21,13],[18,15,19,15],[20,11,20,12],[21,5,22,5],[21,11,21,12],[22,13,23,13],[16,3,18,3],[16,7,17,7],[16,11,16,12],[17,11,17,12],[17,13,18,13],[16,15,17,15],[18,11,18,12],[12,11,12,12],[13,11,13,12],[14,5,18,5],[14,11,14,12],[15,11,15,12],[15,13,16,13],[7,15,7,16],[7,17,7,18],[9,11,9,12],[10,3,15,3],[10,5,13,5],[10,7,15,7],[10,11,10,12],[10,13,14,13],[9,15,14,15],[11,11,11,12],[7,13,7,14],[8,1,8,2],[8,3,8,4],[8,5,8,6],[8,7,8,8],[8,9,8,10],[8,11,8,12],[8,13,8,14],[7,1,7,2],[7,3,7,4],[7,5,7,6],[7,7,7,8],[7,9,7,10],[7,11,7,12],[4,17,4,18],[6,1,6,2],[6,3,6,4],[6,5,6,6],[6,7,6,8],[6,9,6,10],[6,11,6,12],[6,13,6,14],[5,15,5,16],[5,17,5,18],[4,7,4,8],[4,9,4,10],[4,11,4,12],[4,13,4,14],[5,0,5,14],[4,15,4,16],[6,15,6,16],[6,17,6,18],[1,1,1,2],[1,3,1,4],[1,5,1,6],[1,7,1,8],[1,9,1,10],[1,11,1,12],[1,13,1,14],[2,13,2,14],[3,1,3,2],[3,3,3,4],[3,5,4,6],[3,7,3,8],[3,9,3,10],[3,11,3,12],[3,13,3,14],[4,1,4,2],[4,3,4,4],[2,1,2,2],[2,3,2,4],[2,5,2,6],[2,7,2,8],[2,9,2,10],[2,11,2,12]]}
["Клапаны запорно-регулирующие двухходовые, серия 200"]
["КПСР ","КПСР Групп",null,"Danfoss",null,"Ari Armaturen",null,"POLNA",null,"LDM",null,"ADL",null,"TA"]
[null,"Серия 200",null,"VFS 2",null,"STEVI 440",null,"Тип ZH",null,"RV 21x",null,"Гранрег КМ125Ф",null,"CV225"]
[null,null,null,"VEFS 2",null,"STEVI 470/422"]
[null,null,null,"VFGS 2"]
["Тех.характеристики"]
["ДУ max",200,null,250,null,250,null,100,null,400,null,200,null,300]
["Давление, бар",25,null,25,null,"16-40",null,"16-40",null,"16; 40",null,16,null,"16-40"]
["t, °C, max",220,null,250,null,450,null,260,null,"300…500",null,200,null,200]
["ход штока/kv","ход штока","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv","kv",null,"ход штока, max","kv"]
[15,"5; 10"," 0,16; 0,25; 0,4; 0,63; 1; 1,6; 2,5; 3,2; 4",15,"0,4;0,63; 1; 1,6; 2,5; 4",20,"2,5; 4",20,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4",null,null,4,null,20,"0,16; 0,25; 0,4 ;0,63; 1; 1,25; 1,6; 2,5; 4"]
[20,"5; 10","1,6; 2,5; 4; 6,3",null,"4; 6,3",null,"2,5; 4; 6,3",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3",null,null,5,null,null,"2,5; 4; 5; 6,3"]
[25,"7; 20","1,6; 2,5; 4,0; 6,3;10",null,"6,3; 8; 10",null,"6,3; 10",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10",null,null,9,null,null,"5; 6,3; 8; 10"]
[32,"10; 22","6,3; 10; 16",null,"10; 16",null,"16; 10",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16",null,null,15,null,null,"8; 10; 12,5; 16"]
[40,"10; 25","10; 16; 25",null,"16; 20; 25",30,"16; 25",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16; 25",null,null,22,null,null,"12,5; 16; 20;25"]
[50,"10; 32","10; 16; 25; 32; 40",null,"25; 32; 40",null,"25; 40",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16; 25; 40",null,null,40,null,30,"20; 25; 31,5; 40"]
[65,32,"25; 32; 40; 63",40,"40; 50; 63",null,"40; 63","20; 38","16; 25; 40; 63",null,null,63,null,null,"31,5; 40; 50; 63"]
[80,40,"40; 63; 80; 100",null,"63; 80; 100",null,"63; 100",null,"25; 40; 63; 94",null,null,90,null,50,"50; 63; 80; 100"]
[100,50,"63; 80; 100; 125;160",null,"100; 125; 145",null,"100; 160",38,"94; 125; 160",null,null,136,null,null,"80; 100; 125; 160"]
[125,80,"100; 125; 160; 250",null,"125; 160",50,"160; 250",null,null,null,null,230,null,60,"125; 160; 200; 250"]
[150,80,"160; 250; 360",null,"280; 320",null,"250; 400",null,null,null,null,316,null,null,"200; 250; 315; 400"]
[200,80,"250; 360; 450; 630",null,"320; 450",65,630,null,null,null,null,555,null,null,"315; 400; 500; 630"]
[250,null,null,null,"400; 630",null,1000,null,null,null,null,null,null,80,"400; 500; 630; 800"]
[300,null,null,null,null,null,null,null,null,null,null,null,null,null,"630; 800; 1000; 1250"]
[400]
["Разгрузка","с ду 65",null,"Все диаметры",null,"Все диаметры",null,"Разгружены ду 25-100",null,"Все диаметры",null,null,null,"Все диаметры"]

{"sheet":"КПСР 210","index":4,"n_rows":26,"n_cols":19,"rows_kept":26,"cut":false,"hidden":true,"merged":[[0,0,0,18],[8,9,8,10],[25,9,25,10],[19,11,24,12],[24,13,24,14],[21,15,24,16],[21,17,24,18],[25,15,25,16],[25,13,25,14],[25,17,25,18],[1,15,1,16],[1,17,1,18],[2,15,2,16],[2,17,2,18],[3,15,3,16],[3,17,3,18],[4,15,4,16],[4,17,4,18],[25,1,25,2],[25,3,25,4],[25,5,25,6],[25,7,25,8],[25,11,25,12],[23,3,24,4],[19,15,20,15],[21,5,22,5],[21,7,22,7],[22,13,23,13],[16,3,18,3],[16,7,19,7],[16,11,16,12],[17,11,17,12],[17,13,18,13],[17,15,18,15],[18,11,18,12],[19,5,20,5],[19,13,21,13],[12,11,12,12],[13,11,13,12],[14,5,18,5],[14,11,14,12],[15,11,15,12],[15,13,16,13],[9,11,9,12],[23,5,24,6],[23,7,24,8],[10,3,15,3],[10,5,13,5],[10,7,15,7],[10,11,10,12],[10,13,14,13],[7,15,7,16],[7,17,7,18],[8,1,8,2],[8,3,8,4],[8,5,8,6],[8,7,8,8],[8,11,8,12],[8,13,8,14],[8,15,8,16],[8,17,8,18],[7,1,7,2],[7,3,7,4],[7,5,7,6],[7,7,7,8],[7,11,7,12],[7,13,7,14],[7,9,7,10],[10,15,15,15],[11,11,11,12],[5,0,5,18],[6,1,6,2],[6,3,6,4],[6,5,6,6],[6,7,6,8],[6,11,6,12],[6,13,6,14],[6,15,6,16],[6,17,6,18],[6,9,6,10],[3,13,3,14],[4,9,4,10],[4,13,4,14],[1,11,1,12],[1,13,1,14],[2,1,2,2],[2,3,2,4],[2,5,2,6],[2,7,2,8],[2,9,2,10],[2,11,2,12],[2,13,2,14],[1,0,4,0],[1,1,1,2],[1,3,1,4],[1,5,1,6],[1,7,1,8],[1,9,1,10],[3,3,3,4],[3,5,4,6],[3,7,3,8],[3,9,3,10]]}
["Клапаны запорно-регулирующие двухходовые, серия 210"]
["КПСР ","КПСР Групп",null,"Danfoss",null,"Ari Armaturen",null,"POLNA",null,"LDM",null,"ADL",null,"TA",null,"Belimo",null,"Siemens"]
[null,"Серия 210",null,"VFG 2 /VFG 21",null,"STEVI 440",null,"Тип ZH",null,"RV 21x",null,"Гранрег КМ127Ф",null,"CV225",null,"H6xxN",null,"VVF42xx"]
[null,null,null,"VFGS 2",null,"STEVI 470/422",null,"Тип Z",null,null,null,null,null,"CV240S",null,"H6xxS",null,"VVF43xx"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"CV240E",null,"H6xxSP",null,"VVF53xx"]
["Тех.характеристики"]
["ДУ max",400,null,250,null,250,null,250,null,400,null,100,null,300,null,150,null,150]
["Давление, бар",25,null,"16 - 25",null,"16-40",null,"10; 16; 25; 40",null,"16; 40",null,40,null,"16-40",null,"16; 25",null,16]
["t, °C, max",260,null,250,null,450,null,450,null,"300…500",null,300,null,200,null,150,null,"150; 220"]
["ход штока/kv","ход штока","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv",null,null,"kv",null,"ход штока, max","kv","ход штока, max","kv","ход штока, max","kv"]
[15,"5; 10"," 0,16; 0,25; 0,4; 0,63; 1; 1,6; 2,5; 3,2; 4",15,"0,4;0,63; 1; 1,6; 2,5; 4",20,"2,5; 4",20,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; 0,4; 0,63; 1; 1,6; 2,5; 4",null,null,4,null,20,"0,16; 0,25; 0,4 ;0,63; 1; 1,25; 1,6; 2,5; 4",15,"0,4; 0,63; 1; 1,6; 2,5;4",null,"0,16 - 4"]
[20,"5; 10","1,6; 2,5; 4; 6,3",null,"4; 6,3",null,"2,5; 4; 6,3",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3",null,null,5,null,null,"2,5; 4; 5; 6,3",null,"4; 6,3",null,6.3]
[25,"7; 20","1,6; 2,5; 4,0; 6,3;10",null,"6,3; 8; 10",null,"6,3; 10",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10",null,null,9,null,null,"5; 6,3; 8; 10",null,"6,3; 10",null,"5,0 - 10"]
[32,"10; 22","6,3; 10; 16",null,"10; 16",null,"16; 10",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16",null,null,15,null,null,"8; 10; 12,5; 16",null,"10; 16",null,16]
[40,"10; 25","10; 16; 25",null,"16; 20; 25",30,"16; 25",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16; 25",null,null,22,null,null,"12,5; 16; 20;25",null,"16; 25",null,"12,5 - 25"]
[50,"10; 32","10; 16; 25; 32; 40",null,"25; 32; 40",null,"25; 40",null,"0,01; 0,016; 0,025; 0,04; 0,063; 0,1; 0,16; 0,25; ,04; 0,63,; 1; 1,6; 2,5; 4; 6,3; 10; 16; 25; 40",null,null,40,null,30,"20; 25; 31,5; 40",null,"25; 40",null,"31,5; 40"]
[65,32,"25; 32; 40; 63",40,"40; 50; 63",null,"40; 63","20; 38","16; 25; 40; 63",null,null,63,null,null,"31,5; 40; 50; 63","18; 30","58; 63",null,"50; 63"]
[80,40,"40; 63; 80; 100",null,"63; 80; 100",null,"63; 100",null,"25; 40; 63; 94",null,null,90,null,50,"50; 63; 80; 100",30,"90; 100",null,"80; 100"]
[100,50,"63; 80; 100; 125;160",null,"100; 125; 145",null,"100; 160",null,"40; 63; 94; 125; 160",null,null,136,null,null,"80; 100; 125; 160",null,"125; 145",null,"125; 160"]
[125,80,"100; 125; 160; 250",null,"125; 160",50,"160; 250",null,"40; 63; 94; 125; 160",null,null,null,null,60,"125; 160; 200; 250",40,200,null,"200; 250"]
[150,80,"160; 250; 360",null,"280; 320",null,"250; 400","38; 50"," 63; 94; 125; 160; 250; 320",null,null,null,null,null,"200; 250; 315; 400",null,320,null,"315; 360; 400"]
[200,80,"250; 360; 450; 630",null,"320; 450",65,630,"38; 50; 63","94; 125; 160; 250; 320; 500",null,null,null,null,null,"315; 400; 500; 630"]
[250,80,"400; 630; 800; 1000",null,"400; 630",null,1000,null,"125; 160; 250; 320; 500; 630",null,null,null,null,80,"400; 500; 630; 800"]
[300,100,"1000; 1250; 1600",null,null,null,null,null,null,null,null,null,null,null,"630; 800; 1000; 1250"]
[400,100,"1250; 1600; 2000; 2500"]
["Разгрузка","с ду 50",null,"Все диаметры",null,"Все диаметры",null,"Разгружены ду 40-250",null,"Все диаметры",null,null,null,"Все диаметры",null,"частично разгружены ду 65-100",null,"С компенсацией давления с ду 50"]

{"sheet":"КССР","index":5,"n_rows":24,"n_cols":19,"rows_kept":24,"cut":false,"hidden":true,"merged":[[24,13,24,14],[19,15,24,16],[21,17,24,18],[0,0,0,18],[24,11,24,12],[21,1,24,2],[21,3,24,4],[21,5,24,6],[20,7,24,8],[21,9,24,10],[21,11,21,12],[22,11,22,12],[22,13,23,13],[23,11,23,12],[18,17,20,17],[19,1,20,1],[13,11,13,12],[14,11,14,12],[15,11,15,12],[16,15,17,15],[17,3,18,3],[17,11,17,12],[17,13,18,13],[18,9,20,9],[18,11,18,12],[19,3,20,3],[19,5,20,5],[19,11,19,12],[19,13,21,13],[20,11,20,12],[16,1,17,1],[16,5,18,5],[16,7,17,7],[16,11,16,12],[8,17,8,18],[9,11,9,12],[10,3,15,3],[10,5,15,5],[10,7,15,7],[10,9,17,9],[10,11,10,12],[10,13,14,13],[10,17,17,17],[11,11,11,12],[12,11,12,12],[13,1,14,1],[7,15,7,16],[7,17,7,18],[8,1,8,2],[8,3,8,4],[8,5,8,6],[8,7,8,8],[8,9,8,10],[8,11,8,12],[8,13,8,14],[8,15,8,16],[6,13,6,14],[6,15,6,16],[6,17,6,18],[7,1,7,2],[7,3,7,4],[7,5,7,6],[7,7,7,8],[7,9,7,10],[7,11,7,12],[7,13,7,14],[6,1,6,2],[6,3,6,4],[6,5,6,6],[6,7,6,8],[6,9,6,10],[6,11,6,12],[1,9,1,10],[4,17,4,18],[3,17,3,18],[4,5,4,6],[4,9,4,10],[2,13,2,14],[2,15,2,16],[2,17,2,18],[3,5,3,6],[3,9,3,10],[3,11,3,12],[3,13,3,14],[1,0,4,0],[5,0,5,18],[1,11,1,12],[1,13,1,14],[1,15,1,16],[1,17,1,18],[2,1,2,2],[2,3,2,4],[2,5,2,6],[2,7,2,8],[2,9,2,10],[2,11,2,12],[1,1,1,2],[1,3,1,4],[1,5,1,6],[1,7,1,8]]}
["Клапаны смесительные трехходовые"]
["КССР","КПСР Групп",null,"Danfoss",null,"Ari Armaturen",null,"POLNA",null,"LDM",null,"ADL",null,"TA",null,"Belimo",null,"Siemens"]
[null,"Серия 100",null,"VF3",null,"STEVI 450",null,"Тип Z3",null,"RV 113 M",null,"Гранрег КМ 307Ф",null,"CV306/316 GG",null,"H7xxR",null,"VXF42xx"]
[null,null,null,null,null,null,null,null,null,null,null,"Гранрег КМ317Ф",null,"CV316",null,null,null,"VXF43xx"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VXF53xx"]
["Тех.характеристики"]
["ДУ max",150,null,150,null,300,null,150,null,150,null,300,null,200,null,120,null,220]
["Давление, бар",16,null,16,null,"16-40",null,"16; 25; 40",null,"6; 16",null,16,null,"6; 16",null,6,null,"16; 25"]
["t, °C, max",150,null,200,null,150,null,450,null,150,null,230,null,300,null,100,null,150]
["ход штока/kv","ход штока","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv","ход штока, max","kv","kv",null,"ход штока, max","kv","ход штока, max","kv","ход штока, max","kv"]
[15,10," 0,16; 0,25; 0,4; 0,63; 1; 1,6; 2,5;  4",15,"0,63; 1; 1,6; 2,5; 4",20,"2,5; 4",20,"0,63; 1; 1,6; 2,5; 4",20,"1,6; 2,5; 4",4,null,"14; 20","0,63; 1,25; 1,6; 2,5; 4",15,"0,63; 1; 1,6; 2,5;4",20,"1,6; 2,5; 4"]
[20,15,"1,6; 2,5; 4; 6,3",null,6.3,null," 4; 6,3",null,"0,63; 1; 1,6; 2,5; 4; 6,3",null,6.3,6.3,null,null,"2,5; 4; 5; 6,3",null,6.3,null,6.3]
[25,20,"1,6; 2,5; 4,0; 6,3;10",null,10,null,"6,3; 10",null,"0,63; 1; 1,6; 2,5; 4; 6,3; 10",null,10,10,null,null,"5; 6,3; 8; 10",null,10,null,"6,3; 10"]
[32,22,"6,3; 10; 16",null,16,null,"16; 10",null,"6,3; 10; 16",null,16,16,null,null,"8; 10; 12,5; 16",null,16,null,16]
[40,null,"10; 16; 25",null,25,null,"16; 25",null,"10; 16; 25",null,25,25,null,null,"12,5; 16; 20; 25",null,25,null,"16; 25"]
[50,25,"10; 16; 25; 40",null,40,null,"25; 40",null,"16; 25; 40",null,40,40,null,"14; 30","20; 25; 31,5; 40",null,40,null,"31,5; 40"]
[65,32,"25; 32; 40; 63",20,63,30,"40; 63","20; 38","25; 40; 63",null,63,63,null,"20; 30","31,5; 40; 50; 63",18,58,null,"50; 63"]
[80,null,"40; 63;100",30,100,null,"63; 100",null,"40; 63; 94",null,100,"70; 100",null,50,"50; 63; 80; 100",null,90,null,"80; 100"]
[100,null,"63; 80; 100; 125;160",null,145,null,"100; 160",38,"63; 94; 125; 160",40,160,"130; 160",null,null,"80; 100; 125;160",30,145,40,"125; 160"]
[125,null,"100; 125; 160; 250",40,220,50,"160; 250","38; 50","125; 160; 250; 320",null,250,"200; 230",null,60,"125; 160; 200; 250",null,null,null,"200; 250"]
[150,null,"160; 250; 360",null,320,null,"250; 320",null,null,null,360,"270; 340",null,null,"200; 250; 315; 400",null,null,null,"315; 400"]
[200,null,null,null,null,null,null,null,null,null,null,"600; 420",null,null,"315; 400; 500; 630"]
[250,null,null,null,null,null,null,null,null,null,null,"900; 640",null,80,"400; 500; 630; 800"]
[300,null,null,null,null,null,null,null,null,null,null,"1200; 930",null,null,"630; 800; 1000; 1250"]

{"sheet":"РА 100,200","index":6,"n_rows":34,"n_cols":10,"rows_kept":34,"cut":false,"hidden":true,"merged":[[33,5,33,6],[0,0,0,10],[33,1,33,2],[33,3,33,4],[33,7,33,8],[33,9,33,10],[17,9,25,10],[22,7,25,8],[22,5,25,6],[31,1,31,2],[31,3,31,4],[31,5,31,6],[31,7,31,8],[31,9,31,10],[32,1,32,2],[32,3,32,4],[32,7,32,8],[32,9,32,10],[32,5,32,6],[29,1,29,2],[29,3,29,4],[29,5,29,6],[29,7,29,8],[29,9,29,10],[26,0,30,0],[26,1,26,2],[26,3,26,4],[26,5,26,6],[26,7,26,8],[26,9,26,10],[27,1,27,2],[27,3,27,4],[27,5,27,6],[27,7,27,8],[30,1,30,2],[30,3,30,4],[30,5,30,6],[30,7,30,8],[30,9,30,10],[27,9,27,10],[28,1,28,2],[28,3,28,4],[28,5,28,6],[28,7,28,8],[28,9,28,10],[24,3,25,4],[23,1,25,2],[22,1,22,2],[22,3,22,4],[23,3,23,4],[19,1,19,2],[19,3,19,4],[20,1,20,2],[20,3,20,4],[14,1,14,2],[14,3,14,4],[14,7,16,7],[14,9,14,10],[15,1,15,2],[15,3,15,4],[15,9,15,10],[20,7,21,8],[21,1,21,2],[21,3,21,4],[16,1,16,2],[16,3,16,4],[16,9,16,10],[17,1,17,2],[17,3,17,4],[17,7,18,7],[18,1,18,2],[18,3,18,4],[10,1,10,2],[10,3,10,4],[10,9,10,10],[11,1,11,2],[11,3,11,4],[11,7,13,7],[11,9,11,10],[12,1,12,2],[12,3,12,4],[12,9,12,10],[13,1,13,2],[13,3,13,4],[13,9,13,10],[8,1,8,2],[8,3,8,4],[8,5,8,6],[8,7,8,8],[8,9,8,10],[9,1,9,2],[9,3,9,4],[9,5,9,6],[9,7,9,8],[9,9,9,10],[6,0,6,10],[7,1,7,2],[7,3,7,4],[7,5,7,6],[7,7,7,8],[7,9,7,10],[4,3,4,4],[4,5,4,6],[4,7,4,8],[5,3,5,4],[5,5,5,6],[5,7,5,8],[3,1,3,2],[3,3,3,4],[3,5,3,6],[3,7,3,8],[2,9,5,10],[1,0,5,0],[1,1,1,2],[1,3,1,4],[1,5,1,6],[1,7,1,8],[1,9,1,10],[2,1,2,2],[2,3,2,4],[2,5,2,6],[2,7,2,8]]}
["Регуляторы давления"]
["РА","КПСР Групп",null,"Danfoss",null,"Ari Armaturen",null,"POLNA",null,"LDM"]
[null,"Серия 100",null,"VFG2 + AFD",null,"ARI-PREDU",null,"Тип ZSN1",null,"RD 122"]
[null,"Серия 200",null,"VFGS2 + AFD",null,null,null,"Тип ZSN3"]
[null,null,null," AVA",null,null,null,"Тип ZSN5"]
[null,null,null,"AVP",null,null,null,"Тип ZSN7"]
["Тех.характеристики"]
["ДУ max",200,null,250,null,150,null,150,null,50]
["Давление, бар","16 ; 25",null,"16-40",null,"16-40",null,"16; 25; 40",null,25]
["t, °C, max",220,null,350,null,350,null,200,null,150]
["kv","kv",null,"kv",null,"ход штока, max","kv","ход штока, max","kv","kv"]
[15," 0,16; 0,25; 0,4; 0,63; 1; 1,6; 2,5; 3,2; 4",null,"1,6; 4; 2,5",null,4,"0,1; 0,4; 1; 2,5; 3,2",6,"1; 1,6; 2,5; 3,2","2,5; 5"]
[20,"1,6; 2,5; 4; 6,3",null,"6,3: 4",null,5,"0,1; 0,4; 1; 2,5; 4; 5",null,"1,6; 2,5; 3,2; 5",8]
[25,"1,6; 2,5; 4,0; 6,3; 8; 10",null,"8; 6,3",null,6,"0,1; 0,4; 1; 2,5; 4; 6,3; 8",null,"2,5; 3,2; 5; 8",10]
[32,"6,3; 10; 16",null,"12,5; 16; 10",null,8,12.5,8,"12,5; 5",15]
[40,"10; 16; 20; 25",null,"20; 16",null,8,20,null,"8; 20",21]
[50,"10; 16; 25; 32; 40",null,"32;25",null,10,32,null,"12,5; 32",32]
[65,"25; 40; 50; 63",null,"50; 40",null,11,50,12,"20; 50"]
[80,"40; 63; 80; 100",null,"80; 63",null,13,80,null,"32; 80"]
[100,"63; 100; 125",null,"125; 100",null,16,125,14,"50; 125"]
[125,"100; 125; 160",null,"160; 125",null,19,190,"спец. Исполнение, по индивид согласованию"]
[150,"160; 280",null,"280; 200",null,22,280]
[200,"250; 360; 450; 630",null,"320; 225"]
[250,null,null,"400; 280"]
[300]
[400]
[" Диапазон настройки, Мпа","0 - (0,01…0,1)",null,"(0,8…1,6)",null,"(0,2…0,6)",null,"(0,01…0,04)",null,"ду 15-25"]
[null,"1 - (0,04...0,16)",null,"(0,3…1,2)",null,"(0,5…1,2)",null,"(0,02…0,08)",null,"(0,015…0,06)"]
[null,"2 - (0,1…0,4)",null,"(0,1…0,6)",null,"(0,8…2,5)",null,"(0,04…0,16)",null,"(0,03…0,21)"]
[null,"3  - (0,3…0,7)",null,"(0,05…0,3)",null,"(2…5)",null,"(0,04…0,16)",null,"(0,06…0,4)"]
[null,"4 - (0,6…1,2)",null,"(0,01…0,07)",null,"(4,5…10)",null,"(0,08…0,32)",null,"ду 32-50"]
[null,null,null,"(0,015…0,15)",null,"(8…16)",null,"(0,1…0,4)",null,"(0,025…0,07)"]
[null,null,null,"(0,005…0,035)",null,null,null,"(0,2…0,8)",null,"(0,04…0,22)"]
[null,null,null,null,null,null,null,"(0,28…1,12)",null,"(0,07…0,41)"]

{"sheet":"RV 103","index":7,"n_rows":49,"n_cols":34,"rows_kept":49,"cut":false,"hidden":false,"merged":[[10,4,10,6],[11,4,11,6],[12,4,12,6],[13,2,13,6],[10,20,10,23],[11,20,11,23],[12,20,12,23],[13,16,14,23],[1,7,1,12],[2,7,2,12],[3,7,3,12],[10,28,20,28],[10,24,20,24],[46,0,46,15],[47,0,47,15],[48,0,48,15],[28,16,29,17],[31,17,33,17],[34,17,35,17],[31,16,35,16]]}
[]
[null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,"RV 103",null,null,null,null,null,null,null,null,null,null,null,null,null,"Клапан КПСР серии 100"]
[null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Для внутренних сетей и ИТП"]
[null,null,null,null,"Материал корпуса: Серый чугун",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,null,null,null,"Рабочая температура: max +150°С",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[null,null,null,null,"Управление (привод)",null,null,"PIKO 524 65","PTE 1","PTN1 MIKRO 655","PTN1","MIKRO 655","PTN 2.20",null,null,null,null,null,null,null,"Управление (привод)",null,null,null,"СЕРИЯ 110","ES05-11","ES05-12","ES06-4","СЕРИЯ 100","ES05-11","ES05-12","ES06-4","ST mini","ST 0"]
[null,null,null,null,"Обозначение в типонометре",null,null,"END","ERE","ERA, ENA","ERA","ENA","ERB",null,null,null,null,null,null,null,"Обозначение в типонометре",null,null,null,null,"1.3500","1.3501","1.3600",null,"1.3500","1.3501","1.3600","1.1100","1.1200"]
[null,null,null,null,"Осевое усилие",null,null,"250 N","500 N","600 N","1200 N","1800 N","2000 N",null,null,null,null,null,null,null,"Осевое усилие",null,null,null,null,600,1000,2000,null,600,1000,2000,1100,4500]
[null,null,"Kvs, м³/ч",null,null,null,null,"ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max",null,null,null,"Kvs, м³/ч",null,null,null,null,null,null,null,null,"ΔP max","ΔP max","ΔP max",null,"ΔP max","ΔP max","ΔP max","ΔP max","ΔP max"]
[null,"DN",1,2,3,4,5,"MPa","MPa","MPa","MPa","MPa","MPa",null,null,"DN",null,null,null,null,null,null,null,null,null,"MPa","MPa","MPa",null,"MPa","MPa","MPa","MPa","MPa"]
[null,15,4,2.5,1.6,1,0.6,1.6,1.6,1.6,1.6,1.6,1.6,null,null,15,0.16,0.25,0.4,0.63,1,1.6,3.2,4,null,1.6,null,1.6,null,0.85,1.4,1.6,1.6,1.6]
[null,20,6.3,4,2.5,"---","---",1.07,1.07,1.32,1.6,1.6,1.6,null,null,20,1.6,2.5,4,6.3,null,null,null,null,null,1.6,null,1.6,null,0.63,1.05,1.6,1.2,1.6]
[null,25,10,6.3,4,"---","---",0.69,0.69,0.85,1.6,1.6,1.6,null,null,25,1.6,2.5,4,6.3,8,10,null,null,null,1.6,null,1.6,null,0.4,0.65,1.6,0.74,1.6]
[null,32,16,10,6.3,"---","---",0.42,0.42,0.52,1.1399999999999999,1.6,1.6,null,null,32,6.3,10,16,null,null,null,null,null,null,1.6,null,1.6,null,0.35,6.2,1.6,0.68,1.6]
[null,40,25,16,10,"---","---",0.27,0.27,0.33,0.74,1.1499999999999999,1.29,null,null,40,10,16,20,25,null,null,null,null,null,1.4,1.6,1.6,null,0.15,0.4,1.6,0.5,1.6]
[null,50,40,25,16,"---","---",0.15,0.15,0.19,0.44,0.69,0.78,null,null,50,10,16,25,32,40,null,null,null,null,1,1.6,1.6,null,null,0.25,1.6,0.8,1.6]
[]
[null,"Пример записи",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Пример записи"]
[null,"RV 103 ENA 4312 16/150-25",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"КПСР 1-1-25-10-1.3500-СЧ-1,6-1-150-У"]
[]
[]
[]
["Тип клапана","Регулирующий клапан",null,null,"RV",null,null,null,null,null,null,null,null,null,null,null,"Тип клапана",null,"Регулирующий клапан",null,null,null,null,null,null,"●","КПСР"]
["Обозначение типа",null,null,null,null,103,null,null,null,null,null,null,null,null,null,null,"Обозначение типа",null,"Регулирующий",null,null,null,null,null,null,"●",1]
[null,"PIKO 524 65",null,null,null,null,"END",null,null,null,null,null,null,null,null,null,null,null,"Запорно-регулирующий",null,null,null,null,null,null,"●",2]
[null,"PTE 1",null,null,null,null,"ERE",null,null,null,null,null,null,null,null,null,"Корпус",null,"Фланцевый",null,null,null,null,null,null,"●",1]
[null,"PTN1",null,null,null,null,"ERA",null,null,null,null,null,null,null,null,null,"Привод","AUMA","ES05-11",null,null,null,null,null,null,"●","1.3500"]
["Привод","MIKRO 655",null,null,null,null,"ENA",null,null,null,null,null,null,null,null,null,null,null,"ES05-12",null,null,null,null,null,null,"●","1.3501"]
[null,"PTN1",null,null,null,null,"ERA",null,null,null,null,null,null,null,null,null,null,null,"ES06-4",null,null,null,null,null,null,"●","1.3600"]
[null,"MIKRO 655",null,null,null,null,"ENA",null,null,null,null,null,null,null,null,null,null,"REGADA","ST mini",null,null,null,null,null,null,"●","1.1100"]
[null,"PTN 2.20",null,null,null,null,"ERB",null,null,null,null,null,null,null,null,null,null,null,"ST 0",null,null,null,null,null,null,"●","1.1200"]
["Исполнение","Прямой, двухход., фланцевый клапан",null,null,null,null,null,4,null,null,null,null,null,null,null,null,"Исполнение",null,"Двухходовой"]
["Материал корпуса","Корпус из серого чугуна EN-JL 1040",null,null,null,null,null,null,3,null,null,null,null,null,null,null,"Материал корпуса",null,"Корпус из серого чугуна EN-JL 1040",null,null,null,null,null,null,"●","СЧ"]
["Расходная","Линейная",null,null,null,null,null,null,null,1,null,null,null,null,null,null,"Расходная",null,"Линейная",null,null,null,null,null,null,"●",1]
["характеристика","Равнопроцентная",null,null,null,null,null,null,null,2,null,null,null,null,null,null,"характеристика",null,"Равнопроцентная",null,null,null,null,null,null,"●",2]
["Kvs","№ столбца значений Kvs клапана согласно табл.",null,null,null,null,null,null,null,null,"X",null,null,null,null,null,"Kvs",null,"Фактическое значение из таблицы",null,null,null,null,null,null,"●",10]
["Давление номин.","PN 16/150 °C ",null,null,null,null,null,null,null,null,null,16,null,null,null,null,"Давление номин.",null,"1,6 МПа",null,null,null,null,null,null,"●",1.6]
["Максим. раб. темп.","150 °C ",null,null,null,null,null,null,null,null,null,null,150,null,null,null,"Максим. раб. темп.",null,"150 °C ",null,null,null,null,null,null,"●",150]
["Диаметр номин.","DN 15 ÷ DN 50",null,null,null,null,null,null,null,null,null,null,null,"ХХ",null,null,"Диаметр номин.",null,"DN 15 ÷ DN 50",null,null,null,null,null,null,"●",25]
[]
[]
["По вопросам продаж и поддержки обращайтесь:"]
[]
["Сайт: http://kpsr.nt-rt.ru  ||  Эл. почта: krp@nt-rt.ru"]

{"sheet":"RV 111","index":8,"n_rows":80,"n_cols":26,"rows_kept":80,"cut":false,"hidden":false,"merged":[[49,24,49,25],[10,19,10,22],[49,1,49,2],[11,7,11,9],[11,19,11,22],[12,7,12,9],[12,19,12,22],[13,15,14,22],[13,2,13,9],[49,10,49,11],[60,1,60,2],[61,1,61,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[1,7,1,13],[2,7,2,13],[3,7,3,13],[10,7,10,9],[52,6,52,7],[53,6,53,7],[54,6,54,7],[55,6,55,7],[56,6,56,7],[57,6,57,7],[49,3,49,5],[56,1,56,2],[57,1,57,2],[58,1,58,2],[59,1,59,2],[56,8,56,9],[74,1,74,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[49,8,49,9],[50,8,50,9],[51,8,51,9],[52,8,52,9],[53,8,53,9],[64,6,64,7],[65,6,65,7],[66,6,66,7],[67,6,67,7],[58,6,58,7],[59,6,59,7],[60,6,60,7],[61,6,61,7],[62,6,62,7],[63,6,63,7],[58,8,58,9],[59,8,59,9],[59,10,59,11],[70,6,70,7],[61,10,61,11],[71,6,71,7],[72,6,72,7],[73,6,73,7],[74,6,74,7],[68,6,68,7],[69,6,69,7],[72,8,72,9],[73,8,73,9],[74,8,74,9],[68,8,68,9],[69,8,69,9],[70,8,70,9],[71,8,71,9],[50,10,50,11],[51,10,51,11],[52,10,52,11],[53,10,53,11],[54,10,54,11],[55,10,55,11],[66,8,66,9],[67,8,67,9],[60,8,60,9],[61,8,61,9],[62,8,62,9],[63,8,63,9],[64,8,64,9],[65,8,65,9],[54,8,54,9],[55,8,55,9],[57,8,57,9],[49,17,49,19],[49,20,49,21],[49,22,49,23],[68,10,68,11],[69,10,69,11],[70,10,70,11],[71,10,71,11],[72,10,72,11],[73,10,73,11],[62,10,62,11],[63,10,63,11],[64,10,64,11],[65,10,65,11],[66,10,66,11],[67,10,67,11],[60,10,60,11],[77,0,77,13],[78,0,78,13],[79,0,79,13],[26,0,28,0],[29,0,30,0],[37,0,39,0],[27,15,28,16],[30,16,32,16],[28,1,28,5],[50,14,58,14],[50,0,58,0],[56,10,56,11],[57,10,57,11],[58,10,58,11],[49,6,49,7],[50,6,50,7],[51,6,51,7],[30,15,32,15],[59,0,67,0],[68,0,74,0],[50,15,58,25],[74,10,74,11],[50,3,74,5],[49,15,49,16]]}
[]
[null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,"RV 111",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Клапан КПСР серии 100"]
[null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Для внутренних сетей и ИТП"]
[null,null,null,null,"Материал корпуса: Серый чугун",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,null,null,null,"Рабочая температура: max +150°С",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Управление (привод)",null,null,null,"AVM 322 S","AVM 234 S","AVF 234 S"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Обозначение в типонометре",null,null,null,"1.2300","1.2100","1.2200"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Осевое усилие",null,null,null,1000,2500,2000]
[null,null,"Kvs, м³/ч",null,null,null,null,null,null,null,"ΔP max",null,null,null,null,"Kvs, м³/ч",null,null,null,null,null,null,null,"ΔP max","ΔP max","ΔP max"]
[null,"DN",1,2,3,4,5,6,7,8,"MPa",null,null,null,"DN",null,null,null,null,null,null,null,null,"MPa","MPa","MPa"]
[null,15,4,2.5,1.6,1,0.63,0.4,0.25,0.16,0.4,null,null,null,15,0.16,0.25,0.4,0.63,1,1.6,3.2,4,1.4,1.6,1.6]
[null,20,6.3,"---","---","---","---","---","---","---",0.35,null,null,null,20,1.6,2.5,4,6.3,null,null,null,null,0.8,1.6,1.6]
[null,25,10,"---","---","---","---","---","---","---",0.2,null,null,null,25,1.6,2.5,4,6.3,8,10,null,null,0.74,1.3,1.3]
[null,32,16,"---","---","---","---","---","---","---",0.11,null,null,null,32,6.3,10,16,null,null,null,null,null,0.62,1,1]
[null,40,25,"---","---","---","---","---","---","---",0.06,null,null,null,40,10,16,20,25,null,null,null,null,null,0.9,0.9]
[]
[null,"Пример записи",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Пример записи"]
[null,"RV 111 R 2331 16/150-25/F",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"КПСР 1-1-25-10-1.2300-СЧ-1,6-1-150-У"]
[]
[]
[]
["Тип клапана","Регулирующий клапан",null,null,"RV",null,null,null,null,null,null,null,null,null,null,"Тип клапана",null,"Регулирующий клапан",null,null,null,null,null,null,"●","КПСР"]
[null,"Вентиль с наружной резьбой",null,null,null,111,null,null,null,null,null,null,null,null,null,"Обозначение типа",null,"Регулирующий",null,null,null,null,null,null,"●",1]
[null,"Ручной маховик с возможностью присоединения электрического привода",null,null,null,null,"R",null,null,null,null,null,null,null,null,null,null,"Запорно-регулирующий",null,null,null,null,null,null,"●",2]
["Исполнение","Двухходовой",null,null,null,null,null,2,null,null,null,null,null,null,null,"Корпус",null,"Фланцевый",null,null,null,null,null,null,"●",1]
[null,"Трехходовой",null,null,null,null,null,3,null,null,null,null,null,null,null,"Привод","Sauter","AVM 322S",null,null,null,null,null,null,"●","1.2300"]
[null,"Серый чугун",null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,"AVM 234 S",null,null,null,null,null,null,"●","1.2200"]
[11,"Линейная (двухход. DN 32, 40 и трехход. исполн.)",null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,"AVF 234 S аварийная функция",null,null,null,null,null,null,"●","1.2100"]
["характеристика","LDMspline® (двухход. исполн. DN 15÷25)",null,null,null,null,null,null,null,2,null,null,null,null,null,"Исполнение",null,"Двухходовой"]
["Kvs","№ столбца значений Kvs клапана согласно табл.",null,null,null,null,null,null,null,null,"X",null,null,null,null,"Материал корпуса",null,"Корпус из серого чугуна EN-JL 1040",null,null,null,null,null,null,"●","СЧ"]
["Давление номин.","PN 16/150 °C ",null,null,null,null,null,null,null,null,null,"16/150",null,null,null,"Расходная",null,"Линейная",null,null,null,null,null,null,"●",1]
["Диаметр номин.","DN 15 ÷ DN 40",null,null,null,null,null,null,null,null,null,null,"XX",null,null,"характеристика",null,"Равнопроцентная",null,null,null,null,null,null,"●",2]
["Присоединение","Муфтовое",null,null,null,null,null,null,null,null,null,null,null,"T",null,"Kvs",null,"Фактическое значение из таблицы",null,null,null,null,null,null,"●",10]
[null,"Фланцевое",null,null,null,null,null,null,null,null,null,null,null,"F",null,"Давление номин.",null,"1,6 МПа",null,null,null,null,null,null,"●",1.6]
[null,"Приварное резьбовое соединение",null,null,null,null,null,null,null,null,null,null,null,"W",null,"Максим. раб. темп.",null,"150 °C ",null,null,null,null,null,null,"●",150]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Диаметр номин.",null,"DN 15 ÷ DN 50",null,null,null,null,null,null,"●",25]
[]
[]
[]
[]
[]
[]
[null,"Привод специфицируется отдельно"]
[]
["Производитель","Тип привода",null,"Исполнение",null,null,"Время перемещения штока",null,"Питание",null,"Управление",null,null,null,"Производитель","Тип привода",null,"Исполнение",null,null,"Время перемещения штока",null,"Питание",null,"Управление"]
["LDM","ANT 3-5.10",null,"Электрический привод",null,null,"66 s",null," 24 V AC",null,"3-position",null,null,null,"Sauter","ВОЗМОЖНО ЗДЕСЬ НАДО ПРОПИСАТЬ НАШИ АНАЛОГИ "]
[null,"ANT 3-5.11",null,null,null,null,"5 s",null," 24 V AC/DC",null,"0÷10 V or 4÷20 mA"]
[null,"ANT 3-5.20",null,null,null,null,"66 s",null," 230 V AC",null,"3-position"]
[null,"ANT 3-5.10SC",null,null,null,null,"33 s",null,"24 V AC/DC",null,"3-position"]
[null,"ANT 3-5.11SC",null,null,null,null,"5 s",null," 24 V AC/DC",null,"0÷10 V or 4÷20 mA"]
[null,"ANT 3-5.22",null,null,null,null,"33 s",null," 230 V AC",null,"3-position"]
[null,"ANT 3-5.21",null,null,null,null,"5 s",null," 230 V AC",null,"0÷10 V or 4÷20 mA"]
[null,"ANT 3-5.20SC",null,null,null,null,"33 s",null," 230 V AC",null,"3-position"]
[null,"ANT 3-5.21SC",null,null,null,null,"5 s",null," 230 V AC",null,"0÷10 V or 4÷20 mA"]
["Siemens","SSC 31",null,null,null,null,"150 s",null,"AC 230 V",null,"3-position"]
[null,"SSC 61",null,null,null,null,"30 s",null,"AC 24 V",null,"0÷10 V"]
[null,"SSC 61.5",null,null,null,null,"30 s",null,"AC 24 V",null,"0÷10 V"]
[null,"SSC 81",null,null,null,null,"150 s",null,"AC 24 V",null,"3-position"]
[null,"SQS 35.00",null,null,null,null,"150 s",null,"AC 230 V",null,"3-position"]
[null,"SQS 35.03",null,null,null,null,"35 s",null,"AC 230 V",null,"3-position"]
[null,"SQS 35.50",null,null,null,null,"150 s",null,"AC 230 V",null,"3-position"]
[null,"SQS 35.53",null,null,null,null,"35 s",null,"AC 230 V",null,"3-position"]
[null,"SQS 65.5",null,null,null,null,"35 s",null,"AC 24 V",null,"0÷10 V"]
["Sauter","AVM105F100",null,null,null,null,"30 s",null,"AC 230 V",null,"3-position"]
[null,"AVM105F120",null,null,null,null,"120 s",null,"AC 230 V",null,"3-position"]
[null,"AVM105F122",null,null,null,null,"120 s",null,"AC 24 V",null,"3-position"]
[null,"AVM115F120",null,null,null,null,"120 s",null,"AC 230 V",null,"3-position"]
[null,"AVM115F122",null,null,null,null,"120 s",null,"AC 24 V",null,"3-position"]
[null,"AVM105SF132",null,null,null,null,"30/60/120 s",null,"AC 24 V",null,"SUT"]
[null,"AVM115SF132",null,null,null,null,"60/120 s",null,"AC 24 V",null,"SUT"]
[]
[]
["По вопросам продаж и поддержки обращайтесь:"]
[]
["Сайт: http://kpsr.nt-rt.ru  ||  Эл. почта: krp@nt-rt.ru"]

{"sheet":"Серия VFM2","index":9,"n_rows":47,"n_cols":19,"rows_kept":47,"cut":false,"hidden":true,"merged":[[15,12,15,18],[37,5,43,7],[14,3,14,5],[14,14,14,15],[14,16,14,18],[15,1,15,7],[16,12,16,18],[18,12,18,18],[11,1,12,7],[14,6,14,7],[11,12,12,18],[1,6,1,11],[2,6,2,11],[3,6,3,11],[14,8,14,11]]}
[]
[null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,"VFM2",null,null,null,null,null,null,null,null,null,null,null,"Серия 100"]
[]
[null,"Рабочее давление: 1,6 МПа (16 атм)",null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,"Рабочая температура: max +150°С",null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,65,80,100,125,150,200,250,null,null,null,null,65,80,100,125,150,200,250]
[null,30,34,40,null,null,50,null,"Ход штока клапана",null,null,null,25,32,40,null,75]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Основные значения"]
[null,63,100,160,250,400,630,900,null,null,null,null,63,"100","160","250","400","630","1000"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Дополнительные значения"]
[null,null,null,null,null,null,null,null,null,null,null,null,"16","40","63",100,160,250,"400"]
[null,null,null,null,null,null,null,null,null,null,null,null,"25","63",80,"125","250","360",630]
[null,null,null,null,null,null,null,null,null,null,null,null,32,80,"100","160","360","400","800"]
[null,null,null,null,null,null,null,null,null,null,null,null,"40",null,"125","200"]
[null,null,null,null,null,null,null,null,null,null,null,null,"50"]
[null,null,null,null,null,null,null,null,null,null,null,null,"80"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[]
[]
["Danfoss","VFM2",65,63,"065В3500","Соответствие",null,null,"КПСР",null,"1.НП-1-65-63-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFM2",80,100,"065В3501",null,null,null,"КПСР",null,"1.НП-1-80-100-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFM2",100,160,"065В3502",null,null,null,"КПСР",null,"1.НП-1-100-160-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFM2",125,250,"065В3503",null,null,null,"КПСР",null,"1.НП-1-125-250-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFM2",150,400,"065В3504",null,null,null,"КПСР",null,"1.НП-1-150-360-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFM2",200,630,"065В3505",null,null,null,"КПСР",null,"1.НП-1-200-630-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFM2",250,900,"065В3506",null,null,null,"КПСР",null,"1.НП-1-250-1000-Х.ХХХХ-СЧ-1,6-1-150-У"]
[]
[null,null,null,null,null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
[null,null,null,null,null,null,null,null,null,"Х.ХХХХ","- маркировка привода"]

{"sheet":"Серия VL2","index":10,"n_rows":54,"n_cols":23,"rows_kept":54,"cut":false,"hidden":true,"merged":[[15,14,15,22],[15,1,15,9],[38,5,44,7],[14,1,14,3],[14,4,14,6],[14,14,14,15],[14,18,14,20],[14,16,14,17],[14,7,14,8],[14,10,14,13],[16,14,16,22],[22,14,22,22],[1,8,1,13],[2,8,2,13],[3,8,3,13],[11,14,12,22],[11,1,12,9]]}
[]
[null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,"VL2",null,null,null,null,null,null,null,null,null,null,null,null,null,"Клапана КПСР серии 100"]
[]
[null,"Рабочее давление: 0,6 МПа (6 атм)",null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,"Рабочая температура: max +120°С",null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,15,20,25,32,40,50,65,80,100,null,null,null,null,15,20,25,32,40,50,65,80,100]
[null,10,null,null,15,null,null,20,null,25,"Ход штока клапана",null,null,null,10,null,20,null,32,null,null,32,40]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Основные значения"]
[null,"0,63",6.3,10,16,25,40,63,100,145,null,null,null,null,0.63,6.3,"10",16,25,40,63,"100","160"]
[null,"1",null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,1.6,null,null,null,null,null,null,null,null,null,null,null,null,1.6]
[null,"2,5",null,null,null,null,null,null,null,null,null,null,null,null,"2,5"]
[null,"4",null,null,null,null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Дополнительные значения"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10,"16","40","63"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.25,2.5,2.5,10,16,16,"25","63",80]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,4,4,null,20,25,32,80,"100"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.2,null,6.3,null,null,32,"40",null,"125"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,"50"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"80"]
[]
[]
[]
[]
[]
[]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[]
[]
["Danfoss","VL2",15,"0,63","065Z0371","Соответствие",null,null,"КПСР",null,"1.НП-1-15-0,63-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL2",15,"1","065Z0372",null,null,null,"КПСР",null,"1.НП-1-15-1-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL2",15,"1,6","065Z0373",null,null,null,"КПСР",null,"1.НП-1-15-1,6-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL2",15,"2,5","065Z0374",null,null,null,"КПСР",null,"1.НП-1-15-2,5-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL2",15,"4","065Z0375",null,null,null,"КПСР",null,"1.НП-1-15-4-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL2",20,"6,3","065Z0376",null,null,null,"КПСР",null,"1.НП-1-20-6,3-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL2",25,"10","065Z0377",null,null,null,"КПСР",null,"1.НП-1-25-10-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL2",32,"16","065Z0378",null,null,null,"КПСР",null,"1.НП-1-32-16-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL2",40,"25","065Z0379",null,null,null,"КПСР",null,"1.НП-1-40-25-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL2",50,"40","065Z0380",null,null,null,"КПСР",null,"1.НП-1-50-40-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL2",65,"63","065Z0381",null,null,null,"КПСР",null,"1.НП-1-65-63-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL2",80,"100","065Z0382",null,null,null,"КПСР",null,"1.НП-1-80-100-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL2",100,"145","065Z3426",null,null,null,"КПСР",null,"1.НП-1-100-145-Х.ХХХХ-СЧ-1,6-1-150-У"]
[]
[null,null,null,null,null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
[null,null,null,null,null,null,null,null,null,"Х.ХХХХ","- маркировка привода"]

{"sheet":"Серия VFS2","index":11,"n_rows":54,"n_cols":23,"rows_kept":54,"cut":false,"hidden":true,"merged":[[15,14,15,22],[15,1,15,9],[37,5,44,7],[14,1,14,6],[14,7,14,9],[14,14,14,15],[14,16,14,17],[14,18,14,20],[14,10,14,13],[16,14,16,22],[22,14,22,22],[1,8,1,13],[2,8,2,13],[3,8,3,13],[11,14,12,22],[11,1,12,9]]}
[]
[null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,"VFS2",null,null,null,null,null,null,null,null,null,null,null,null,null,"Клапана КПСР серии 200"]
[]
[null,"Рабочее давление: 2,5 МПа (25 атм)",null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 2,5 МПа (16 атм)"]
[null,"Материал корпуса: Высокопрочный чугун (EN-GJS-400-18-LT (GGG 40.3))",null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Высокопрочный чугун (EN-JS 1025)"]
[null,"Рабочая температура: max +120°С",null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +220°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,15,20,25,32,40,50,65,80,100,null,null,null,null,15,20,25,32,40,50,65,80,100]
[null,15,null,null,null,null,null,40,null,null,"Ход штока клапана",null,null,null,10,null,20,null,32,null,null,32,40]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Основные значения"]
[null,0.4,6.3,10,16,25,40,63,100,145,null,null,null,null,0.4,6.3,"10",16,25,40,63,"100","160"]
[null,"0,63",null,null,null,null,null,null,null,null,null,null,null,null,0.63]
[null,"1",null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,1.6,null,null,null,null,null,null,null,null,null,null,null,null,1.6]
[null,"2,5",null,null,null,null,null,null,null,null,null,null,null,null,4]
[null,"4",null,null,null,null,null,null,null,null,null,null,null,null,"Дополнительные значения"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10,"16","40","63"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.25,2.5,2.5,10,16,16,"25","63",80]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.2,4,4,null,20,25,32,80,"100"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.3,null,null,32,"40",null,"125"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,"50"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"80"]
[]
[]
[]
[]
[]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[]
[]
["Danfoss","VFS2",15,"0,4","065B1510","Соответствие",null,null,"КПСР",null,"1.НП-1-15-0,4-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFS2",15,"0,63","065B1511",null,null,null,"КПСР",null,"1.НП-1-15-0,63-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFS2",15,"1","065B1512",null,null,null,"КПСР",null,"1.НП-1-15-1-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFS2",15,"1,6","065B1513",null,null,null,"КПСР",null,"1.НП-1-15-1,6-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFS2",15,"2,5","065B1514",null,null,null,"КПСР",null,"1.НП-1-15-2,5-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFS2",15,"4","065B1515",null,null,null,"КПСР",null,"1.НП-1-15-4-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFS2",20,"6,3","065B1520",null,null,null,"КПСР",null,"1.НП-1-20-6,3-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFS2",25,"10","065B1525",null,null,null,"КПСР",null,"1.НП-1-25-10-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFS2",32,"16","065B1532",null,null,null,"КПСР",null,"1.НП-1-32-16-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFS2",40,"25","065B1540",null,null,null,"КПСР",null,"1.НП-1-40-25-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFS2",50,"40","065B1550",null,null,null,"КПСР",null,"1.НП-1-50-40-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFS2",65,"63","065B3365",null,null,null,"КПСР",null,"1.НП-1-65-63-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFS2",80,"100","065B3380",null,null,null,"КПСР",null,"1.НП-1-80-100-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFS2",100,"145","065B3400",null,null,null,"КПСР",null,"1.НП-1-100-145-Х.ХХХХ-ВЧ-2,5-1-220-У"]
[]
[null,null,null,null,null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
[null,null,null,null,null,null,null,null,null,"Х.ХХХХ","- маркировка привода"]

{"sheet":"Серия VFG2 ","index":12,"n_rows":52,"n_cols":31,"rows_kept":52,"cut":false,"hidden":true,"merged":[[18,18,18,30],[20,18,20,30],[17,18,17,30],[17,1,17,13],[13,18,14,30],[13,1,14,13],[16,18,16,19],[16,20,16,21],[16,22,16,24],[16,26,16,27],[16,28,16,30],[16,14,16,17],[16,1,16,3],[16,6,16,7],[16,9,16,10],[16,11,16,13],[7,26,8,26],[7,27,8,28],[9,24,10,24],[1,12,1,17],[2,12,2,17],[3,12,3,17],[9,25,10,26]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,"VFG2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Клапана КПСР серии 200, 210"]
[]
[null,"Рабочее давление: 2,5 (25) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 2,5 (25) МПа (атм)",null,null,null,null,null,null,null,"}","Серия 200"]
[null,"Материал корпуса: Высокопрочный чугун (EN-GJS-400-18-LT (GGG 40.3))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Высокопрочный чугун (EN-JS 1025)"]
[null,"Рабочее давление: 4 (40) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 4 (40) МПа (атм)",null,null,null,null,null,"}","Серия 210"]
[null,"Материал корпуса: Сталь 20 (GP240GH (GS-C 25))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Сталь 20 (1.0443)"]
[null,"Рабочая температура: max +200°С",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +260°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,15,20,25,32,40,50,65,80,100,125,150,200,250,null,null,null,null,15,20,25,32,40,50,65,80,100,125,150,200,250]
[null,6,null,null,9,8,12,null,18,20,null,24,null,null,"Ход штока клапана",null,null,null,10,null,20,null,32,null,null,32,40,null,75]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Основные значения"]
[null,"4","6,3","8","16","20","32",50,80,125,160,280,320,400,null,null,null,null,4,6.3,8,16,20,32,"50",80,"125","160",280,"360","400"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Дополнительные значения"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10,"16","40","63","100","160","250","450"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.25,2.5,2.5,10,16,16,"25","63",80,125,250,"450","630"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,4,4,null,25,25,32,"100","100","250","360","630","800"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.63,null,6.3,null,null,40,"40",null,"160",null,null,null,1000]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"10",null,null,null,63]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6,null,null,null,null,null,"80"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.2]
[]
[]
[]
[]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[]
[null,null,null,null,null,"Py = 25",null,null,null,null,null,null,null,"Py = 40"]
["Danfoss","VFGS2",15,"4",null,"065B2401",null,"1.НП-1-15-4-Х.ХХХХ-ВЧ-2,5-1-220-У",null,null,null,null,null,"065B2411",null,"1.НП-1-15-4-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",20,"6,3",null,"065B2402",null,"1.НП-1-15-0,63-Х.ХХХХ-ВЧ-2,5-1-220-У",null,null,null,null,null,"065B2412",null,"1.НП-1-15-0,63-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",25,"8",null,"065B2403",null,"1.НП-1-15-1-Х.ХХХХ-ВЧ-2,5-1-220-У",null,null,null,null,null,"065B2413",null,"1.НП-1-15-1-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",32,"16",null,"065B2404",null,"1.НП-1-15-1,6-Х.ХХХХ-ВЧ-2,5-1-220-У",null,null,null,null,null,"065B2414",null,"1.НП-1-15-1,6-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",40,"20",null,"065B2405",null,"1.НП-1-15-2,5-Х.ХХХХ-ВЧ-2,5-1-220-У",null,null,null,null,null,"065B2415",null,"1.НП-1-15-2,5-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",50,"32",null,"065B2406",null,"1.НП-1-15-4-Х.ХХХХ-ВЧ-2,5-1-220-У",null,null,null,null,null,"065B2416",null,"1.НП-1-15-4-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",65,"50",null,"065B2407",null,"1.НП-1-20-6,3-Х.ХХХХ-ВЧ-2,5-1-220-У",null,null,null,null,null,"065B2417",null,"1.НП-1-20-6,3-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",80,"80",null,"065B2408",null,"1.НП-1-25-10-Х.ХХХХ-ВЧ-2,5-1-220-У",null,null,null,null,null,"065B2418",null,"1.НП-1-25-10-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",100,"125",null,"065B2409",null,"1.НП-1-32-16-Х.ХХХХ-ВЧ-2,5-1-220-У",null,null,null,null,null,"065B2419",null,"1.НП-1-32-16-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",125,"160",null,"065B2410",null,"1.НП-1-40-25-Х.ХХХХ-ВЧ-2,5-1-220-У",null,null,null,null,null,"065B2420",null,"1.НП-1-40-25-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",150,"280",null,null,null,null,null,null,null,null,null,"065B2421",null,"1.НП-1-40-25-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",200,"320",null,null,null,null,null,null,null,null,null,"065B2422",null,"1.НП-1-40-25-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",250,"400",null,null,null,null,null,null,null,null,null,"065B2423",null,"1.НП-1-40-25-Х.ХХХХ-СТ-4-1-425-У"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Х.ХХХХ","- маркировка привода"]

{"sheet":"Серия VFGS2_16","index":13,"n_rows":52,"n_cols":31,"rows_kept":52,"cut":false,"hidden":true,"merged":[[16,18,16,30],[18,18,18,30],[15,18,15,30],[15,1,15,13],[14,1,14,3],[14,6,14,7],[14,9,14,10],[14,11,14,13],[14,18,14,19],[14,14,14,17],[14,20,14,21],[14,22,14,24],[14,26,14,27],[14,28,14,30],[1,12,1,17],[2,12,2,17],[3,12,3,17],[11,18,12,30],[11,1,12,13],[7,25,8,25],[7,26,8,28]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,"VFGS2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Клапана КПСР серии 100"]
[]
[null,"Рабочее давление: 1,6 (16) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 (16)МПа (атм)"]
[null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,"Рабочая температура: max +350°С",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,15,20,25,32,40,50,65,80,100,125,150,200,250,null,null,null,null,15,20,25,32,40,50,65,80,100,125,150,200,250]
[null,6,null,null,9,8,12,null,18,20,null,24,null,null,"Ход штока клапана",null,null,null,10,null,20,null,32,null,null,32,40,null,75]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Основные значения"]
[null,"4","6,3","8","16","20","32",50,80,125,160,280,320,400,null,null,null,null,4,6.3,"10",16,20,32,"50",80,"125","160",280,"360","400"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Дополнительные значения"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10,"16","40","63","100","160","250","450"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.25,2.5,2.5,10,16,16,"25","63",80,125,250,"450","630"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,4,4,null,25,25,32,"100","100","250","360","630","800"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.63,null,6.3,null,null,40,"40",null,"160",null,null,null,1000]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,63]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6,null,null,null,null,null,"80"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.2]
[]
[]
[]
[]
[]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[null,null,null,null,null,null,null,null,null,"КЛАПАНА КПСР серии 100"]
[null,null,null,null,"Py = 16"]
["Danfoss","VFGS2",15,"4","065B2430",null,null,"КПСР",null,"1.НП-1-15-4-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFGS2",20,"6,3","065B2431",null,null,"КПСР",null,"1.НП-1-20-6,3-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFGS2",25,"8","065B2432",null,null,"КПСР",null,"1.НП-1-25-8-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFGS2",32,"16","065B2433",null,null,"КПСР",null,"1.НП-1-32-16-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFGS2",40,"20","065B2434",null,null,"КПСР",null,"1.НП-1-40-20-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFGS2",50,"32","065B2435",null,null,"КПСР",null,"1.НП-1-50-32-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFGS2",65,"50","065B2436",null,null,"КПСР",null,"1.НП-1-65-50-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFGS2",80,"80","065B2437",null,null,"КПСР",null,"1.НП-1-80-80-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFGS2",100,"125","065B2438",null,null,"КПСР",null,"1.НП-1-100-125-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFGS2",125,"160","065B2439",null,null,"КПСР",null,"1.НП-1-125-160-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFGS2",150,"280","065B2440",null,null,"КПСР",null,"1.НП-1-150-280-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFGS2",200,"320","065B2441",null,null,"КПСР",null,"1.НП-1-200-320-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VFGS2",250,"400","065B2442",null,null,"КПСР",null,"1.НП-1-250-400-Х.ХХХХ-СЧ-1,6-1-150-У"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Х.ХХХХ","- маркировка привода"]

{"sheet":"Серия VFGS2_25","index":14,"n_rows":45,"n_cols":31,"rows_kept":45,"cut":false,"hidden":true,"merged":[[16,18,16,30],[18,18,18,30],[14,20,14,21],[14,22,14,24],[14,26,14,27],[14,28,14,30],[15,1,15,13],[15,18,15,30],[11,1,12,13],[11,18,12,30],[14,1,14,3],[14,6,14,7],[14,9,14,10],[14,11,14,13],[14,14,14,17],[14,18,14,19],[1,12,1,17],[2,12,2,17],[3,12,3,17],[7,26,8,26],[7,27,8,29]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,"VFGS2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Клапана КПСР серии 200"]
[]
[null,"Рабочее давление: 2,5 (25) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 2,5 (25) МПа (атм)"]
[null,"Материал корпуса: Высокопрочный чугун (EN-GJS-400-18-LT (GGG 40.3))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Высокопрочный чугун (EN-JS 1025)"]
[null,"Рабочая температура: max +350°С",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +220°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,15,20,25,32,40,50,65,80,100,125,150,200,250,null,null,null,null,15,20,25,32,40,50,65,80,100,125,150,200,250]
[null,6,null,null,9,8,12,null,18,20,null,24,null,null,"Ход штока клапана",null,null,null,10,null,20,null,32,null,null,32,40,null,75]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Основные значения"]
[null,"4","6,3","8","16","20","32",50,80,125,160,280,320,400,null,null,null,null,4,6.3,"10",16,20,32,"50",80,"125","160",280,"360","400"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Дополнительные значения"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10,"16","40","63","100","160","250","450"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.25,2.5,2.5,10,16,16,"25","63",80,125,250,"450","630"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,4,4,null,25,25,32,"100","100","250","360","630","800"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.63,null,6.3,null,null,40,"40",null,"160",null,null,null,1000]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,63]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6,null,null,null,null,null,"80"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.2]
[]
[]
[]
[]
[]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[null,null,null,null,null,null,null,null,null,"КЛАПАНА КПСР серии 200"]
[null,null,null,null,"Py = 25"]
["Danfoss","VFGS2",15,"4","065B2443",null,null,"КПСР",null,"1.НП-1-15-4-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFGS2",20,"6,3","065B2444",null,null,"КПСР",null,"1.НП-1-15-0,63-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFGS2",25,"8","065B2445",null,null,"КПСР",null,"1.НП-1-15-1-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFGS2",32,"16","065B2446",null,null,"КПСР",null,"1.НП-1-15-1,6-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFGS2",40,"20","065B2447",null,null,"КПСР",null,"1.НП-1-15-2,5-Х.ХХХХ-ВЧ-2,5-1-220-У",null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
["Danfoss","VFGS2",50,"32","065B2448",null,null,"КПСР",null,"1.НП-1-15-4-Х.ХХХХ-ВЧ-2,5-1-220-У",null,null,null,null,null,"Х.ХХХХ","- маркировка привода"]
["Danfoss","VFGS2",65,"50","065B2449",null,null,"КПСР",null,"1.НП-1-20-6,3-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFGS2",80,"80","065B2450",null,null,"КПСР",null,"1.НП-1-25-10-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFGS2",100,"125","065B2451",null,null,"КПСР",null,"1.НП-1-32-16-Х.ХХХХ-ВЧ-2,5-1-220-У"]
["Danfoss","VFGS2",125,"160","065B2452",null,null,"КПСР",null,"1.НП-1-40-25-Х.ХХХХ-ВЧ-2,5-1-220-У"]

{"sheet":"Серия VFGS2_40","index":15,"n_rows":52,"n_cols":31,"rows_kept":52,"cut":false,"hidden":true,"merged":[[16,18,16,30],[18,18,18,30],[14,20,14,21],[14,22,14,24],[14,26,14,27],[14,28,14,30],[1,12,1,17],[2,12,2,17],[3,12,3,17],[15,1,15,13],[15,18,15,30],[7,24,8,24],[7,25,8,27],[11,1,12,13],[11,18,12,30],[14,1,14,3],[14,6,14,7],[14,9,14,10],[14,11,14,13],[14,14,14,17],[14,18,14,19]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,"VFGS2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Клапана КПСР серии 210"]
[]
[null,"Рабочее давление: 4 (40) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 4 (40) МПа (атм)"]
[null,"Материал корпуса: Сталь 20 (GP240GH (GS-C 25))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Сталь 20 (1.0443)"]
[null,"Рабочая температура: max +350°С",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +425°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,15,20,25,32,40,50,65,80,100,125,150,200,250,null,null,null,null,15,20,25,32,40,50,65,80,100,125,150,200,250]
[null,6,null,null,9,8,12,null,18,20,null,24,null,null,"Ход штока клапана",null,null,null,10,null,20,null,32,null,null,32,40,null,75]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Основные значения"]
[null,"4","6,3","8","16","20","32",50,80,125,160,280,320,400,null,null,null,null,4,6.3,"10",16,20,32,"50",80,"125","160",280,"360","400"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Дополнительные значения"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10,"16","40","63","100","160","250","450"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.25,2.5,2.5,10,16,16,"25","63",80,125,250,"450","630"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,4,4,null,25,25,32,"100","100","250","360","630","800"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.63,null,6.3,null,null,40,"40",null,"160",null,null,null,1000]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,63]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6,null,null,null,null,null,"80"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.2]
[]
[]
[]
[]
[]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[null,null,null,null,null,null,null,null,null,null,null,null,"КЛАПАНА КПСР серии 210"]
[null,null,null,null,"Py = 16",null,null,null,null,null,"Py = 40"]
["Danfoss","VFGS2",15,"4","065B2430",null,null,"КПСР",null,null,"065B2453",null,"1.НП-1-15-4-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",20,"6,3","065B2431",null,null,"КПСР",null,null,"065B2454",null,"1.НП-1-15-0,63-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",25,"8","065B2432",null,null,"КПСР",null,null,"065B2455",null,"1.НП-1-15-1-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",32,"16","065B2433",null,null,"КПСР",null,null,"065B2456",null,"1.НП-1-15-1,6-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",40,"20","065B2434",null,null,"КПСР",null,null,"065B2457",null,"1.НП-1-15-2,5-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",50,"32","065B2435",null,null,"КПСР",null,null,"065B2458",null,"1.НП-1-15-4-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",65,"50","065B2436",null,null,"КПСР",null,null,"065B2459",null,"1.НП-1-20-6,3-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",80,"80","065B2437",null,null,"КПСР",null,null,"065B2460",null,"1.НП-1-25-10-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",100,"125","065B2438",null,null,"КПСР",null,null,"065B2461",null,"1.НП-1-32-16-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",125,"160","065B2439",null,null,"КПСР",null,null,"065B2462",null,"1.НП-1-40-25-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",150,"280","065B2440",null,null,"КПСР",null,null,"065B2463",null,"1.НП-1-40-25-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",200,"320","065B2441",null,null,"КПСР",null,null,"065B2464",null,"1.НП-1-40-25-Х.ХХХХ-СТ-4-1-425-У"]
["Danfoss","VFGS2",250,"400","065B2442",null,null,"КПСР",null,null,"065B2465",null,"1.НП-1-40-25-Х.ХХХХ-СТ-4-1-425-У"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Х.ХХХХ","- маркировка привода"]

{"sheet":"Серия VM2","index":16,"n_rows":47,"n_cols":15,"rows_kept":47,"cut":false,"hidden":true,"merged":[[1,6,1,11],[2,6,2,11],[3,6,3,11],[31,5,37,7],[14,7,14,8],[15,9,15,14],[15,1,15,6],[11,9,12,14],[11,1,12,6],[14,9,14,10],[14,12,14,14],[14,1,14,2],[14,4,14,6],[16,9,16,14],[22,9,22,14]]}
[]
[null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,"VМ 2",null,null,null,null,null,null,null,"Клапана КПСР серии 110"]
[]
[null,"Рабочее давление: 1,6 МПа (16 атм)",null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,"Материал корпуса: Красная бронза (Rg 5)",null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,"Рабочая температура: max +150°С",null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,15,20,25,32,40,50,null,null,15,20,25,32,40,50]
[null,5,null,7,10,null,null,"Ход штока клапана",null,5,null,7,10]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,null,null,null,null,null,null,null,null,"Основные значения"]
[null,0.25,4,6.3,10,16,25,null,null,0.25,4,6.3,10,16,25]
[null,0.4,6.3,8,null,null,null,null,null,0.4,6.3,8]
[null,0.63,null,null,null,null,null,null,null,0.63]
[null,1,null,null,null,null,null,null,null,1]
[null,1.6,null,null,null,null,null,null,null,1.6]
[null,2.5,null,null,null,null,null,null,null,"Дополнительные значения"]
[null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10]
[null,null,null,null,null,null,null,null,null,3.2,2.5,2.5,16,20,16]
[null,null,null,null,null,null,null,null,null,4,null,4,null,25,32]
[null,null,null,null,null,null,null,null,null,null,null,10,null,null,40]
[]
[]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[]
["Danfoss","VM2",15,"0,25","065B2010","Соответствие",null,null,"КПСР",null,"1.НП-1.1-1-15-0,25-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VM2",15,"0,4","065B2011",null,null,null,"КПСР",null,"1.НП-1.1-1-15-0,4-1.3500-СЧ-1,6-1.1-150-У"]
["Danfoss","VM2",15,"0,63","065B2012",null,null,null,"КПСР",null,"1.НП-1.1-1-15-0,63-1.3500-СЧ-1,6-1.1-150-У"]
["Danfoss","VM2",15,"1","065B2013",null,null,null,"КПСР",null,"1.НП-1.1-1-15-1.1-1.3500-СЧ-1,6-1.1-150-У"]
["Danfoss","VM2",15,"1,6","065B2014",null,null,null,"КПСР",null,"1.НП-1.1-1-15-1,6-1.3500-СЧ-1,6-1.1-150-У"]
["Danfoss","VM2",15,"2,5","065B2015",null,null,null,"КПСР",null,"1.НП-1.1-1-15-2,5-1.3500-СЧ-1,6-1.1-150-У"]
["Danfoss","VM2",20,"4","065B2016",null,null,null,"КПСР",null,"1.НП-1.1-1-20-4-1.3500-СЧ-1,6-1.1-150-У"]
["Danfoss","VM2",20,"6,3","065B2027",null,null,null,"КПСР",null,"1.НП-1.1-1-20-6,3-1.3500-СЧ-1,6-1.1-150-У"]
["Danfoss","VM2",25,"6,3","065B2017",null,null,null,"КПСР",null,"1.НП-1.1-1-25-6,3-1.3500-СЧ-1,6-1.1-150-У"]
["Danfoss","VM2",25,"8","065B2028",null,null,null,"КПСР",null,"1.НП-1.1-1-25-8-1.3500-СЧ-1,6-1.1-150-У"]
["Danfoss","VM2",32,"10","065B2018",null,null,null,"КПСР",null,"1.НП-1.1-1-32-10-1.3501-СЧ-1,6-1.1-150-У"]
["Danfoss","VM2",40,"16","065B2019",null,null,null,"КПСР",null,"1.НП-1.1-1-40-16-1.3501-СЧ-1,6-1.1-150-У"]
["Danfoss","VM2",50,"25","065B2020",null,null,null,"КПСР",null,"1.НП-1.1-1-50-25-1.3501-СЧ-1,6-1.1-150-У"]
[]
[null,null,null,null,null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
[null,null,null,null,null,null,null,null,null,584390,"- маркировка привода"]

{"sheet":"Серия VRB2","index":17,"n_rows":43,"n_cols":15,"rows_kept":43,"cut":false,"hidden":true,"merged":[[15,9,15,14],[15,1,15,6],[30,5,36,7],[14,2,14,6],[1,6,1,11],[2,6,2,11],[3,6,3,11],[11,9,12,14],[11,1,12,6],[14,9,14,10],[14,12,14,14],[14,7,14,8],[16,9,16,14],[22,9,22,14]]}
[]
[null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,"VRB 2",null,null,null,null,null,null,null,"Клапана КПСР серии 110"]
[]
[null,"Рабочее давление: 1,6 МПа (16 атм)",null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,"Материал корпуса: Красная бронза (Rg 5)",null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,"Рабочая температура: max +130°С",null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,15,20,25,32,40,50,null,null,15,20,25,32,40,50]
[null,10,15,null,null,null,null,"Ход штока клапана",null,5,null,7,10]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,null,null,null,null,null,null,null,null,"Основные значения"]
[null,0.25,4,6.3,10,16,25,null,null,0.25,4,6.3,10,16,25]
[null,0.4,6.3,8,null,null,null,null,null,0.4,6.3,8]
[null,0.63,null,null,null,null,null,null,null,0.63]
[null,1,null,null,null,null,null,null,null,1]
[null,1.6,null,null,null,null,null,null,null,1.6]
[null,2.5,null,null,null,null,null,null,null,"Дополнительные значения"]
[null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10]
[null,null,null,null,null,null,null,null,null,3.2,2.5,2.5,16,20,16]
[null,null,null,null,null,null,null,null,null,4,null,4,null,25,32]
[null,null,null,null,null,null,null,null,null,null,null,10,null,null,40]
[]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[]
["Danfoss","VRB2",15,"0,63","065Z0171","Соответствие",null,null,"КПСР",null,"1.НП-1.1-1-15-0,63-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"1","065Z0172",null,null,null,"КПСР",null,"1.НП-1.1-1-15-1.1-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"1,6","065Z0173",null,null,null,"КПСР",null,"1.НП-1.1-1-15-1,6-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"2,5","065Z0174",null,null,null,"КПСР",null,"1.НП-1.1-1-15-2,5-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"4","065Z0175",null,null,null,"КПСР",null,"1.НП-1.1-1-15-4-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",20,"6,3","065Z0176",null,null,null,"КПСР",null,"1.НП-1.1-1-20-6,3-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",25,"10","065Z0177",null,null,null,"КПСР",null,"1.НП-1.1-1-25-10-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",32,"16","065Z0178",null,null,null,"КПСР",null,"1.НП-1.1-1-32-16-1.3501-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",40,"25","065Z0179",null,null,null,"КПСР",null,"1.НП-1.1-1-40-25-1.3501-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",50,"40","065Z0180",null,null,null,"КПСР",null,"1.НП-1.1-1-50-40-1.3501-СЧ-1,6-1-150-У"]
[]
[null,null,null,null,null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
[null,null,null,null,null,null,null,null,null,584390,"- маркировка привода"]

{"sheet":"Серия VRG2","index":18,"n_rows":42,"n_cols":15,"rows_kept":42,"cut":false,"hidden":true,"merged":[[15,9,15,14],[15,1,15,6],[29,5,35,7],[14,2,14,6],[1,6,1,11],[2,6,2,11],[3,6,3,11],[11,9,12,14],[11,1,12,6],[14,9,14,10],[14,12,14,14],[14,7,14,8],[16,9,16,14],[22,9,22,14]]}
[]
[null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,"VRG 2",null,null,null,null,null,null,null,"Клапан КПСР серии 110"]
[]
[null,"Рабочее давление: 1,6 МПа (16 атм)",null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,"Материал корпуса: Серый чугун (GG-25)",null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,"Рабочая температура: max +130°С",null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,15,20,25,32,40,50,null,null,15,20,25,32,40,50]
[null,10,15,null,null,null,null,"Ход штока клапана",null,5,null,7,10]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,null,null,null,null,null,null,null,null,"Основные значения"]
[null,0.63,6.3,10,16,25,40,null,null,0.63,6.3,10,16,25,40]
[null,1,null,null,null,null,null,null,null,1]
[null,1.6,null,null,null,null,null,null,null,1.6]
[null,2.5,null,null,null,null,null,null,null,4]
[null,4]
[null,null,null,null,null,null,null,null,null,"Дополнительные значения"]
[null,null,null,null,null,null,null,null,null,0.16,4,1.6,6.3,10,10]
[null,null,null,null,null,null,null,null,null,0.25,1.6,2.5,10,20,16]
[null,null,null,null,null,null,null,null,null,0.4,2.5,4,null,16,25]
[null,null,null,null,null,null,null,null,null,3.2,null,6.3,null,null,32]
[null,null,null,null,null,null,null,null,null,null,null,8]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
["Danfoss","VRB2",15,"0,63","065Z0131","Соответствие",null,null,"КПСР",null,"1.НП-1.1-1-15-0,63-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"1","065Z0132",null,null,null,"КПСР",null,"1.НП-1.1-1-15-1-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"1,6","065Z0133",null,null,null,"КПСР",null,"1.НП-1.1-1-15-1,6-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"2,5","065Z0134",null,null,null,"КПСР",null,"1.НП-1.1-1-15-2,5-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"4","065Z0135",null,null,null,"КПСР",null,"1.НП-1.1-1-15-4-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",20,"6,3","065Z0136",null,null,null,"КПСР",null,"1.НП-1.1-1-20-6,3-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",25,"10","065Z0137",null,null,null,"КПСР",null,"1.НП-1.1-1-25-10-1.3500-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",32,"16","065Z0138",null,null,null,"КПСР",null,"1.НП-1.1-1-32-16-1.3501-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",40,"25","065Z0139",null,null,null,"КПСР",null,"1.НП-1.1-1-40-25-1.3501-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",50,"40","065Z0140",null,null,null,"КПСР",null,"1.НП-1.1-1-50-40-1.3501-СЧ-1,6-1-150-У"]
[]
[null,null,null,null,null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
[null,null,null,null,null,null,null,null,null,584390,"- маркировка привода"]

{"sheet":"Серия VL3","index":19,"n_rows":52,"n_cols":23,"rows_kept":52,"cut":false,"hidden":true,"merged":[[14,4,14,6],[14,7,14,8],[15,14,15,22],[15,1,15,9],[36,5,42,7],[14,14,14,15],[14,16,14,17],[14,18,14,20],[14,1,14,3],[14,10,14,13],[16,14,16,22],[21,14,21,22],[1,8,1,13],[2,8,2,13],[3,8,3,13],[11,14,12,22],[11,1,12,9]]}
[]
[null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,null,"VL3",null,null,null,null,null,null,null,null,null,null,null,null,"Клапана КССР серии 100"]
[]
[null,"Рабочее давление: 0,6 МПа (6 атм)",null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,"Рабочая температура: max +120°С",null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,15,20,25,32,40,50,65,80,100,null,null,null,null,15,20,25,32,40,50,65,80,100]
[null,10,null,null,15,null,null,20,null,25,"Ход штока клапана",null,null,null,10,null,20,null,32,null,null,32,40]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Основные значения"]
[null,"0,63",6.3,10,16,25,40,63,100,145,null,null,null,null,0.63,6.3,"10",16,"25","40","63","100","160"]
[null,"1",null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,1.6,null,null,null,null,null,null,null,null,null,null,null,null,1.6]
[null,"2,5",null,null,null,null,null,null,null,null,null,null,null,null,4]
[null,"4",null,null,null,null,null,null,null,null,null,null,null,null,"Дополнительные значения"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,1.6,1.6,6.3,10,16,"25","40",80]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.2,2.5,2.5,10,16,25,40,"63","100"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,4,null,null,null,null,80,"125"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[]
[]
[]
[]
[]
[]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[]
[]
["Danfoss","VL3",15,"0,63","065Z0351","Соответствие",null,null,"КССР",null,"1.НП-15-0,63-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL3",15,"1","065Z0352",null,null,null,"КССР",null,"1.НП-15-1-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL3",15,"1,6","065Z0353",null,null,null,"КССР",null,"1.НП-15-1,6-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL3",15,"2,5","065Z0354",null,null,null,"КССР",null,"1.НП-15-2,5-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL3",15,"4","065Z0355",null,null,null,"КССР",null,"1.НП-15-4-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL3",20,"6,3","065Z0356",null,null,null,"КССР",null,"1.НП-20-6,3-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL3",25,"10","065Z0357",null,null,null,"КССР",null,"1.НП-25-10-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL3",32,"16","065Z0358",null,null,null,"КССР",null,"1.НП-32-16-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL3",40,"25","065Z0359",null,null,null,"КССР",null,"1.НП-40-25-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL3",50,"40","065Z0360",null,null,null,"КССР",null,"1.НП-50-40-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL3",65,"63","065Z0361",null,null,null,"КССР",null,"1.НП-65-63-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL3",80,"100","065Z0362",null,null,null,"КССР",null,"1.НП-80-100-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VL3",100,"145","065Z3413",null,null,null,"КССР",null,"1.НП-100-145-Х.ХХХХ-СЧ-1,6-1-150-У"]
[]
[null,null,null,null,null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
[null,null,null,null,null,null,null,null,null,"Х.ХХХХ","- маркировка привода"]

{"sheet":"Серия VF3","index":20,"n_rows":54,"n_cols":25,"rows_kept":54,"cut":false,"hidden":true,"merged":[[15,16,15,24],[15,1,15,11],[36,5,42,7],[14,2,14,6],[14,7,14,8],[14,10,14,11],[14,16,14,17],[14,18,14,19],[14,20,14,22],[14,12,14,15],[16,16,16,24],[21,16,21,24],[1,8,1,13],[2,8,2,13],[3,8,3,13],[11,16,12,24],[11,1,12,11]]}
[]
[null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,null,"VF3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Клапана КССР серии 100"]
[]
[null,"Рабочее давление: 1,6 МПа (16 атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,"Рабочая температура: max +130 (150) °С",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,15,20,25,32,40,50,65,80,100,125,150,null,null,null,null,15,20,25,32,40,50,65,80,100]
[null,10,15,null,null,null,null,20,null,30,40,null,"Ход штока клапана",null,null,null,10,null,20,null,32,null,null,32,40]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Основные значения"]
[null,"0,63",6.3,10,16,25,40,63,100,145,220,320,null,null,null,null,0.63,6.3,"10",16,"25","40","63","100","160"]
[null,"1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,1.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6]
[null,"2,5",null,null,null,null,null,null,null,null,null,null,null,null,null,null,4]
[null,"4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Дополнительные значния"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,1.6,1.6,6.3,10,16,"25","40",80]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.2,2.5,2.5,10,16,25,40,"63","100"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,4,null,null,null,"56",80,"125"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[]
[]
[]
[]
[]
[]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[]
[]
["Danfoss","VF3",15,"0,63","065Z0251","Соответствие",null,null,"КССР",null,"1.НП-15-0,63-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VF3",15,"1","065Z0252",null,null,null,"КССР",null,"1.НП-15-1-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VF3",15,"1,6","065Z0253",null,null,null,"КССР",null,"1.НП-15-1,6-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VF3",15,"2,5","065Z0254",null,null,null,"КССР",null,"1.НП-15-2,5-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VF3",15,"4","065Z0255",null,null,null,"КССР",null,"1.НП-15-4-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VF3",20,"6,3","065Z0256",null,null,null,"КССР",null,"1.НП-20-6,3-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VF3",25,"10","065Z0257",null,null,null,"КССР",null,"1.НП-25-10-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VF3",32,"16","065Z0258",null,null,null,"КССР",null,"1.НП-32-16-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VF3",40,"25","065Z0259",null,null,null,"КССР",null,"1.НП-40-25-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VF3",50,"40","065Z0260",null,null,null,"КССР",null,"1.НП-50-40-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VF3",65,"63","065Z0261",null,null,null,"КССР",null,"1.НП-65-63-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VF3",80,"100","065Z0262",null,null,null,"КССР",null,"1.НП-80-100-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VF3",100,"145","065Z1685",null,null,null,"КССР",null,"1.НП-100-145-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VF3",125,"220","065B3125"]
["Danfoss","VF3",150,"320","065B3150"]
[]
[null,null,null,null,null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
[null,null,null,null,null,null,null,null,null,"Х.ХХХХ","- маркировка привода"]

{"sheet":"Серия VRB3","index":21,"n_rows":41,"n_cols":15,"rows_kept":41,"cut":false,"hidden":true,"merged":[[15,9,15,14],[15,1,15,6],[28,5,34,7],[1,6,1,11],[2,6,2,11],[3,6,3,11],[11,9,12,14],[11,1,12,6],[14,9,14,10],[14,12,14,14],[14,7,14,8],[14,2,14,6],[16,9,16,14],[21,9,21,14]]}
[]
[null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,"VRB 3",null,null,null,null,null,null,null,"Клапана КССР серии 100"]
[]
[null,"Рабочее давление: 1,6 МПа (16 атм)",null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,"Материал корпуса: Красная бронза (Rg 5)",null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,"Рабочая температура: max +130°С",null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,15,20,25,32,40,50,null,null,15,20,25,32,40,50]
[null,10,15,null,null,null,null,"Ход штока клапана",null,5,null,7,10]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,0.63,6.3,10,16,25,40,null,null,"Основные значения"]
[null,1,null,null,null,null,null,null,null,0.63,6.3,10,16,25,40]
[null,1.6,null,null,null,null,null,null,null,1]
[null,2.5,null,null,null,null,null,null,null,1.6]
[null,4,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,"Дополнительные значения"]
[null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10]
[null,null,null,null,null,null,null,null,null,0.25,2.5,2.5,10,16,16]
[null,null,null,null,null,null,null,null,null,0.4,4,4,null,20,25]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании",null,null,null,null,null,null,null,null,3.2,null,6.3,null,null,32]
[null,null,null,null,null,null,null,null,null,null,null,8]
[]
["Danfoss","VRB2",15,"0,63","065Z0151","Соответствие",null,null,"КССР",null,"1.НП-15-0,63-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"1","065Z0152",null,null,null,"КССР",null,"1.НП-15-1-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"1,6","065Z0153",null,null,null,"КССР",null,"1.НП-15-1,6-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"2,5","065Z0154",null,null,null,"КССР",null,"1.НП-15-2,5-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"4","065Z0155",null,null,null,"КССР",null,"1.НП-15-4-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",20,"6,3","065Z0156",null,null,null,"КССР",null,"1.НП-20-6,3-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",25,"10","065Z0157",null,null,null,"КССР",null,"1.НП-25-10-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",32,"16","065Z0158",null,null,null,"КССР",null,"1.НП-32-16-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",40,"25","065Z0159",null,null,null,"КССР",null,"1.НП-40-25-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",50,"40","065Z0160",null,null,null,"КССР",null,"1.НП-50-40-Х.ХХХХ-СЧ-1,6-1-150-У"]
[]
[null,null,null,null,null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
[null,null,null,null,null,null,null,null,null,"Х.ХХХХ","- маркировка привода"]

{"sheet":"Серия VRG3","index":22,"n_rows":41,"n_cols":15,"rows_kept":41,"cut":false,"hidden":true,"merged":[[15,9,15,14],[15,1,15,6],[28,5,34,7],[1,6,1,11],[2,6,2,11],[3,6,3,11],[11,9,12,14],[11,1,12,6],[14,9,14,10],[14,12,14,14],[14,7,14,8],[14,2,14,6],[16,9,16,14],[21,9,21,14]]}
[]
[null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,"VRG 3",null,null,null,null,null,null,null,"Клапана КССР серии100"]
[]
[null,"Рабочее давление: 1,6 МПа (16 атм)",null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,"Материал корпуса: Серый чугун (GG-25)",null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,"Рабочая температура: max +130°С",null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[]
[null,"Dn, мм",null,null,null,null,null,null,null,"Dn, мм"]
[]
[null,15,20,25,32,40,50,null,null,15,20,25,32,40,50]
[null,10,15,null,null,null,null,"Ход штока клапана",null,5,null,7,10]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
[null,0.63,6.3,10,16,25,40,null,null,"Основные значения"]
[null,1,null,null,null,null,null,null,null,0.63,6.3,10,16,25,40]
[null,1.6,null,null,null,null,null,null,null,1]
[null,2.5,null,null,null,null,null,null,null,1.6]
[null,4,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,"Дополнительные значения"]
[null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10]
[null,null,null,null,null,null,null,null,null,0.25,2.5,2.5,10,16,16]
[null,null,null,null,null,null,null,null,null,0.4,4,4,null,20,25]
["Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании",null,null,null,null,null,null,null,null,3.2,null,6.3,null,null,32]
[null,null,null,null,null,null,null,null,null,null,null,8]
[]
["Danfoss","VRB2",15,"0,63","065Z0111","Соответствие",null,null,"КССР",null,"1.НП-15-0,63-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"1","065Z0112",null,null,null,"КССР",null,"1.НП-15-1-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"1,6","065Z0113",null,null,null,"КССР",null,"1.НП-15-1,6-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"2,5","065Z0114",null,null,null,"КССР",null,"1.НП-15-2,5-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",15,"4","065Z0115",null,null,null,"КССР",null,"1.НП-15-4-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",20,"6,3","065Z0116",null,null,null,"КССР",null,"1.НП-20-6,3-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",25,"10","065Z0117",null,null,null,"КССР",null,"1.НП-25-10-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",32,"16","065Z0118",null,null,null,"КССР",null,"1.НП-32-16-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",40,"25","065Z0119",null,null,null,"КССР",null,"1.НП-40-25-Х.ХХХХ-СЧ-1,6-1-150-У"]
["Danfoss","VRB2",50,"40","065Z0120",null,null,null,"КССР",null,"1.НП-50-40-Х.ХХХХ-СЧ-1,6-1-150-У"]
[]
[null,null,null,null,null,null,null,null,null,"НП","- номер проектировщика (присваивается произодителем)"]
[null,null,null,null,null,null,null,null,null,"Х.ХХХХ","- маркировка привода"]

{"sheet":"Серия AVP","index":23,"n_rows":41,"n_cols":26,"rows_kept":41,"cut":false,"hidden":true,"merged":[[28,13,29,16],[27,14,27,15],[27,4,27,6],[27,11,27,12],[16,1,16,7],[16,10,16,15],[20,10,20,15],[5,19,5,20],[5,21,5,25],[6,19,7,19],[6,20,7,20],[17,10,17,15],[1,7,1,12],[2,7,2,12],[3,7,3,12],[13,1,14,7],[13,10,14,15]]}
[]
[null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,"AVP",null,null,null,null,null,null,null,null,"Регулятор перепада давления РА серии 100",null,null,null,null,null,null,null,null,"Danfoss",null,"КПСР-Групп"]
[null,null,null,null,null,null,null,null,null,null,"для внутренних сетей и ИТП",null,null,null,null,null,null,null,null,"0,2-1","0,3-2",0,1,2,3,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Бар",null,null,"0,1-1","0,4-1,6","1-4","3-7","6-12"]
[null,"Рабочее давление: 2,5 МПа (25 атм)",null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 (16); 2,5 (25) МПа (атм)",null,null,null,null,null,null,null,0.1]
[null,"Материал корпуса: Высокопрочный чугун (EN-GJS-400-18-LT)",null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,0.2]
[null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Высокопрочный чугун (EN-JS 1025)",null,null,null,null,null,null,null,0.3]
[null,"Рабочая температура: max +150°С",null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С",null,null,null,null,null,null,null,0.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.7]
[null,"Dn, мм",null,null,null,null,null,null,null,null,"Dn, мм",null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6]
[null,15,20,25,32,null,40,50,null,null,15,20,25,32,40,50,null,null,2]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,3]
[null,1.6,6.3,8,12.5,null,20,25,null,null,"Основные значения",null,null,null,null,null,null,null,4]
[null,2.5,null,null,null,null,null,null,null,null,1.6,6.3,8,16,20,25,null,null,5]
[null,4,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,6]
[null,null,null,null,null,null,null,null,null,null,"Дополнительные значения",null,null,null,null,null,null,null,7]
[null,null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10,null,null,8]
[null,null,null,null,null,null,null,null,null,null,0.25,2.5,2.5,10,16,16,null,null,10]
[null,null,null,null,null,null,null,null,null,null,0.4,4,4,null,25,32,null,null,12]
[null,null,null,null,null,null,null,null,null,null,0.63,null,6.3,null,null,40,null,null,16]
[null,null,null,null,null,null,null,null,null,null,1,null,10]
[null,null,null,null,null,null,null,null,null,null,3.2]
[null,null,null,null,"трубопровод",null,null,null,null,null,null,"трубопровод",null,null,"Заменить",null,null,null,"Диапазону 0,2-1 соответствует диапазон 0,1-1"]
[null,null,null,null,"Обратный ",null,"Подающий",null,null,null,null,"Обратный ","Подающий"," значение -Х- на 0, 1 или 2 в зависимости от диапазона настройки согласно таблице ",null,null,null,null,"Диапазону 0,3-2 соответствует диапазон 0,1-1,6 или 1-4"]
[null,null,null,null,"Настройка 0,2-1,0",null,"Настройка 0,2-1,0",null,null,null,null,"Настройка 0,3-2,0","Настройка 0,3-2,0",null,null,null,null,null,"Значение настраемого давления должно находится в среднем значении диапазона"]
["Danfoss","AVP",15,"1,6","003H06283",null,"003H6315","РА-М","42-1-15-1,6-0-СЧ-1,6-1-150-У",null,null,"003H06293","003H6325","РА-М","42-1-15-1,6-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVP",15,"2,5","003H06284",null,"003H6316","РА-М","42-1-15-2,5-0-СЧ-1,6-1-150-У",null,null,"003H06294","003H6326","РА-М","42-1-15-2,5-Х-СЧ-1,6-1-150-У",null,null,null,"Также можно заказать регулятор с другими диапазона из таблицы"]
["Danfoss","AVP",15,"4","003H06285",null,"003H6317","РА-М","42-1-15-4-0-СЧ-1,6-1-150-У",null,null,"003H06295","003H6327","РА-М","42-1-15-4-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVP",20,6.3,"003H06286",null,"003H6318","РА-М","42-1-20-6,3-0-СЧ-1,6-1-150-У",null,null,"003H06296","003H6328","РА-М","42-1-20-6,3-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVP",25,"8","003H06287",null,"003H6319","РА-М","42-1-25-8-0-СЧ-1,6-1-150-У",null,null,"003H06297","003H6329","РА-М","42-1-25-8-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVP",15,"4","003H06345",null,"003H6369","РА-М","42-1-15-4-0-СЧ-1,6-1-150-У",null,null,"003H06351","003H6375","РА-М","42-1-15-4-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVP",20,"6,3","003H06346",null,"003H6370","РА-М","42-1-20-6,3-0-СЧ-1,6-1-150-У",null,null,"003H06352","003H6376","РА-М","42-1-20-6,3-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVP",25,"8","003H06347",null,"003H6371","РА-М","42-1-20-8-0-СЧ-1,6-1-150-У",null,null,"003H06353","003H6377","РА-М","42-1-20-8-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVP",32,"12,5","003H06348",null,"003H6372","РА-М","42-1-32-16-0-СЧ-1,6-1-150-У",null,null,"003H06354","003H6378","РА-М","42-1-32-16-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVP",40,20,"003H06349",null,"003H6373","РА-М","42-1-40-20-0-СЧ-1,6-1-150-У",null,null,"003H06355","003H6379","РА-М","42-1-40-20-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVP",50,25,"003H06350",null,"003H6374","РА-М","42-1-50-25-0-СЧ-1,6-1-150-У",null,null,"003H06356","003H6380","РА-М","42-1-50-25-Х-СЧ-1,6-1-150-У"]

{"sheet":"Серия AVA","index":24,"n_rows":37,"n_cols":26,"rows_kept":37,"cut":false,"hidden":true,"merged":[[29,8,30,11],[17,10,17,15],[19,10,19,15],[1,7,1,12],[2,7,2,12],[3,7,3,12],[13,1,14,7],[13,10,14,15],[16,1,16,7],[16,10,16,15],[28,9,28,10],[5,19,5,20],[5,21,5,25],[5,18,7,18],[6,19,7,19],[6,20,7,20]]}
[]
[null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,"AVA",null,null,null,null,null,null,null,null,"Регулятор давления \"до себя\" РА серии 100",null,null,null,null,null,null,null,"Бар","Danfoss",null,"КПСР-Групп"]
[null,null,null,null,null,null,null,null,null,null,"для внутренних сетей и ИТП",null,null,null,null,null,null,null,null,"1-4,5","3-11",0,1,2,3,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0,1-1","0,4-1,6","1-4","3-7","6-12"]
[null,"Рабочее давление: 2,5 МПа (25 атм)",null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 (16); 2,5 (25) МПа (атм)",null,null,null,null,null,null,null,0.1]
[null,"Материал корпуса: Высокопрочный чугун (EN-GJS-400-18-LT)",null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,0.2]
[null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Высокопрочный чугун (EN-JS 1025)",null,null,null,null,null,null,null,0.3]
[null,"Рабочая температура: max +150°С",null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С",null,null,null,null,null,null,null,0.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.7]
[null,"Dn, мм",null,null,null,null,null,null,null,null,"Dn, мм",null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6]
[null,15,20,25,32,null,40,50,null,null,15,20,25,32,40,50,null,null,2]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,3]
[null,4,6.3,8,12.5,null,20,25,null,null,"Основные значения",null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,4,6.3,8,16,20,25,null,null,4.5]
[null,null,null,null,null,null,null,null,null,null,"Дополнительные значения",null,null,null,null,null,null,null,5]
[null,null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10,null,null,6]
[null,null,null,null,null,null,null,null,null,null,0.25,2.5,2.5,10,16,16,null,null,7]
[null,null,null,null,null,null,null,null,null,null,0.4,4,4,null,25,32,null,null,8]
[null,null,null,null,null,null,null,null,null,null,0.63,null,6.3,null,null,40,null,null,10]
[null,null,null,null,null,null,null,null,null,null,1,null,10,null,null,null,null,null,11]
[null,null,null,null,null,null,null,null,null,null,1.6,null,null,null,null,null,null,null,12]
[null,null,null,null,null,null,null,null,null,null,3.2,null,null,null,null,null,null,null,16]
[]
[null,null,null,null,null,null,null,null,null,"Заменить",null,null,null,null,null,null,null,null,"Диапазону 1-4,5 соответствует диапазон 1-4"]
[null,null,null,null,null,null,null,null," значение -Х- на 2, 3 или 4 в зависимости от диапазона настройки согласно таблице ",null,null,null,null,null,null,null,null,null,"Диапазону 3-11 соответствует диапазон 3-7 или 6-12"]
[null,null,null,null,"Настройка   1 - 4,5",null,"Настройка   3 - 11"]
["Danfoss","AVA",15,"4","003H06614",null,"003H6620",null,"РА-В","42-1-15-4-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,"Значение настраемого давления должно находится в среднем значении диапазона"]
["Danfoss","AVA",20,"6,3","003H06615",null,"003H6621",null,"РА-В","42-1-20-6,3-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVA",25,"8","003H06616",null,"003H6622",null,"РА-В","42-1-20-8-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,"Также можно заказать регулятор с другими диапазона из таблицы"]
["Danfoss","AVA",32,"12,5","003H06626",null,"003H6629",null,"РА-В","42-1-32-16-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVA",40,20,"003H06627",null,"003H6630",null,"РА-В","42-1-40-20-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVA",50,25,"003H06628",null,"003H6631",null,"РА-В","42-1-50-25-Х-СЧ-1,6-1-150-У"]

{"sheet":"Серия AVD","index":25,"n_rows":37,"n_cols":27,"rows_kept":37,"cut":false,"hidden":true,"merged":[[16,1,16,7],[16,10,16,15],[28,9,28,10],[17,10,17,15],[19,10,19,15],[1,7,1,12],[2,7,2,12],[3,7,3,12],[5,18,7,18],[13,1,14,7],[13,10,14,15],[5,19,5,20],[5,21,5,25],[6,19,7,19],[6,20,7,20],[29,8,30,11]]}
[]
[null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,"AVD",null,null,null,null,null,null,null,null,"Регулятор давления \"после себя\" РА серии 100",null,null,null,null,null,null,null,"Бар","Danfoss",null,"КПСР-Групп"]
[null,null,null,null,null,null,null,null,null,null,"для внутренних сетей и ИТП",null,null,null,null,null,null,null,null,"1-5","3-12",0,1,2,3,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0,1-1","0,4-1,6","1-4","3-7","6-12"]
[null,"Рабочее давление: 2,5 МПа (25 атм)",null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 (16); 2,5 (25) МПа (атм)",null,null,null,null,null,null,null,0.1]
[null,"Материал корпуса: Высокопрочный чугун (EN-GJS-400-18-LT)",null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,0.2]
[null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Высокопрочный чугун (EN-JS 1025)",null,null,null,null,null,null,null,0.3]
[null,"Рабочая температура: max +150°С",null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С",null,null,null,null,null,null,null,0.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.7,null,null,null,null,null,null,null,"Предлагаем все диапазоны"]
[null,"Dn, мм",null,null,null,null,null,null,null,null,"Dn, мм",null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6]
[null,15,20,25,32,null,40,50,null,null,15,20,25,32,40,50,null,null,2]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,3]
[null,4,6.3,8,12.5,null,20,25,null,null,"Основные значения",null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,4,6.3,8,16,20,25,null,null,5]
[null,null,null,null,null,null,null,null,null,null,"Дополнительные значения",null,null,null,null,null,null,null,6]
[null,null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10,null,null,7]
[null,null,null,null,null,null,null,null,null,null,0.25,2.5,2.5,10,16,16,null,null,8]
[null,null,null,null,null,null,null,null,null,null,0.4,4,4,null,25,32,null,null,10]
[null,null,null,null,null,null,null,null,null,null,0.63,null,6.3,null,null,40,null,null,11]
[null,null,null,null,null,null,null,null,null,null,1,null,10,null,null,null,null,null,12]
[null,null,null,null,null,null,null,null,null,null,1.6,null,null,null,null,null,null,null,16]
[null,null,null,null,null,null,null,null,null,null,3.2]
[]
[null,null,null,null,null,null,null,null,null,"Заменить",null,null,null,null,null,null,null,null,"Диапазону 1-4,5 соответствует диапазон 1-4 "]
[null,null,null,null,null,null,null,null," значение -Х- на 2, 3 или 4 в зависимости от диапазона настройки согласно таблице ",null,null,null,null,null,null,null,null,null,"Диапазону 3-12 соответствует диапазон 3-7 или 6-12"]
[null,null,null,null,"Настройка  1 - 5",null,"Настройка   3 - 12"]
["Danfoss","AVD",15,"4","003H06644",null,"003H6650",null,"РА-А","42-1-15-4-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,"Значение настраемого давления должно находится в среднем значении диапазона"]
["Danfoss","AVD",20,"6,3","003H06645",null,"003H6651",null,"РА-А","42-1-20-6,3-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVD",25,"8","003H06646",null,"003H6652",null,"РА-А","42-1-20-8-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,"Также можно заказать регулятор с другими диапазона из таблицы"]
["Danfoss","AVD",32,"12,5","003H06659",null,"003H6662",null,"РА-А","42-1-32-16-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVD",40,20,"003H06660",null,"003H6663",null,"РА-А","42-1-40-20-Х-СЧ-1,6-1-150-У"]
["Danfoss","AVD",50,25,"003H06661",null,"003H6664",null,"РА-А","42-1-50-25-Х-СЧ-1,6-1-150-У"]

{"sheet":"Серия AVDS","index":26,"n_rows":37,"n_cols":24,"rows_kept":37,"cut":false,"hidden":true,"merged":[[16,1,16,3],[16,8,16,10],[29,8,29,9],[17,8,17,10],[21,8,21,10],[1,4,1,10],[2,4,2,10],[3,4,3,10],[5,15,7,15],[13,1,14,3],[13,8,14,10],[5,16,5,17],[5,18,5,22],[6,16,7,16],[6,17,7,17],[30,7,31,10]]}
[]
[]
[]
[]
[]
[null,"AVDS",null,null,null,null,null,null,"Регулятор давления \"после себя\" РА серии 100",null,null,null,null,null,null,"Бар","Danfoss",null,"КПСР-Групп"]
[null,null,null,null,null,null,null,null,"для внутренних сетей и ИТП",null,null,null,null,null,null,null,"1-5","3-12",0,1,2,3,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0,1-1","0,4-1,6","1-4","3-7","6-12"]
[null,"Рабочее давление: 2,5 МПа (25 атм)",null,null,null,null,null,null,"Рабочее давление: 1,6 (16); 2,5 (25) МПа (атм)",null,null,null,null,null,null,0.1]
[null,"Материал корпуса: Высокопрочный чугун (EN-GJS-400-18-LT)",null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,0.2]
[null,null,null,null,null,null,null,null,"Материал корпуса: Высокопрочный чугун (EN-JS 1025)",null,null,null,null,null,null,0.3]
[null,"Рабочая температура: max +150°С",null,null,null,null,null,null,"Рабочая температура: max +150°С",null,null,null,null,null,null,0.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.7,null,null,null,null,null,null,null,"Предлагаем все диапазоны"]
[null,"Dn, мм",null,null,null,null,null,null,"Dn, мм",null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6]
[null,15,20,25,null,null,null,null,15,20,25,null,null,null,null,2]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,3]
[null,1,4.5,6.3,null,null,null,null,"Основные значения",null,null,null,null,null,null,4]
[null,1.6,null,null,null,null,null,null,1,4,6.3,null,null,null,null,4.5]
[null,3.2,null,null,null,null,null,null,1.6,null,null,null,null,null,null,5]
[null,null,null,null,null,null,null,null,3.2,null,null,null,null,null,null,6]
[null,null,null,null,null,null,null,null,"Дополнительные значения",null,null,null,null,null,null,7]
[null,null,null,null,null,null,null,null,0.16,1.6,1.6,null,null,null,null,8]
[null,null,null,null,null,null,null,null,0.25,2.5,2.5,null,null,null,null,10]
[null,null,null,null,null,null,null,null,0.4,6.3,4,null,null,null,null,11]
[null,null,null,null,null,null,null,null,0.63,null,8,null,null,null,null,12]
[null,null,null,null,null,null,null,null,4,null,10,null,null,null,null,16]
[]
[]
[null,null,null,null,null,null,null,null,"Заменить",null,null,null,null,null,null,"Диапазону 1-5 соответствует диапазон 1-4 или 3-7"]
[null,null,null,null,null,null,null," значение -Х- на 2, 3 или 4 в зависимости от диапазона настройки согласно таблице ",null,null,null,null,null,null,null,"Диапазону 3-12 соответствует диапазон 3-7 или 6-12"]
[null,null,null,null,"Настройка  1 - 5","Настройка   3 - 12"]
["Danfoss","AVDS",15,"1","003H06665","003H6670",null,"РА-А","42-2-15-4-Х-ВЧ-2,5-1-220-У",null,null,null,null,null,null,"Значение настраемого давления должно находится в среднем значении диапазона"]
["Danfoss","AVDS",15,"1,6","003H06666","003H6671",null,"РА-А","42-2-15-4-Х-ВЧ-2,5-1-220-У"]
["Danfoss","AVDS",15,"3,2","003H06667","003H6672",null,"РА-А","42-2-15-4-Х-ВЧ-2,5-1-220-У",null,null,null,null,null,null,"Также можно заказать регулятор с другими диапазона из таблицы"]
["Danfoss","AVDS",20,"4,5","003H06668","003H6673",null,"РА-А","42-2-15-4-Х-ВЧ-2,5-1-220-У"]
["Danfoss","AVDS",25,"6,3","003H06669","003H6674",null,"РА-А","42-2-15-4-Х-ВЧ-2,5-1-220-У"]

{"sheet":"Серия AFP-VFG2_16","index":27,"n_rows":41,"n_cols":39,"rows_kept":41,"cut":false,"hidden":true,"merged":[[26,14,26,15],[27,13,28,16],[15,15,15,27],[17,15,17,27],[9,30,16,30],[14,1,14,13],[14,15,14,27],[8,32,14,32],[15,31,23,31],[5,29,7,29],[5,30,5,33],[13,33,19,33],[7,22,8,22],[7,23,8,24],[11,1,12,13],[11,15,12,27],[1,12,1,14],[3,12,3,14],[5,34,5,38],[6,30,7,30],[6,33,7,33],[6,31,7,31],[6,32,7,32]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,"AFP/VFG2",null,null,null,null,null,null,null,null,null,null,null,null,null,"Регулятор перепада давления РА серии 100",null,null,null,null,null,null,null,null,null,null,null,null,null,"Бар","Danfoss",null,null,null,"КПСР-Групп"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0,15-1,5","1-6","0,1-0,7","0,5-3",0,1,2,3,4]
[null,"Рабочее давление: 1,6 (16) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 (16)МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0,1-1","0,4-1,6","1-4","3-7","6-12"]
[null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,null,null,null,null,null,null,0.1,null,null,"AFP"]
[null,"Рабочая температура: max +200°С",null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +220°С",null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,"AFP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.2]
[null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,null,0.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4]
[null,15,20,25,32,40,50,65,80,100,125,150,200,250,null,15,20,25,32,40,50,65,80,100,125,150,200,250,null,0.5,null,null,null,"AFP-9"]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,null,0.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Основные значения",null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"AFP-9"]
[null,"4","6,3","8","16","20","32",50,80,125,160,280,320,400,null,4,6.3,8,16,20,32,"50",80,"125","160",280,"360","400",null,1.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Дополнительные значения",null,null,null,null,null,null,null,null,null,null,null,null,null,1.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10,"16","40","63","100","160","250","450",null,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.25,2.5,2.5,10,16,16,"25","63",80,125,250,"450","630",null,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,4,4,null,25,25,32,"100","100","250","360","630","800",null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.63,null,6.3,null,null,40,"40",null,"160",null,null,null,1000,null,4.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"10",null,null,null,null,null,null,null,null,null,null,null,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6,null,null,null,null,null,63,null,null,null,null,null,null,null,6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.2,null,null,null,null,null,"80",null,null,null,null,null,null,null,7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[null,null,null,null,null,null,null,"VFG2",null,null,null,null,null,null,"Заменить",null,null,null,null,null,null,null,null,null,null,null,null,null,null,10]
[null,null,null,null,null,null,null,"Py=16",null,null,null,null,null," значение -Х- на 0, 1, 2 или 3 в зависимости от диапазона настройки согласно таблице ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11]
[null,"Danfoss",null,"AFP/VFG2",null,15,"4","065B2388",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12]
[null,"Danfoss",null,"AFP/VFG2",null,20,"6,3","065B2389",null,null,null,null,"РА-А","42-1-15-4-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,25,"8","065B2390",null,null,null,null,"РА-А","42-1-20-6,3-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Диапазону 0,15-1,5 соответствует диапазон 0,4-1,6"]
[null,"Danfoss",null,"AFP/VFG2",null,32,"16","065B2391",null,null,null,null,"РА-А","42-1-25-8-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Диапазону 1-6 соответствует диапазон 1-4 или 3-7"]
[null,"Danfoss",null,"AFP/VFG2",null,40,"20","065B2392",null,null,null,null,"РА-А","42-1-32-16-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Диапазону 0,1-0,7 соответствует диапазон 0,1-1"]
[null,"Danfoss",null,"AFP/VFG2",null,50,"32","065B2393",null,null,null,null,"РА-А","42-1-40-20-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Диапазону 0,5-3 соответствует диапазон 1-4"]
[null,"Danfoss",null,"AFP/VFG2",null,65,50,"065B2394",null,null,null,null,"РА-А","42-1-50-32-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,80,80,"065B2395",null,null,null,null,"РА-А","42-1-65-50-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Значение настраемого давления должно находится в среднем значении диапазона"]
[null,"Danfoss",null,"AFP/VFG2",null,100,125,"065B2396",null,null,null,null,"РА-А","42-1-80-80-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,125,160,"065B2397",null,null,null,null,"РА-А","42-1-100-125-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Также можно заказать регулятор с другими диапазона из таблицы"]
[null,"Danfoss",null,"AFP/VFG2",null,150,280,"065B2398",null,null,null,null,"РА-А","42-1-125-160-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,200,320,"065B2399",null,null,null,null,"РА-А","42-1-150-280-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,250,400,"065B2400",null,null,null,null,"РА-А","42-1-20-320-Х-СЧ-1,6-1-150-У"]

{"sheet":"Серия AFP-VFG2_25","index":28,"n_rows":40,"n_cols":34,"rows_kept":40,"cut":false,"hidden":true,"merged":[[28,7,28,10],[28,13,28,14],[28,15,29,18],[15,13,15,22],[17,13,17,22],[11,1,12,10],[11,13,12,22],[13,28,19,28],[15,26,23,26],[14,1,14,10],[14,13,14,22],[8,27,14,27],[7,22,8,22],[9,25,16,25],[1,14,1,16],[2,14,2,16],[5,24,7,24],[5,25,5,28],[5,29,5,33],[6,25,7,25],[6,26,7,26],[6,27,7,27],[6,28,7,28]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,"AFP/VFG2",null,null,null,null,null,null,null,null,null,null,null,"Регулятор перепада давления РА серии 200",null,null,null,null,null,null,null,null,null,null,"Бар","Danfoss",null,null,null,"КПСР-Групп"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0,15-1,5","1-7","0,1-0,7","0,5-3",0,1,2,3,4]
[null,"Рабочее давление: 2,5 (25) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 2,5 (25) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0,1-1","0,4-1,6","1-4","3-7","6-12"]
[null,"Материал корпуса: Высокопрочный чугун (EN-GJS-400-18-LT (GGG 40.3))",null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Высокопрочный чугун (EN-JS 1025)",null,null,null,null,null,null,null,null,null,null,0.1,null,null,"AFP"]
[null,"Рабочая температура: max +200°С",null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +220°С",null,null,null,null,null,null,null,null,null,null,0.15,"AFP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.2]
[null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,0.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4]
[null,15,20,25,32,40,50,65,80,100,125,null,null,15,20,25,32,40,50,65,80,100,125,null,0.5,null,null,null,"AFP-9"]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,0.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Основные значения",null,null,null,null,null,null,null,null,null,null,1,null,"AFP-9"]
[null,"4","6,3","8","16","20","32",50,80,125,160,null,null,4,6.3,8,16,20,32,"50",80,"125","160",null,1.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Дополнительные значения",null,null,null,null,null,null,null,null,null,null,1.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0.16,1.6,1.6,6.3,10,10,"16","40","63","100",null,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0.25,2.5,2.5,10,16,16,"25","63",80,125,null,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,4,4,null,25,25,32,"100","100","250",null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0.63,null,6.3,null,null,40,"40",null,"160",null,null,4.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"10",null,null,null,null,null,null,null,null,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,1.6,null,null,null,null,null,63,null,null,null,null,6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,3.2,null,null,null,null,null,"80",null,null,null,null,7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Заменить",null,null,null,null,null,null,null,11]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," значение -Х- на 1, 2, 3 или 4 в зависимости от диапазона настройки согласно таблице ",null,null,null,null,null,null,null,null,12]
[null,null,null,null,null,null,null,null,"Py = 25"]
[null,"Danfoss",null,"AFP/VFG2",null,15,"4",null,"065B2401",null,null,null,null,null,"РА-А","42-1-15-4-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,"Диапазону 0,15-1,5 соответствует диапазон 0,4-1,6"]
[null,"Danfoss",null,"AFP/VFG2",null,20,"6,3",null,"065B2402",null,null,null,null,null,"РА-А","42-1-20-6,3-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,"Диапазону 1-6 соответствует диапазон 1-4 или 3-7"]
[null,"Danfoss",null,"AFP/VFG2",null,25,"8",null,"065B2403",null,null,null,null,null,"РА-А","42-1-25-8-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,"Диапазону 0,1-0,7 соответствует диапазон 0,1-1"]
[null,"Danfoss",null,"AFP/VFG2",null,32,"16",null,"065B2404",null,null,null,null,null,"РА-А","42-1-32-16-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,"Диапазону 0,5-3 соответствует диапазон 1-4"]
[null,"Danfoss",null,"AFP/VFG2",null,40,"20",null,"065B2405",null,null,null,null,null,"РА-А","42-1-40-20-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,50,"32",null,"065B2406",null,null,null,null,null,"РА-А","42-1-50-32-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,"Значение настраемого давления должно находится в среднем значении диапазона"]
[null,"Danfoss",null,"AFP/VFG2",null,65,50,null,"065B2407",null,null,null,null,null,"РА-А","42-1-65-50-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,80,80,null,"065B2408",null,null,null,null,null,"РА-А","42-1-80-80-Х-СЧ-1,6-1-150-У",null,null,null,null,null,null,null,null,"Также можно заказать регулятор с другими диапазона из таблицы"]
[null,"Danfoss",null,"AFP/VFG2",null,100,125,null,"065B2409",null,null,null,null,null,"РА-А","42-1-100-125-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,125,160,null,"065B2410",null,null,null,null,null,"РА-А","42-1-125-160-Х-СЧ-1,6-1-150-У"]

{"sheet":"Серия AFA-VFG2","index":29,"n_rows":45,"n_cols":42,"rows_kept":45,"cut":false,"hidden":true,"merged":[[29,7,29,11],[6,32,7,32],[6,33,7,33],[11,21,12,21],[11,22,12,23],[15,1,16,13],[15,15,16,27],[18,1,18,13],[18,15,18,27],[7,22,8,22],[7,23,8,24],[9,24,10,24],[9,25,10,26],[28,20,28,21],[29,17,29,18],[29,19,31,22],[5,37,5,41],[6,30,7,30],[6,31,7,31],[6,36,7,36],[1,12,1,14],[2,12,2,14],[3,12,3,14],[5,29,7,29],[5,30,5,36],[6,34,7,34],[6,35,7,35]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,"AFA/VFG2",null,null,null,null,null,null,null,null,null,null,null,null,null,"Регулятор перепада давления РА серии 100, 200, 210",null,null,null,null,null,null,null,null,null,null,null,null,null,"Бар","Danfoss",null,null,null,null,null,null,"КПСР-Групп"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3-11","10-16","1-5","0,5-2,5","0,15-1,2","0,1-0,6","0,05-0,35",0,1,2,3,4]
[null,"Рабочее давление: 1,6 (16) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 (16)МПа (атм)",null,null,null,null,null,null,"}","Серия 100",null,null,null,null,null,null,null,null,null,null,null,null,null,"0,1-1","0,4-1,6","1-4","3-7","6-12"]
[null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,null,null,null,null,null,null,0.05]
[null,"Рабочее давление: 2,5 (25) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 2,5 (25) МПа (атм)",null,null,null,null,null,null,null,null,"}","Серия 200",null,null,null,0.1]
[null,"Материал корпуса: Высокопрочный чугун (EN-GJS-400-18-LT (GGG 40.3))",null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Высокопрочный чугун (EN-JS 1025)",null,null,null,null,null,null,null,null,null,null,null,null,null,0.15]
[null,"Рабочее давление: 4 (40) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 4 (40) МПа (атм)",null,null,null,null,null,"}","Серия 210",null,null,null,null,null,null,0.35]
[null,"Материал корпуса: Сталь 20 (GP240GH (GS-C 25))",null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Сталь 20 (1.0443)",null,null,null,null,null,null,null,null,null,null,null,null,null,0.4]
[null,"Рабочая температура: max +200°С",null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +260°С",null,null,null,null,null,null,null,null,null,null,null,null,null,0.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.6]
[null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,null,0.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,15,20,25,32,40,50,65,80,100,125,150,200,250,null,15,20,25,32,40,50,65,80,100,125,150,200,250,null,1.2]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,null,1.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.16,null,null,null,null,null,null,null,null,null,null,null,null,null,2.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.25,1.6,1.6,6.3,10,10,"16","40","63","100","160","250","400",null,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,2.5,2.5,10,16,16,"25","63",80,125,250,"360","450",null,4]
[null,"4","6,3","8","16","20","32",50,80,125,160,280,320,400,null,0.63,4,4,16,20,25,32,80,"100","160","360","450","630",null,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,6.3,6.3,null,25,32,"40","100","125","250",null,"630","800",null,6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6,null,8,null,null,40,"50",null,"160",null,null,null,1000,null,7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.2,null,"10",null,null,null,63,null,null,null,null,null,null,null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,"80",null,null,null,null,null,null,null,10]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Заменить",null,null,null,null,null,null,null,null,12]
[null,null,null,null,null,null,null,"VFG2",null,null,null,null,null,null,null,null,null,null,null," значение -Х- на 1, 2, 3 или 4 в зависимости от диапазона настройки согласно таблице ",null,null,null,null,null,null,null,null,null,16]
[]
[null,null,null,null,null,null,null,"Py=16",null,"Py = 25",null,"Py = 40"]
[null,"Danfoss",null,"AFP/VFG2",null,15,"4","065B2388",null,"065B2401",null,"065B2411",null,null,null,null,null,null,"РА-А","42-1-15-4-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,20,"6,3","065B2389",null,"065B2402",null,"065B2412",null,null,null,null,null,null,"РА-А","42-1-20-6,3-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,25,"8","065B2390",null,"065B2403",null,"065B2413",null,null,null,null,null,null,"РА-А","42-1-25-8-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,32,"16","065B2391",null,"065B2404",null,"065B2414",null,null,null,null,null,null,"РА-А","42-1-32-16-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,40,"20","065B2392",null,"065B2405",null,"065B2415",null,null,null,null,null,null,"РА-А","42-1-40-20-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,50,"32","065B2393",null,"065B2406",null,"065B2416",null,null,null,null,null,null,"РА-А","42-1-50-32-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,65,50,"065B2394",null,"065B2407",null,"065B2417",null,null,null,null,null,null,"РА-А","42-1-65-50-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,80,80,"065B2395",null,"065B2408",null,"065B2418",null,null,null,null,null,null,"РА-А","42-1-80-80-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,100,125,"065B2396",null,"065B2409",null,"065B2419",null,null,null,null,null,null,"РА-А","42-1-100-125-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,125,160,"065B2397",null,"065B2410",null,"065B2420",null,null,null,null,null,null,"РА-А","42-1-125-160-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,150,280,"065B2398",null,null,null,"065B2421",null,null,null,null,null,null,"РА-А","42-1-150-280-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,200,320,"065B2399",null,null,null,"065B2422",null,null,null,null,null,null,"РА-А","42-1-20-320-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,250,400,"065B2400"]

{"sheet":"Серия AFD-VFG2","index":30,"n_rows":45,"n_cols":41,"rows_kept":45,"cut":false,"hidden":true,"merged":[[9,24,10,24],[9,25,10,26],[28,20,28,21],[29,7,29,11],[29,17,29,18],[29,19,31,22],[11,21,12,21],[11,22,12,23],[15,1,16,13],[15,15,16,27],[18,1,18,13],[18,15,18,27],[1,12,1,14],[2,12,2,14],[3,12,3,14],[5,29,7,29],[5,30,5,35],[6,34,7,34],[6,35,7,35],[7,22,8,22],[7,23,8,24],[5,36,5,40],[6,30,7,30],[6,31,7,31],[6,33,7,33],[6,32,7,32]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,"AFD/VFG2",null,null,null,null,null,null,null,null,null,null,null,null,null,"Регулятор  давления \"после себя\" РА серии 100, 200, 210",null,null,null,null,null,null,null,null,null,null,null,null,null,"Бар","Danfoss",null,null,null,null,null,"КПСР-Групп"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10-16","3-12","0,5-3","1-6","0,1-0,7","0,15-1,5",0,1,2,3,4]
[null,"Рабочее давление: 1,6 (16) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 (16)МПа (атм)",null,null,null,null,null,null,"}","Серия 100",null,null,null,null,null,null,null,null,null,null,null,null,"0,1-1","0,4-1,6","1-4","3-7","6-12"]
[null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)",null,null,null,null,null,null,null,null,null,null,null,null,null,0.05]
[null,"Рабочее давление: 2,5 (25) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 2,5 (25) МПа (атм)",null,null,null,null,null,null,null,null,"}","Серия 200",null,null,null,0.1]
[null,"Материал корпуса: Высокопрочный чугун (EN-GJS-400-18-LT (GGG 40.3))",null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Высокопрочный чугун (EN-JS 1025)",null,null,null,null,null,null,null,null,null,null,null,null,null,0.15]
[null,"Рабочее давление: 4 (40) МПа (атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 4 (40) МПа (атм)",null,null,null,null,null,"}","Серия 210",null,null,null,null,null,null,0.35]
[null,"Материал корпуса: Сталь 20 (GP240GH (GS-C 25))",null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Сталь 20 (1.0443)",null,null,null,null,null,null,null,null,null,null,null,null,null,0.4]
[null,"Рабочая температура: max +200°С",null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +260°С",null,null,null,null,null,null,null,null,null,null,null,null,null,0.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.6]
[null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,null,"Dn, мм",null,null,null,null,null,null,null,null,null,null,null,null,null,0.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,15,20,25,32,40,50,65,80,100,125,150,200,250,null,15,20,25,32,40,50,65,80,100,125,150,200,250,null,1.2]
[null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч",null,null,null,null,null,null,null,null,null,null,null,null,null,1.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.16,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.25,1.6,1.6,6.3,10,10,"16","40","63","100","160","250","400",null,2.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,2.5,2.5,10,16,16,"25","63",80,125,250,"360","450",null,3]
[null,"4","6,3","8","16","20","32",50,80,125,160,280,320,400,null,0.63,4,4,16,20,25,32,80,"100","160","360","450","630",null,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,6.3,6.3,null,25,32,"40","100","125","250",null,"630","800",null,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.6,null,8,null,null,40,"50",null,"160",null,null,null,1000,null,6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.2,null,"10",null,null,null,63,null,null,null,null,null,null,null,7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,"80",null,null,null,null,null,null,null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Заменить",null,null,null,null,null,null,null,null,11]
[null,null,null,null,null,null,null,"VFG2",null,null,null,null,null,null,null,null,null,null,null," значение -Х- на 1, 2, 3 или 4 в зависимости от диапазона настройки согласно таблице ",null,null,null,null,null,null,null,null,null,12]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16]
[null,null,null,null,null,null,null,"Py=16",null,"Py = 25",null,"Py = 40"]
[null,"Danfoss",null,"AFP/VFG2",null,15,"4","065B2388",null,"065B2401",null,"065B2411",null,null,null,null,null,null,"РА-А","42-1-15-4-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,20,"6,3","065B2389",null,"065B2402",null,"065B2412",null,null,null,null,null,null,"РА-А","42-1-20-6,3-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,25,"8","065B2390",null,"065B2403",null,"065B2413",null,null,null,null,null,null,"РА-А","42-1-25-8-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,32,"16","065B2391",null,"065B2404",null,"065B2414",null,null,null,null,null,null,"РА-А","42-1-32-16-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,40,"20","065B2392",null,"065B2405",null,"065B2415",null,null,null,null,null,null,"РА-А","42-1-40-20-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,50,"32","065B2393",null,"065B2406",null,"065B2416",null,null,null,null,null,null,"РА-А","42-1-50-32-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,65,50,"065B2394",null,"065B2407",null,"065B2417",null,null,null,null,null,null,"РА-А","42-1-65-50-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,80,80,"065B2395",null,"065B2408",null,"065B2418",null,null,null,null,null,null,"РА-А","42-1-80-80-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,100,125,"065B2396",null,"065B2409",null,"065B2419",null,null,null,null,null,null,"РА-А","42-1-100-125-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,125,160,"065B2397",null,"065B2410",null,"065B2420",null,null,null,null,null,null,"РА-А","42-1-125-160-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,150,280,"065B2398",null,null,null,"065B2421",null,null,null,null,null,null,"РА-А","42-1-150-280-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,200,320,"065B2399",null,null,null,"065B2422",null,null,null,null,null,null,"РА-А","42-1-20-320-Х-СЧ-1,6-1-150-У"]
[null,"Danfoss",null,"AFP/VFG2",null,250,400,"065B2400"]

{"sheet":"RV 113R","index":31,"n_rows":66,"n_cols":28,"rows_kept":66,"cut":false,"hidden":false,"merged":[[10,20,10,23],[10,5,11,7],[10,8,11,10],[10,11,11,12],[11,20,11,23],[10,1,11,3],[10,4,11,4],[13,2,13,3],[1,7,1,12],[2,7,2,12],[3,7,3,12],[27,15,28,16],[15,2,17,2],[18,2,20,2],[12,1,12,3],[12,20,12,23],[13,16,14,23],[63,0,63,13],[64,0,64,13],[65,0,65,13],[31,16,33,16],[30,15,33,15]]}
[]
[null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,"RV 103",null,null,null,null,null,null,null,null,null,null,null,null,"Клапан КПСР серии 100"]
[null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Для внутренних сетей и ИТП"]
[null,null,null,null,"Материал корпуса: Серый чугун",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,null,null,null,"Рабочая температура: max +150°С",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[null,"Управление (привод)",null,null,"Siemens","Belimo",null,null,"Ekorex",null,null,"LDM",null,null,null,null,null,null,null,null,"Управление (привод)",null,null,null,"ES06-4","ST 0","ST 0,1","ST 1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Обозначение в типонометре",null,null,null,"1.3600","1.1200","1.1200","1.1200"]
[null,"Осевое усилие",null,null,"700 N","800 N","1600 N","2000 N","2000 N","3200 N","4000 N","2000 N","2500 N",null,null,null,null,null,null,null,"Осевое усилие",null,null,null,2000,4500,4500,4500]
[null,null,"Kvs, м³/ч",null,"ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max",null,null,null,"Kvs, м³/ч",null,null,null,null,null,null,null,"ΔP max","ΔP max","ΔP max","ΔP max"]
[null,"DN","H",1,"MPa","MPa","MPa","MPa","MPa","MPa","MPa","MPa","MPa",null,null,"DN",null,null,null,null,null,null,null,null,"MPa","MPa","MPa","MPa"]
[null,50,20,40,1.6,1.6,1.6,"---",1.6,1.6,1.6,1.6,1.6,null,null,50,0.16,0.25,0.4,0.63,1,1.6,3.2,4,0.7,0.8,1.5,"---"]
[null,65,null,63,1.6,1.6,1.6,"---",1.6,1.6,1.6,1.6,1.6,null,null,65,1.6,2.5,4,6.3,null,null,null,null,0.1,1.5,1.6,"---"]
[null,80,null,100,1.6,1.6,1.6,"---",1.6,1.6,1.6,1.6,1.6,null,null,80,1.6,2.5,4,6.3,8,10,null,null,0.8,1,1.6,"---"]
[null,100,40,160,"---","---","---",1.6,1.6,1.6,1.6,1.6,1.6,null,null,100,6.3,10,16,null,null,null,null,null,"---",0.8,1.4,1.6]
[null,125,null,250,"---","---","---",1.6,1.6,1.6,1.6,1.6,1.6,null,null,125,10,16,20,25,null,null,null,null,"---","---",1,1.2]
[null,150,null,360,"---","---","---",1.6,1.6,1.6,1.6,1.6,1.6,null,null,150,10,16,25,32,40,null,null,null,"---","---","---",1]
[]
[null,"Пример записи",null,null,null,null,null,null,null,null,null,null,null,null,null,"Пример записи"]
[null,"RV 103 ENA 4312 16/150-25",null,null,null,null,null,null,null,null,null,null,null,null,null,"КПСР 1-1-25-10-1.3500-СЧ-1,6-1-150-У"]
[]
[]
[null,null,null,null,"XX","XXX","XXX",null,"XX",null,"XX","/",null,null,null,"Тип клапана",null,"Регулирующий клапан",null,null,null,null,null,null,"●","КПСР"]
["Тип клапана","Регулирующий клапан",null,null,"RV",null,null,null,null,null,null,null,null,null,null,"Обозначение типа",null,"Регулирующий",null,null,null,null,null,null,"●",1]
[null,"Корпус из серого чугуна EN-JL 1040",null,null,null,113,null,null,null,null,null,null,null,null,null,null,null,"Запорно-регулирующий",null,null,null,null,null,null,"●",2]
[null,null,null,null,null,null,"R",null,null,null,null,null,null,null,null,"Корпус",null,"Фланцевый",null,null,null,null,null,null,"●",1]
[null,null,null,null,null,null,null,43,null,null,null,null,null,null,null,"Привод","AUMA","ES06-4",null,null,null,null,null,null,"●","1.3600"]
["Расходная","Линейная",null,null,null,null,null,null,3,null,null,null,null,null,null,null,"REGADA","ST 0",null,null,null,null,null,null,"●","1.1200"]
["характеристика",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ST 0,1",null,null,null,null,null,null,"●","1.1300"]
["Kvs","№ столбца значений Kvs клапана согласно табл.",null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,"ST 1",null,null,null,null,null,null,"●","1.1400"]
["Давление номин.","PN 16/150 °C ",null,null,null,null,null,null,null,null,"16/150",null,null,null,null,"Исполнение",null,"Двухходовой"]
["Диаметр номин.","DN 15 ÷ DN 50",null,null,null,null,null,null,null,null,null,"XX",null,null,null,"Материал корпуса",null,"Корпус из серого чугуна EN-JL 1040",null,null,null,null,null,null,"●","СЧ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Расходная",null,"Линейная",null,null,null,null,null,null,"●",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"характеристика",null,"Равнопроцентная",null,null,null,null,null,null,"●",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kvs",null,"Фактическое значение из таблицы",null,null,null,null,null,null,"●",10]
["Привод специфицируется отдельно",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Давление номин.",null,"1,6 МПа",null,null,null,null,null,null,"●",1.6]
["Производитель","Тип привода",null,"Макс. ход","Питание","Управление",null,null,null,null,null,null,null,null,null,"Максим. раб. темп.",null,"150 °C ",null,null,null,null,null,null,"●",150]
["LDM","ANT40.11",null,"40 mm","24/230 V","3-pos.,prop.",null,null,null,null,null,null,null,null,null,"Диаметр номин.",null,"DN 15 ÷ DN 50",null,null,null,null,null,null,"●",25]
["LDM","ANT40.11S",null,"40 mm","24/230 V","3-pos.,prop."]
["LDM","AN40.11R",null,"40 mm","24/230 V","3-pos.,prop."]
["Ekorex+","PTN 2.20",null,"25 mm","24/230 V","3-pos.,prop."]
["Ekorex+","PTN 2.32",null,"25 mm","24/230 V","3-pos.,prop."]
["Ekorex+","PTN 2.40",null,"25 mm","24/230 V","3-pos.,prop."]
["Siemens","SKD 32.00 a SQX 32.03",null,"20 mm","230 V","3-position"]
["Siemens","SKD 82.00 a SQX 82.03",null,"20 mm","24 V","3-position"]
["Siemens","SKD 62",null,"20 mm","24 V","0÷10 V"]
["Belimo","NV24-3",null,"20 mm","24 V","3-position"]
["Belimo","NV230-3",null,"20 mm","230 V","3-position"]
["Belimo","NV24-MFT",null,"20 mm","24 V","0÷10V, 3-pos."]
["Belimo","NV24-MFT-E",null,"20 mm","24 V","0÷10V, 3-pos."]
["Belimo","NVG24-MFT",null,"20 mm","24 V","0÷10V, 3-pos."]
["Belimo","NVY24-MFT ",null,"20 mm","24 V","3-position"]
["Belimo","AV24-3",null,"40 mm","230 V","3-position"]
["Belimo","AV230-3",null,"40 mm","24 V","0÷10 V"]
["Belimo","AV24-MFT",null,"40 mm","24 V","0÷10 V"]
["Belimo","AVY24-MFT",null,"40 mm","24 V","0÷10 V"]
[]
[]
[]
["По вопросам продаж и поддержки обращайтесь:"]
[]
["Сайт: http://kpsr.nt-rt.ru  ||  Эл. почта: krp@nt-rt.ru"]

{"sheet":"RD 103 (D,V)","index":32,"n_rows":53,"n_cols":36,"rows_kept":53,"cut":false,"hidden":false,"merged":[[1,7,1,11],[2,7,2,11],[3,7,3,11],[15,2,15,7],[10,2,10,4],[10,5,10,7],[11,2,11,4],[12,2,12,7],[13,2,13,7],[10,16,10,18],[10,19,10,21],[11,16,11,18],[12,16,12,21],[13,16,13,21],[29,16,29,21],[30,16,30,21],[14,2,14,7],[39,0,40,0],[41,0,44,0],[37,13,38,14],[39,13,40,14],[41,13,44,14],[18,2,18,7],[15,16,15,21],[16,16,16,21],[17,16,17,21],[16,2,16,7],[17,2,17,7],[14,16,14,21],[50,0,50,13],[51,0,51,13],[52,0,52,13],[9,27,9,30],[9,31,9,35],[9,26,10,26],[27,0,30,1],[37,0,38,0],[27,13,30,15],[27,2,27,7],[28,2,28,7],[29,2,29,7],[30,2,30,7],[18,16,18,21],[27,16,27,21],[28,16,28,21]]}
[]
[null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,"RD 103",null,null,null,null,null,null,null,null,null,null,null,null,"Регулятор давления по типу РА"]
[null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)",null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,null,null,null,"Материал корпуса: Серый чугун",null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,null,null,null,"Рабочая температура: max +150°С",null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"МПа","LDM",null,null,null,"КПСР-Групп"]
["Конструкционный ряд",null,"V",null,null,"D",null,null,null,null,null,null,null,"Конструкционный ряд",null,null,"-А",null,null,"-М",null,null,null,null,null,null,null,"Дапазоны настройки",null,null,null,0,1,2,3,4]
["Исполнение",null,"регулятор после себя",null,null,"регулятор перепада давления",null,null,null,null,null,null,null,"Исполнение",null,null,"регулятор после себя",null,null,"регулятор перепада давления",null,null,null,null,null,null,0.01]
["Диапазон диаметров",null,"15 ÷ 50",null,null,null,null,null,null,null,null,null,null,"Диапазон диаметров",null,null,"15 ÷ 50",null,null,null,null,null,null,null,null,null,2.5000000000000001E-2]
["Условное давление",null,"PN 16",null,null,null,null,null,null,null,null,null,null,"Условное давление",null,null,"PN 16",null,null,null,null,null,null,null,null,null,0.04]
["Материал корпуса",null,"серый чугун EN-JL1040",null,null,null,null,null,null,null,null,null,null,"Материал корпуса",null,null,"серый чугун EN-JL1040",null,null,null,null,null,null,null,null,null,0.05]
["Материал мембраны",null,"EPDM",null,null,null,null,null,null,null,null,null,null,"Материал мембраны",null,null,"EPDM",null,null,null,null,null,null,null,null,null,0.08]
["Рабочая температура",null,"0 ÷ 150°C",null,null,null,null,null,null,null,null,null,null,"Рабочая температура",null,null,"0 ÷ 150°C",null,null,null,null,null,null,null,null,null,0.1]
["Тип конуса",null,"Фасонный. Разгруженный по давлению",null,null,null,null,null,null,null,null,null,null,"Тип конуса",null,null,"Фасонный. Разгруженный по давлению",null,null,null,null,null,null,null,null,null,0.16]
["Расходная характеристика",null,"Линейная",null,null,null,null,null,null,null,null,null,null,"Расходная характеристика",null,null,"Линейная",null,null,null,null,null,null,null,null,null,0.2]
[null,null,"ДУ","kvs",null,null,null,null,null,null,null,null,null,null,null,null,"ДУ","kvs",null,null,null,null,null,null,null,null,0.3]
[null,null,15,2,null,null,null,null,null,null,null,null,null,null,null,null,15,"0,16  0,25  0,4   0,63   1   1,6   2,5   3,2  4",null,null,null,null,null,null,null,null,0.4]
[null,null,20,3.2,null,null,null,null,null,null,null,null,null,null,null,null,20,"1,6  2,5  4  6,3",null,null,null,null,null,null,null,null,0.5]
[null,null,25,5,null,null,null,null,null,null,null,null,null,null,null,null,25,"1,6  2,5  4  6,3  8  10",null,null,null,null,null,null,null,null,0.6]
["Значения kvs",null,32,8,null,null,null,null,null,null,null,null,null,"Значения kvs",null,null,32,"6,3  10  16",null,null,null,null,null,null,null,null,0.65]
[null,null,40,12.5,null,null,null,null,null,null,null,null,null,null,null,null,40,"10  16  20  25",null,null,null,null,null,null,null,null,0.7]
[null,null,50,20,null,null,null,null,null,null,null,null,null,null,null,null,50,"10  16  25  32  40",null,null,null,null,null,null,null,null,0.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.9]
["Диапазон настройки, МПа",null,"0,025 - 0,1",null,null,null,null,null,null,null,null,null,null,"Диапазон настройки, МПа",null,null,"0,01 - 0,1",null,null,null,null,null,null,null,null,null,1]
[null,null,"0,08 - 0,3",null,null,null,null,null,null,null,null,null,null,null,null,null,"0,04 - 0,16",null,null,null,null,null,null,null,null,null,1.1000000000000001]
[null,null,"0,2 - 0,65",null,null,null,null,null,null,null,null,null,null,null,null,null,"0,1 - 0,4",null,null,null,null,null,null,null,null,null,1.2]
[null,null,"0,3 - 1",null,null,null,null,null,null,null,null,null,null,null,null,null,"0,3 - 0,7"]
[]
[null,"Пример записи",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Пример записи"]
[null,"RD 103 V43 16/140-20",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"РА-А 25-10-2-СЧ-1,6-1-150-У1"]
[]
["Тип клапана","Регулятор давления",null,null,"RD",null,null,null,null,null,null,null,null,"Тип клапана",null,"Регулятор давления",null,null,null,null,null,null,"●","РА"]
["Обозначение типа","Вентиль из серого чугунв",null,null,null,103,null,null,null,null,null,null,null,"Присоединение",null,"Фланцевый",null,null,null,null,null,null,"●",1]
["Функция","После себя",null,null,null,null,"V",null,null,null,null,null,null,"Функция",null,"После себя",null,null,null,null,null,null,"●","-А"]
[null,"Перепада давления",null,null,null,null,"D",null,null,null,null,null,null,null,null,"Перепада давления",null,null,null,null,null,null,"●","-М"]
["Исполнение","С манометром",null,null,null,null,null,3]
[null,"без манометра",null,null,null,null,null,4]
["Диапазон настройки","0,025 до 0,1",null,null,null,null,null,null,1,null,null,null,null,"Диапазон настройки",null,"0,01 - 0,1",null,null,null,null,null,null,"●",0]
[null,"0,08 до 0,3",null,null,null,null,null,null,2,null,null,null,null,null,null,"0,04-0,16",null,null,null,null,null,null,"●",1]
[null,"0,2 до 0,65",null,null,null,null,null,null,3,null,null,null,null,null,null,"0,1-0,4",null,null,null,null,null,null,"●",2]
[null,"0,3 до 1",null,null,null,null,null,null,4,null,null,null,null,null,null,"0,3-0,7",null,null,null,null,null,null,"●",3]
["Давление номин.","PN 16/150 °C ",null,null,null,null,null,null,null,16,null,null,null,"Давление номин.",null,"1,6 МПа",null,null,null,null,null,null,"●",1.6]
["Максим. раб. темп.","150 °C ",null,null,null,null,null,null,null,null,140,null,null,"Максим. раб. темп.",null,"150 °C ",null,null,null,null,null,null,"●",150]
["Диаметр номин.","DN 15 ÷ DN 50",null,null,null,null,null,null,null,null,null,"ХХ",null,"Диаметр номин.",null,"DN 15 ÷ DN 50",null,null,null,null,null,null,"●",25]
[]
[]
["По вопросам продаж и поддержки обращайтесь:"]
[]
["Сайт: http://kpsr.nt-rt.ru  ||  Эл. почта: krp@nt-rt.ru"]

{"sheet":"RV 210-220","index":33,"n_rows":112,"n_cols":48,"rows_kept":112,"cut":false,"hidden":false,"merged":[[1,11,1,16],[2,11,2,16],[3,11,3,16],[13,34,13,37],[13,38,23,38],[13,42,23,42],[14,34,14,37],[15,34,15,37],[23,2,23,10],[16,30,17,37],[16,8,21,10],[10,8,15,10],[31,30,32,31],[34,30,38,30],[34,31,36,31],[37,31,38,31],[25,1,26,1],[27,1,29,1],[30,1,31,1],[32,1,33,1],[41,1,43,1],[44,1,46,1],[47,1,49,1],[50,1,52,1],[75,0,76,0],[58,1,58,5],[59,1,59,5],[87,1,87,2],[60,1,60,2],[56,0,57,0],[58,0,59,0],[62,0,63,0],[65,0,71,0],[72,0,74,0],[77,0,79,0],[80,0,85,0],[86,0,91,0],[93,0,95,0],[96,0,101,0],[81,21,81,23],[82,21,82,23],[71,21,71,23],[72,21,72,23],[73,21,73,23],[74,21,74,23],[80,21,80,23],[75,21,75,23],[76,21,76,23],[77,21,77,23],[78,21,78,23],[79,21,79,23],[56,21,56,23],[57,21,57,23],[58,21,58,23],[59,21,59,23],[60,21,60,23],[61,21,61,23],[62,21,62,23],[63,21,63,23],[64,21,64,23],[65,21,65,23],[66,21,66,23],[67,21,67,23],[68,21,68,23],[69,21,69,23],[70,21,70,23],[88,21,88,23],[94,21,94,23],[95,21,95,23],[96,21,96,23],[97,21,97,23],[89,21,89,23],[90,21,90,23],[91,21,91,23],[92,21,92,23],[93,21,93,23],[83,21,83,23],[84,21,84,23],[85,21,85,23],[86,21,86,23],[87,21,87,23],[109,0,109,13],[110,0,110,13],[111,0,111,13],[98,21,98,23],[99,21,99,23],[100,21,100,23],[103,0,106,0]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"RV/UV 210",null,null,null,null,null,null,null,"RV/UV 220",null,null,null,null,null,null,null,null,null,null,"Клапан КПСР серии 100"]
[null,null,null,null,null,null,null,null,"Рабочее давление: ",null,null,"DN 15-150 : PN 16, 40; DN 200-400 : PN 16",null,null,null,null,"Рабочее давление: ",null,null,"PN 16, 25, 40",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Для внутренних сетей и ИТП"]
[null,null,null,null,null,null,null,null,"Материал корпуса: ",null,null,"Высокопрочный чугун EN-JS 1025",null,null,null,null,"Материал корпуса: ",null,null,"Литая сталь 1.0619",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,null,null,null,null,null,null,null,"Рабочая температура: ",null,null," -20 до 300°С",null,null,null,null,"Рабочая температура: ",null,null," -20 до 500°С",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[null,null,null,null,null,null,null,null,"Управление (привод)",null,null,"PTN 2.20","ST 0","PTN 2.32","MIDI 660","AUMA","Zepadyn","AUMA","AUMA","Zapadyn","Modast Cont","Modast MTR","AUMA","Modast MTR","AUMA","Modast MTR","AUMA"]
[null,null,null,null,null,null,null,null,null,null,null,"MIDI 660",null,"MIDI 660","ST 0","Schiebel","ST 1 Ex","Schiebel","Schiebel","Modast MTR","Modast MTN","ST 2","Schiebel","ST 2","Schiebel","Modast MTN","Schiebel"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ST 0,1","Rotork","ST 0,1","Rotork","Rotork","PTN 6","AUMA","Zapadyn 671","Rotork","Zapadyn 671","EMG","Modast Cont"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PTN 2.40","EMG","PTN 6","EMG","EMG",null,"Schiebel","PTN 7","EMG","PTN 7","Zapadyn 671","ST 2",null,null,null,null,null,null,null,null,"Управление (привод)",null,null,null,"СЕРИЯ 110","ES05-11","ES05-12","ES06-4","СЕРИЯ 100","ES05-11","ES05-12","ES06-4","ST mini","ST 0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Modast MTN",null,"PTN 7",null,null,null,null,null,null,null,null,null,"Обозначение в типонометре",null,null,null,null,"1.3500","1.3501","1.3600",null,"1.3500","1.3501","1.3600","1.1100","1.1200"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Modast Cont",null,null,null,null,null,null,null,null,null,null,null,"Осевое усилие",null,null,null,null,600,1000,2000,null,600,1000,2000,1100,4500]
[null,null,null,null,null,null,null,null,"Обозначение в типонометре",null,null,"ERB","EPK","ERC","ENB","EA…","ENC","EA…","EA…","ENC","EYA","EPD","EA…","EPD","EA…","EPD","EA…",null,null,null,"Kvs, м³/ч",null,null,null,null,null,null,null,null,"ΔP max","ΔP max","ΔP max",null,"ΔP max","ΔP max","ΔP max","ΔP max","ΔP max"]
[null,null,null,null,null,null,null,null,null,null,null,"ENB",null,"ENB","EPK","EZ…","EPJ","EZ…","EZ…","EPD","EYA","EPM","EZ…","EPM","EZ…","EYA","EZ…",null,null,"DN",null,null,null,null,null,null,null,null,null,"MPa","MPa","MPa",null,"MPa","MPa","MPa","MPa","MPa"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EPL","EQ…","EPL","EQ…","EQ…","ERD","EA…","ENE","EQ…","ENE","ED…","EYB",null,null,null,15,0.16,0.25,0.4,0.63,1,1.6,3.2,4,null,1.6,null,1.6,null,0.85,1.4,1.6,1.6,1.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC","ED…","ERD","ED…","ED…",null,"EZ…","ERG","ED…","ERG","ENE","EPM",null,null,null,20,1.6,2.5,4,6.3,null,null,null,null,null,1.6,null,1.6,null,0.63,1.05,1.6,1.2,1.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EYA",null,"ERG",null,null,null,null,25,1.6,2.5,4,6.3,8,10,null,null,null,1.6,null,1.6,null,0.4,0.65,1.6,0.74,1.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EYB",null,null,null,null,null,null,32,6.3,10,16,null,null,null,null,null,null,1.6,null,1.6,null,0.35,6.2,1.6,0.68,1.6]
[null,null,null,null,null,null,null,null,"Осевое усилие",null,null,"2 kN","2,5 kN","3,2 kN","4,0 kN","5 kN","6,3 kN","7,5 kN","10 kN","10 kN","15 kN","16 kN","15 kN","16 kN","20 kN","25 kN","32 kN",null,null,40,10,16,20,25,null,null,null,null,null,1.4,1.6,1.6,null,0.15,0.4,1.6,0.5,1.6]
[null,null,"Kvs, м³/ч",null,null,null,null,null,null,null,null,"ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max",null,null,50,10,16,25,32,40,null,null,null,null,1,1.6,1.6,null,null,0.25,1.6,0.8,1.6]
[null,"DN",1,2,3,4,5,6,7,8,9,"мет    PTFE","мет    PTFE","мет    PTFE","мет    PTFE","мет    PTFE","мет    PTFE","мет    PTFE","мет    PTFE","мет    PTFE","мет    PTFE","мет    PTFE","графит PTFE","графит PTFE","графит PTFE","графит PTFE","графит PTFE"]
[null,15,"---",2.5,1.6,1,0.6,0.4,0.25,0.16,0.1,"4         ---","4         ---","4         ---","4         ---","4         ---","4         ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","---","---","---","---","---",null,null,null,null,null,null,null,null,"Пример записи"]
[null,null,4,"---","---","---","---","---","---","---","---","4         ---","4         ---","4         ---","4         ---","4         ---","4         ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","---","---","---","---","---",null,null,null,null,null,null,null,null,"КПСР 1-1-25-10-1.3500-СЧ-1,6-1-150-У"]
[null,20,"---","---",2.5,1.6,1,0.6,"---","---","---","4         ---","4         ---","4         ---","4         ---","4         ---","4         ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","---","---","---","---","---"]
[null,null,"---",4,"---","---","---","---","---","---","---","4         ---","4         ---","4         ---","4         ---","4         ---","4         ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","---","---","---","---","---"]
[null,null,6.3,"---","---","---","---","---","---","---","---","3,77     ---","4         ---","4         ---","4         ---","4         ---","4         ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","---","---","---","---","---"]
[null,25,"---","---","---",2.5,1.6,"---","---","---","---","4         ---","4         ---","4         ---","4         ---","4         ---","4         ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","---","---","---","---","---",null,null,null,"Тип клапана",null,"Регулирующий клапан",null,null,null,null,null,null,"●","КПСР"]
[null,null,10,6.3,4,null,"---","---","---","---","---","2,24   2,65","3,16   3,57","4          4","4          4","4          4","4          4"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","---","---","---","---","---",null,null,null,"Обозначение типа",null,"Регулирующий",null,null,null,null,null,null,"●",1]
[null,32,"---","---","---",4,"---","---","---","---","---","4         ---","4         ---","4         ---","4         ---","4         ---","4         ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","---","---","---","---","---",null,null,null,null,null,"Запорно-регулирующий",null,null,null,null,null,null,"●",2]
[null,null,16,10,6.3,"---","---","---","---","---","---","1,28    1,6","1,83   2,15","2,61   2,92","3,49   3,81","4          4","4          4"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","---","---","---","---","---",null,null,null,"Корпус",null,"Фланцевый",null,null,null,null,null,null,"●",1]
[null,40,25,16,10,"---","---","---","---","---","---","0,77   1,02","1,12   1,38","1,62   1,87","2,19   2,44","2,9     3,15","3,6      3,9"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","---","---","---","---","---",null,null,null,"Привод","AUMA","ES05-11",null,null,null,null,null,null,"●","1.3500"]
[null,50,40,25,16,"---","---","---","---","---","---"," ---        ---","0,63   0,82","0,93   1,12","1,27   1,46","1,69   1,88","2,1      2,3","2,76   2,95","3,82     4","3,82      4"," ---        ---"," ---        ---","---","---","---","---","---",null,null,null,null,null,"ES05-12",null,null,null,null,null,null,"●","1.3501"]
[null,65,63,40,25,"---","---","---","---","---","---"," ---        ---","0,35    0,5","0,53   0,68","0,74   0,89","1      1,15","1,2     1,4","1,65     1,8","2,3     2,45","2,3     2,45"," ---        ---"," ---        ---","---","---","---","---","---",null,null,null,null,null,"ES06-4",null,null,null,null,null,null,"●","1.3600"]
[null,80,100,63,40,"---","---","---","---","---","---"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","0,73   0,86","1,01   1,13","1,46   1,58","1,46   1,58","2,36   2,48","2,54   2,66","---","---","---","---","---",null,null,null,null,"REGADA","ST mini",null,null,null,null,null,null,"●","1.1100"]
[null,100,160,100,63,"---","---","---","---","---","---"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","0,45   0,56","0,63   0,73","0,92   1,02","0,92   1,02","1,5     1,61","1,62    1,72","---","---","---","---","---",null,null,null,null,null,"ST 0",null,null,null,null,null,null,"●","1.1200"]
[null,125,250,160,100,"---","---","---","---","---","---"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","0,27    0,36","0,39   0,47","0,58   0,66","0,58    0,66","0,96    1,04","1,03   1,12","---","---","---","---","---",null,null,null,"Исполнение",null,"Двухходовой"]
[null,150,360,250,160,"---","---","---","---","---","---"," ---        ---"," ---        ---"," ---        ---"," ---        ---"," ---        ---","0,18   0,25","0,26   0,33","0,39    0,46","0,39    0,46","0,66   0,73","0,71    0,78","---","---","---","---","---",null,null,null,"Материал корпуса",null,"Корпус из серого чугуна EN-JL 1040",null,null,null,null,null,null,"●","СЧ"]
[null,200,"---","---",250,160,100,"---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","1,12   1,46","1,24   1,58","1,71   2,05","2,31   2,64","3,14   3,47",null,null,null,"Расходная",null,"Линейная",null,null,null,null,null,null,"●",1]
[null,null,"---",400,"---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","0,48   0,63","0,53   0,68","0,75    0,9","1,01   1,17","1,39   1,54",null,null,null,"характеристика",null,"Равнопроцентная",null,null,null,null,null,null,"●",2]
[null,null,570,"---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","0,26   0,34","0,29   0,37","0,41    0,5","0,56   0,65","0,77   0,86",null,null,null,"Kvs",null,"Фактическое значение из таблицы",null,null,null,null,null,null,"●",10]
[null,250,"---","---",400,250,160,"---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","0,41   0,59","0,47   0,64","0,68   0,86","0,95   1,13","1,33    1,5",null,null,null,"Давление номин.",null,"1,6 МПа",null,null,null,null,null,null,"●",1.6]
[null,null,"---",630,"---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","0,22   0,32","0,25   0,35","0,37   0,47","0,52   0,62","0,74    0,84",null,null,null,"Максим. раб. темп.",null,"150 °C ",null,null,null,null,null,null,"●",150]
[null,null,800,"---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","0,16   0,23","0,18   0,26","0,27   0,35","0,39   0,46","0,55   0,63",null,null,null,"Диаметр номин.",null,"DN 15 ÷ DN 50",null,null,null,null,null,null,"●",25]
[null,300,"---","---",630,400,250,"---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","0,22   0,32","0,25   0,35","0,37   0,47","0,52   0,62","0,74   0,84"]
[null,null,"---",800,"---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","0,16   0,23","0,18   0,26","0,27   0,35","0,39   0,46","0,55   0,63"]
[null,null,1000,"---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","0,13   0,19","0,15   0,21","0,23   0,29","0,33   0,39","0,46   0,53"]
[null,400,"---","---",630,400,250,"---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","0,22   0,32","0,25   0,35","0,37   0,47","0,52   0,62","0,74   0,84"]
[null,null,"---",1000,"---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","0,13   0,19","0,15   0,21","0,23   0,29","0,33   0,39","0,46   0,53"]
[null,null,1600,"---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","---","0,07   0,10","0,08   0,11","0,12   0,16","0,18   0,22","0,26   0,30"]
[]
[]
[]
["Тип клапана","Регулирующий клапан",null,null,null,"RV",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," PTN 2.20",null,null,"E R B"]
[null,"Запорный клапан",null,null,null,"UV",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," PTN 2.32; PTN 2.40",null,null,"E R C"]
["Серия","Сфероидальный чугун EN-JS 1025)",null,null,null,null,21,null,null,null,null,null,null,null,null,null,null,null,null,null,null," PTN 6",null,null,"E R D"]
[null,"Углеродистая сталь 1.0619, 1.7357",null,null,null,null,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null," PTN 7",null,null,"E R G"]
[null,"Прямой клапан",null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null," 660 MIDI",null,null,"E N B"]
[null,"Разгруженный, прямопроходный",null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null," Zepadyn 670",null,null,"E N C"]
["Привод","Электрический привод",null,null,null,null,null,null,"E",null,null,null,null,null,null,null,null,null,null,null,null," Zepadyn 671",null,null,"E N E"]
[null,"Пневматический привод",null,null,null,null,null,null,"P",null,null,null,null,null,null,null,null,null,null,null,null," Modact MTR",null,null,"E P D"]
[null,"Siemens",null,null,null,null,null,null,null,"L","X",null,null,null,null,null,null,null,null,null,null," ST 0",null,null,"E P K"]
["Производитель","Belimo",null,null,null,null,null,null,null,"B","X",null,null,null,null,null,null,null,null,null,null," ST 0.1",null,null,"E P L"]
[null,"ZPA Nová Paka",null,null,null,null,null,null,null,"N","X",null,null,null,null,null,null,null,null,null,null," Isomact ST 1 Ex",null,null,"E P J"]
[null,"Regada Prešov",null,null,null,null,null,null,null,"P","X",null,null,null,null,null,null,null,null,null,null," Isomact ST 2",null,null,"E P M"]
[null,"SPA Praha",null,null,null,null,null,null,null,"J","X",null,null,null,null,null,null,null,null,null,null," Modact MTN Control, MTP Control",null,null,"E Y A"]
[null,"Ekorex+",null,null,null,null,null,null,null,"R","X",null,null,null,null,null,null,null,null,null,null," Modact MTN, MTP",null,null,"E Y B"]
[null,"Flowserve",null,null,null,null,null,null,null,"F","X",null,null,null,null,null,null,null,null,null,null," Modact MTNED, MTPED",null,null,"E Y A"]
[null,"LDM",null,null,null,null,null,null,null,"V ","X",null,null,null,null,null,null,null,null,null,null," Auma SA 07.1",null,null,"E A A"]
["Присоединение","Фланцевое с  выступом В1",null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null," Auma SA Ex 07.1",null,null,"E A B"]
[null,"Фланцевое с выточкой F",null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null," Auma SAR 07.1",null,null,"E A C"]
[null,"Фланцевое с проточкой D",null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,null," Auma SAR Ex 07.1",null,null,"E A D"]
["Материал корпуса","Углеродистая сталь 1.0619",null,null,null,"(-20 ÷ 400 °C)",null,null,null,null,null,null,1,null,null,null,null,null,null,null,null," Auma SA 07.5",null,null,"E A E"]
[null,"Сфероидальный чугун \nEN-JS 1025",null,null,null,"(-20 ÷ 300 °C)",null,null,null,null,null,null,4,null,null,null,null,null,null,null,null," SA Ex 07.5",null,null,"E A F"]
["Уплотнение в седле","Металл-металл",null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null," Auma SAR 07.5",null,null,"E A G"]
[null,"Мягкое уплотнение (metal - PTFE) 1)",null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null," Auma SAR Ex 07.5",null,null,"E A H"]
[null,"Наварка в седле",null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null," Auma SA 10.1",null,null,"E A I"]
["Уплотнитель","O - ring EPDM 3)",null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null," Auma SAR 10.1",null,null,"E A J"]
[null,"DRSpack® (PTFE)",null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null," Auma SAR Ex 10.1",null,null,"E A K"]
[null,"Графит 3)",null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null," Auma SA Ex 10.1",null,null,"E A L"]
[null,"Сильфонs 6)",null,null,null,null,null,null,null,null,null,null,null,null,7,null,null,null,null,null,null," Rotork IQM 7",null,null,"E Q A"]
[null,"Сильфон с мягким  PTFE уплотнением 6)",null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,null,null,null," Rotork Ex IQM 7",null,null,"E Q B"]
[null,"Сильфон с графитовым уплотнением 3)6)",null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,null,null,null," Schiebel AB3",null,null,"E Z A"]
["Расходная характеристика","Линейная",null,null,null,null,null,null,null,null,null,null,null,null,null,"L",null,null,null,null,null," Schiebel exAB3",null,null,"E Z B"]
[null,"Равнопроцентная (прямая ветвь для 3-хход.)",null,null,null,null,null,null,null,null,null,null,null,null,null,"R",null,null,null,null,null," Schiebel rAB3",null,null,"E Z C"]
[null,"LDMspline® 5)",null,null,null,null,null,null,null,null,null,null,null,null,null,"S",null,null,null,null,null," Schiebel exrAB3",null,null,"E Z D"]
[null,"Линейная - перфорир. конус 5)",null,null,null,null,null,null,null,null,null,null,null,null,null,"D",null,null,null,null,null," Schiebel AB5",null,null,"E Z E"]
[null,"Равнопроцентная  - перфорирован. конус 5)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Q",null,null,null,null,null," Schiebel exAB5",null,null,"E Z F"]
[null,"Параболическая  - перфорирован. конус 5)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Z",null,null,null,null,null," Schiebel rAB5",null,null,"E Z G"]
["Kvs","No. В колонке для Kvs клапана в таблице",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X",null,null,null,null," Schiebel exrAB5",null,null,"E Z H"]
["Номинальное давление","PN 16",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null," Schiebel rAB8",null,null,"E Z K"]
[null,"PN 25 (DN 200 ÷ DN 400)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,null,null,null," Schiebel exrAB8",null,null,"E Z L"]
[null,"PN 40",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,null,null,null," EMG Drehmo D 30",null,null,"E D A"]
["Рабочая температура","O - ring EPDM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,140,null,null," EMG Drehmo D R 30",null,null,"E D B"]
[null,"DRSpack® (PTFE), сильфон",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,220,null,null," EMG Drehmo DMI 30",null,null,"E D C"]
[null,"DRSpack® (PTFE),сильфон",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,260,null,null," EMG Drehmo DMI R 30",null,null,"E D D"]
[null,"Графит, сильфон",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,null,null," EMG Drehmo D R 30 Ex",null,null,"E D I"]
[null,"Графит, сильфон",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,null,null," EMG Drehmo DMI R 30 Ex",null,null,"E D K"]
[null,"Графит, сильфон",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500]
["Номинальный диаметр","DN 15 ÷ DN 400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"XXX"]
["Исполнение","Нормальное"]
[null,"Взырывозащищенное",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ex"]
[null,"Для кислорода",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ox"]
[null,"С гигиеническим сертификатом",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Px"]
[]
[]
["По вопросам продаж и поддержки обращайтесь:"]
[]
["Сайт: http://kpsr.nt-rt.ru  ||  Эл. почта: krp@nt-rt.ru"]

{"sheet":"RV 212-222","index":34,"n_rows":47,"n_cols":42,"rows_kept":47,"cut":false,"hidden":false,"merged":[[1,11,1,14],[2,11,2,14],[3,11,3,14],[10,8,15,10],[13,28,13,31],[13,36,23,36],[14,28,14,31],[15,28,15,31],[13,32,23,32],[16,8,21,10],[16,24,17,31],[23,2,23,10],[40,1,40,13],[41,1,41,13],[42,1,42,13],[31,24,32,25],[34,24,38,24],[34,25,36,25],[37,25,38,25]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"RV/UV 212",null,null,null,"RV/UV 222",null,null,null,null,null,null,null,null,"Клапан КПСР серии 100"]
[null,null,null,null,null,null,null,null,"Рабочее давление: ",null,null,"DN 25-150 : PN 16, 40; DN 200-400 : PN 16",null,null,null,"Рабочее давление: ",null,"PN 16, 25, 40",null,null,null,null,null,null,null,null,null,null,null,"Для внутренних сетей и ИТП"]
[null,null,null,null,null,null,null,null,"Материал корпуса: ",null,null,"Высокопрочный чугун EN-JS 1025",null,null,null,"Материал корпуса: ",null,"Литая сталь 1.0619",null,null,null,null,null,null,null,null,null,null,null,"Рабочее давление: 1,6 МПа (16 атм)"]
[null,null,null,null,null,null,null,null,"Рабочая температура: ",null,null," -20 до 260°С",null,null,null,"Рабочая температура: ",null," -20 до 260°С",null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса: Серый чугун (EN-JS 1040)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура: max +150°С"]
[null,null,null,null,null,null,null,null,"Управление (привод)",null,null,"PTN 2.20","ST 0","AUMA","Zepadyn","Modast Cont","Modast MTR","AUMA","Modast MTR","AUMA","Modast MTR"]
[null,null,null,null,null,null,null,null,null,null,null,"MIDI 660",null,"Schiebel","ST 1 Ex","Modast MTN","ST 2","Schiebel","ST 2","Schiebel","Modast MTN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Rotork","ST 0,1",null,"Zapadyn 671","Rotork","Zapadyn 671","EMG","Modast Cont"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"EMG","PTN 6",null,"PTN 7","Modast MTN","PTN 7","Zapadyn 671","ST 2",null,null,null,null,null,null,null,"Управление (привод)",null,null,null,"СЕРИЯ 110","ES05-11","ES05-12","ES06-4","СЕРИЯ 100","ES05-11","ES05-12","ES06-4","ST mini","ST 0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Modast Cont",null,"PTN 7",null,null,null,null,null,null,null,null,"Обозначение в типонометре",null,null,null,null,"1.3500","1.3501","1.3600",null,"1.3500","1.3501","1.3600","1.1100","1.1200"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Осевое усилие",null,null,null,null,600,1000,2000,null,600,1000,2000,1100,4500]
[null,null,null,null,null,null,null,null,"Обозначение в типонометре",null,null,"ERB","EPK","EA…","ENC","EYA","EPD","EA…","EPD","EA…","EPD",null,null,null,"Kvs, м³/ч",null,null,null,null,null,null,null,null,"ΔP max","ΔP max","ΔP max",null,"ΔP max","ΔP max","ΔP max","ΔP max","ΔP max"]
[null,null,null,null,null,null,null,null,null,null,null,"ENB",null,"EZ…","EPJ","EYA","EPM","EZ…","EPM","EZ…","EYA",null,null,"DN",null,null,null,null,null,null,null,null,null,"MPa","MPa","MPa",null,"MPa","MPa","MPa","MPa","MPa"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"EQ…","EPL",null,"ENE","ED…","ENE","ED…","EYB",null,null,15,0.16,0.25,0.4,0.63,1,1.6,3.2,4,null,1.6,null,1.6,null,0.85,1.4,1.6,1.6,1.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"ED…","ERD",null,"ERG","EYA","ERG","ENE","EPM",null,null,20,1.6,2.5,4,6.3,null,null,null,null,null,1.6,null,1.6,null,0.63,1.05,1.6,1.2,1.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EYB",null,"ERG",null,null,null,25,1.6,2.5,4,6.3,8,10,null,null,null,1.6,null,1.6,null,0.4,0.65,1.6,0.74,1.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,32,6.3,10,16,null,null,null,null,null,null,1.6,null,1.6,null,0.35,6.2,1.6,0.68,1.6]
[null,null,null,null,null,null,null,null,"Осевое усилие",null,null,"2 kN","2,5 kN","5 kN","6,3 kN","15 kN","16 kN","15 kN","16 kN","20 kN","25 kN",null,null,40,10,16,20,25,null,null,null,null,null,1.4,1.6,1.6,null,0.15,0.4,1.6,0.5,1.6]
[null,null,"Kvs, м³/ч",null,null,null,null,null,null,null,null,"ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max","ΔP max",null,null,50,10,16,25,32,40,null,null,null,null,1,1.6,1.6,null,null,0.25,1.6,0.8,1.6]
[null,"DN",1,2,3,4,5,6,7,8,9,null,null,"мет    PTFE","мет    PTFE","мет    PTFE","мет    PTFE","графит PTFE","графит PTFE","графит PTFE","графит PTFE"]
[null,25,10,6.3,4,2.5,1.6,"---","---","---","---",4,4,"---",4,"---","---","---","---","---","---",null,null,null,null,null,null,null,null,"Пример записи"]
[null,32,16,10,6.3,4,2.5,"---","---","---","---",4,4,"---",4,"---","---","---","---","---","---",null,null,null,null,null,null,null,null,"КПСР 1-1-25-10-1.3500-СЧ-1,6-1-150-У"]
[null,40,25,16,10,6.3,4,"---","---","---","---",4,4,"---",4,"---","---","---","---","---","---"]
[null,50,40,25,16,10,6.3,"---","---","---","---","---",4,4,4,"---","---","---","---","---","---"]
[null,65,63,40,25,16,10,"---","---","---","---","---",4,4,4,"---","---","---","---","---","---"]
[null,80,100,63,40,25,16,"---","---","---","---","---","---",4,4,4,4,"---","---","---","---",null,null,null,"Тип клапана",null,"Регулирующий клапан",null,null,null,null,null,null,"●","КПСР"]
[null,100,160,100,63,40,25,"---","---","---","---","---","---",4,4,4,4,"---","---","---","---",null,null,null,"Обозначение типа",null,"Регулирующий",null,null,null,null,null,null,"●",1]
[null,125,250,160,100,63,40,"---","---","---","---","---","---",4,4,4,4,"---","---","---","---",null,null,null,null,null,"Запорно-регулирующий",null,null,null,null,null,null,"●",2]
[null,150,360,250,160,100,63,"---","---","---","---","---","---",4,4,4,4,"---","---","---","---",null,null,null,"Корпус",null,"Фланцевый",null,null,null,null,null,null,"●",1]
[null,200,570,400,250,160,100,"---","---","---","---","---","---","---","---","---","---",4,4,"---","---",null,null,null,"Привод","AUMA","ES05-11",null,null,null,null,null,null,"●","1.3500"]
[null,250,800,630,400,250,160,"---","---","---","---","---","---","---","---","---","---","---","---",4,4,null,null,null,null,null,"ES05-12",null,null,null,null,null,null,"●","1.3501"]
[null,300,1000,800,630,400,250,"---","---","---","---","---","---","---","---","---","---","---","---",4,4,null,null,null,null,null,"ES06-4",null,null,null,null,null,null,"●","1.3600"]
[null,400,1600,1000,630,400,250,"---","---","---","---","---","---","---","---","---","---","---","---",4,4,null,null,null,null,"REGADA","ST mini",null,null,null,null,null,null,"●","1.1100"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ST 0",null,null,null,null,null,null,"●","1.1200"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Исполнение",null,"Двухходовой"]
[null,"По вопросам продаж и поддержки обращайтесь:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса",null,"Корпус из серого чугуна EN-JL 1040",null,null,null,null,null,null,"●","СЧ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Расходная",null,"Линейная",null,null,null,null,null,null,"●",1]
[null,"Сайт: http://kpsr.nt-rt.ru  ||  Эл. почта: krp@nt-rt.ru",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"характеристика",null,"Равнопроцентная",null,null,null,null,null,null,"●",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kvs",null,"Фактическое значение из таблицы",null,null,null,null,null,null,"●",10]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Давление номин.",null,"1,6 МПа",null,null,null,null,null,null,"●",1.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Максим. раб. темп.",null,"150 °C ",null,null,null,null,null,null,"●",150]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Диаметр номин.",null,"DN 15 ÷ DN 50",null,null,null,null,null,null,"●",25]

{"sheet":"Подбор RV","index":35,"n_rows":341,"n_cols":37,"rows_kept":341,"cut":false,"hidden":false,"merged":[[3,0,5,0],[1048333,21,1048334,21],[4,17,4,19],[4,20,4,23],[3,24,5,24],[3,6,5,6],[3,7,5,7],[3,8,5,8],[3,9,5,9],[3,12,5,12],[3,1,5,1],[3,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[3,3,3,5],[3,30,5,30],[3,13,5,13],[3,14,5,14],[3,15,5,15],[3,16,5,16],[3,17,3,23],[3,26,5,26],[3,27,5,27],[3,28,5,28],[3,29,5,29],[3,25,5,25]]}
[]
[]
[]
["Марка","Серия","Привод","Исполнение",null,null,{"$f":"Q4","v":"Kvs, м³/ч"},"Pn, Bar","T","DN","ΔP max. Мпа",null,"Тип изделия","Тип клапана","Хар-ка регул-ния","DN","Kvs, м³/ч","Электропривод",null,null,null,null,null,null,{"$f":"E5","v":"Материал корпуса"},"Pn, МПа","Присоеди-нение к тр-ду","Т","Клим исполн","ΔP max. Мпа серия 100","ΔP max. Мпа серия 110","Привод AUMA ES05-11","Привод AUMA ES05-12","Привод AUMA ES06-4","ΔP max. Мпа серия 100","Привод Regada ST mini","Привод Regada ST 0"]
[null,null,null,"Тип клапана","Материал корпуса","Хар-ка",null,null,null,null,null,null,null,null,null,null,null,"AUMA серия 110",null,null,"REGADA серия 100"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ES05-11","ES05-12","ES06-4","ST mini","ST 0","ST 0.1","ST 1"]
[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31]
["RV",103,"END",4,3,1,1,16,150,15,0.81,null,"КПСР",1,1,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,{"$f":"M8&\" \"&N8&\"-\"&O8&\"-\"&P8&\"-\"&Q8&\"-\"&R8&\"-\"&Y8&\"-\"&Z8&\"-\"&AA8&\"-\"&AB8&\"-\"&AC8","v":"КПСР 1-1-15-4-1.3500-СЧ-1,6-1-150-У"},null,null,1.6,{"$f":"M8&\" \"&N8&\"-\"&O8&\"-\"&P8&\"-\"&Q8&\"-\"&U8&\"-\"&Y8&\"-\"&Z8&\"-\"&AA8&\"-\"&AB8&\"-\"&AC8","v":"КПСР 1-1-15-4-1.1100-СЧ-1,6-1-150-У"}]
["RV",103,"ERE",4,3,1,1,16,150,15,1.6,null,"КПСР",1,1,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,{"$f":"M9&\" \"&N9&\"-\"&O9&\"-\"&P9&\"-\"&Q9&\"-\"&R9&\"-\"&Y9&\"-\"&Z9&\"-\"&AA9&\"-\"&AB9&\"-\"&AC9","v":"КПСР 1-1-15-4-1.3500-СЧ-1,6-1-150-У"},null,null,1.6,{"$f":"M9&\" \"&N9&\"-\"&O9&\"-\"&P9&\"-\"&Q9&\"-\"&U9&\"-\"&Y9&\"-\"&Z9&\"-\"&AA9&\"-\"&AB9&\"-\"&AC9","v":"КПСР 1-1-15-4-1.1100-СЧ-1,6-1-150-У"}]
["RV",103,"ERA",4,3,1,1,16,150,15,1.6,null,"КПСР",1,1,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-4-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,1,16,150,15,1.6,null,"КПСР",1,1,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-4-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,1,16,150,15,1.6,null,"КПСР",1,1,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-4-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,1,16,150,15,1.6,null,"КПСР",1,1,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-4-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,1,16,150,15,1.6,null,"КПСР",1,1,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-4-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,2,16,150,15,0.81,null,"КПСР",1,1,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,2,16,150,15,1.6,null,"КПСР",1,1,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,2,16,150,15,1.6,null,"КПСР",1,1,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,2,16,150,15,1.6,null,"КПСР",1,1,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,2,16,150,15,1.6,null,"КПСР",1,1,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,2,16,150,15,1.6,null,"КПСР",1,1,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,2,16,150,15,1.6,null,"КПСР",1,1,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,3,16,150,15,0.81,null,"КПСР",1,1,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1,6-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1,6-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,3,16,150,15,1.6,null,"КПСР",1,1,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1,6-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1,6-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,3,16,150,15,1.6,null,"КПСР",1,1,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1,6-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1,6-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,3,16,150,15,1.6,null,"КПСР",1,1,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1,6-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1,6-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,3,16,150,15,1.6,null,"КПСР",1,1,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1,6-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1,6-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,3,16,150,15,1.6,null,"КПСР",1,1,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1,6-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1,6-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,3,16,150,15,1.6,null,"КПСР",1,1,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1,6-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1,6-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,4,16,150,15,0.81,null,"КПСР",1,1,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,4,16,150,15,1.6,null,"КПСР",1,1,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,4,16,150,15,1.6,null,"КПСР",1,1,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,4,16,150,15,1.6,null,"КПСР",1,1,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,4,16,150,15,1.6,null,"КПСР",1,1,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,4,16,150,15,1.6,null,"КПСР",1,1,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,4,16,150,15,1.6,null,"КПСР",1,1,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-1-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-1-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,5,16,150,15,0.81,null,"КПСР",1,1,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-0,63-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-0,63-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,5,16,150,15,1.6,null,"КПСР",1,1,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-0,63-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-0,63-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,5,16,150,15,1.6,null,"КПСР",1,1,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-0,63-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-0,63-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,5,16,150,15,1.6,null,"КПСР",1,1,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-0,63-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-0,63-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,5,16,150,15,1.6,null,"КПСР",1,1,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-0,63-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-0,63-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,5,16,150,15,1.6,null,"КПСР",1,1,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-0,63-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-0,63-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,5,16,150,15,1.6,null,"КПСР",1,1,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6,"КПСР 1-1-15-0,63-1.3500-СЧ-1,6-1-150-У",null,null,1.6,"КПСР 1-1-15-0,63-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,1,16,150,20,0.45,null,"КПСР",1,1,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-6,3-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,1,16,150,20,1.07,null,"КПСР",1,1,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-6,3-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,1,16,150,20,1.32,null,"КПСР",1,1,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-6,3-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,1,16,150,20,1.32,null,"КПСР",1,1,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-6,3-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,1,16,150,20,1.6,null,"КПСР",1,1,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-6,3-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,1,16,150,20,1.6,null,"КПСР",1,1,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-6,3-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,1,16,150,20,1.6,null,"КПСР",1,1,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-6,3-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,2,16,150,20,0.45,null,"КПСР",1,1,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-4-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,2,16,150,20,1.07,null,"КПСР",1,1,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-4-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,2,16,150,20,1.32,null,"КПСР",1,1,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-4-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,2,16,150,20,1.32,null,"КПСР",1,1,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-4-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,2,16,150,20,1.6,null,"КПСР",1,1,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-4-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,2,16,150,20,1.6,null,"КПСР",1,1,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-4-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,2,16,150,20,1.6,null,"КПСР",1,1,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-4-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,3,16,150,20,0.45,null,"КПСР",1,1,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,3,16,150,20,1.07,null,"КПСР",1,1,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,3,16,150,20,1.32,null,"КПСР",1,1,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,3,16,150,20,1.32,null,"КПСР",1,1,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,3,16,150,20,1.6,null,"КПСР",1,1,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,3,16,150,20,1.6,null,"КПСР",1,1,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,3,16,150,20,1.6,null,"КПСР",1,1,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6,"КПСР 1-1-20-2,5-1.3500-СЧ-1,6-1-150-У",null,null,1.2,"КПСР 1-1-20-2,5-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,1,16,150,25,0.28000000000000003,null,"КПСР",1,1,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,{"$f":"M64&\" \"&N64&\"-\"&O64&\"-\"&P64&\"-\"&Q64&\"-\"&R64&\"-\"&Y64&\"-\"&Z64&\"-\"&AA64&\"-\"&AB64&\"-\"&AC64","v":"КПСР 1-1-25-10-1.3500-СЧ-1,6-1-150-У"},null,null,0.74,"КПСР 1-1-25-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,1,16,150,25,0.69,null,"КПСР",1,1,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-10-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,1,16,150,25,0.85,null,"КПСР",1,1,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-10-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,1,16,150,25,0.85,null,"КПСР",1,1,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-10-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,1,16,150,25,1.6,null,"КПСР",1,1,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-10-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,1,16,150,25,1.6,null,"КПСР",1,1,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-10-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,1,16,150,25,1.6,null,"КПСР",1,1,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-10-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,2,16,150,25,0.28000000000000003,null,"КПСР",1,1,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-6,3-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,2,16,150,25,0.69,null,"КПСР",1,1,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-6,3-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,2,16,150,25,0.85,null,"КПСР",1,1,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,{"$f":"M73&\" \"&N73&\"-\"&O73&\"-\"&P73&\"-\"&Q73&\"-\"&R73&\"-\"&Y73&\"-\"&Z73&\"-\"&AA73&\"-\"&AB73&\"-\"&AC73","v":"КПСР 1-1-25-6,3-1.3500-СЧ-1,6-1-150-У"},null,null,0.74,{"$f":"M73&\" \"&N73&\"-\"&O73&\"-\"&P73&\"-\"&Q73&\"-\"&U73&\"-\"&Y73&\"-\"&Z73&\"-\"&AA73&\"-\"&AB73&\"-\"&AC73","v":"КПСР 1-1-25-6,3-1.1100-СЧ-1,6-1-150-У"}]
["RV",103,"ENA",4,3,1,2,16,150,25,0.85,null,"КПСР",1,1,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-6,3-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,2,16,150,25,1.6,null,"КПСР",1,1,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-6,3-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,2,16,150,25,1.6,null,"КПСР",1,1,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-6,3-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,2,16,150,25,1.6,null,"КПСР",1,1,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-6,3-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,3,16,150,25,0.28000000000000003,null,"КПСР",1,1,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-4-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,3,16,150,25,0.69,null,"КПСР",1,1,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-4-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,3,16,150,25,0.85,null,"КПСР",1,1,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-4-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,3,16,150,25,0.85,null,"КПСР",1,1,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-4-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,3,16,150,25,1.6,null,"КПСР",1,1,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-4-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,3,16,150,25,1.6,null,"КПСР",1,1,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-4-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,3,16,150,25,1.6,null,"КПСР",1,1,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6,"КПСР 1-1-25-4-1.3500-СЧ-1,6-1-150-У",null,null,0.74,"КПСР 1-1-25-4-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,1,16,150,32,0.16,null,"КПСР",1,1,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-16-1.3500-СЧ-1,6-1-150-У",{"$f":"M85&\" \"&N85&\"-\"&O85&\"-\"&P85&\"-\"&Q85&\"-\"&S85&\"-\"&Y85&\"-\"&Z85&\"-\"&AA85&\"-\"&AB85&\"-\"&AC85","v":"КПСР 1-1-32-16--СЧ-1,6-1-150-У"},null,0.68,"КПСР 1-1-32-16-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,1,16,150,32,0.42,null,"КПСР",1,1,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-16-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-16--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-16-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,1,16,150,32,0.52,null,"КПСР",1,1,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-16-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-16--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-16-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,1,16,150,32,0.52,null,"КПСР",1,1,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-16-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-16--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-16-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,1,16,150,32,1.1399999999999999,null,"КПСР",1,1,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-16-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-16--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-16-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,1,16,150,32,1.6,null,"КПСР",1,1,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-16-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-16--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-16-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,1,16,150,32,1.6,null,"КПСР",1,1,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-16-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-16--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-16-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,2,16,150,32,0.16,null,"КПСР",1,1,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-10-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-10--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,2,16,150,32,0.42,null,"КПСР",1,1,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-10-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-10--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,2,16,150,32,0.52,null,"КПСР",1,1,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-10-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-10--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,2,16,150,32,0.52,null,"КПСР",1,1,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-10-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-10--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,2,16,150,32,1.1399999999999999,null,"КПСР",1,1,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-10-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-10--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,2,16,150,32,1.6,null,"КПСР",1,1,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-10-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-10--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,2,16,150,32,1.6,null,"КПСР",1,1,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-10-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-10--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-10-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,3,16,150,32,0.16,null,"КПСР",1,1,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-6,3-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-6,3--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,3,16,150,32,0.42,null,"КПСР",1,1,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-6,3-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-6,3--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,3,16,150,32,0.52,null,"КПСР",1,1,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-6,3-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-6,3--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,3,16,150,32,0.52,null,"КПСР",1,1,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-6,3-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-6,3--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,3,16,150,32,1.1399999999999999,null,"КПСР",1,1,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-6,3-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-6,3--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,3,16,150,32,1.6,null,"КПСР",1,1,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-6,3-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-6,3--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,3,16,150,32,1.6,null,"КПСР",1,1,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6,"КПСР 1-1-32-6,3-1.3500-СЧ-1,6-1-150-У","КПСР 1-1-32-6,3--СЧ-1,6-1-150-У",null,0.68,"КПСР 1-1-32-6,3-1.1100-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,1,16,150,40,0.1,null,"КПСР",1,1,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-25--СЧ-1,6-1-150-У","КПСР 1-1-40-25-1.3501-СЧ-1,6-1-150-У",{"$f":"M106&\" \"&N106&\"-\"&O106&\"-\"&P106&\"-\"&Q106&\"-\"&T106&\"-\"&Y106&\"-\"&Z106&\"-\"&AA106&\"-\"&AB106&\"-\"&AC106","v":"КПСР 1-1-40-25--СЧ-1,6-1-150-У"},0.5,"КПСР 1-1-40-25-1.1100-СЧ-1,6-1-150-У",{"$f":"M106&\" \"&N106&\"-\"&O106&\"-\"&P106&\"-\"&Q106&\"-\"&V106&\"-\"&Y106&\"-\"&Z106&\"-\"&AA106&\"-\"&AB106&\"-\"&AC106","v":"КПСР 1-1-40-25--СЧ-1,6-1-150-У"}]
["RV",103,"ERE",4,3,1,1,16,150,40,0.27,null,"КПСР",1,1,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-25--СЧ-1,6-1-150-У","КПСР 1-1-40-25-1.3501-СЧ-1,6-1-150-У",{"$f":"M107&\" \"&N107&\"-\"&O107&\"-\"&P107&\"-\"&Q107&\"-\"&T107&\"-\"&Y107&\"-\"&Z107&\"-\"&AA107&\"-\"&AB107&\"-\"&AC107","v":"КПСР 1-1-40-25--СЧ-1,6-1-150-У"},0.5,"КПСР 1-1-40-25-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-25--СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,1,16,150,40,0.33,null,"КПСР",1,1,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-25--СЧ-1,6-1-150-У","КПСР 1-1-40-25-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-25--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-25-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-25--СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,1,16,150,40,0.33,null,"КПСР",1,1,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-25--СЧ-1,6-1-150-У","КПСР 1-1-40-25-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-25--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-25-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-25--СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,1,16,150,40,0.74,null,"КПСР",1,1,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-25--СЧ-1,6-1-150-У","КПСР 1-1-40-25-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-25--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-25-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-25--СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,1,16,150,40,1.1499999999999999,null,"КПСР",1,1,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-25--СЧ-1,6-1-150-У","КПСР 1-1-40-25-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-25--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-25-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-25--СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,1,16,150,40,1.29,null,"КПСР",1,1,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-25--СЧ-1,6-1-150-У","КПСР 1-1-40-25-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-25--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-25-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-25--СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,2,16,150,40,0.1,null,"КПСР",1,1,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-16--СЧ-1,6-1-150-У","КПСР 1-1-40-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,2,16,150,40,0.27,null,"КПСР",1,1,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-16--СЧ-1,6-1-150-У","КПСР 1-1-40-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,2,16,150,40,0.33,null,"КПСР",1,1,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-16--СЧ-1,6-1-150-У","КПСР 1-1-40-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,2,16,150,40,0.33,null,"КПСР",1,1,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-16--СЧ-1,6-1-150-У","КПСР 1-1-40-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,2,16,150,40,0.74,null,"КПСР",1,1,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-16--СЧ-1,6-1-150-У","КПСР 1-1-40-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,2,16,150,40,1.1499999999999999,null,"КПСР",1,1,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-16--СЧ-1,6-1-150-У","КПСР 1-1-40-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,2,16,150,40,1.29,null,"КПСР",1,1,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-16--СЧ-1,6-1-150-У","КПСР 1-1-40-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-16--СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,3,16,150,40,0.1,null,"КПСР",1,1,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-10--СЧ-1,6-1-150-У","КПСР 1-1-40-10-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-10-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,3,16,150,40,0.27,null,"КПСР",1,1,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-10--СЧ-1,6-1-150-У","КПСР 1-1-40-10-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-10-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,3,16,150,40,0.33,null,"КПСР",1,1,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-10--СЧ-1,6-1-150-У","КПСР 1-1-40-10-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-10-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,3,16,150,40,0.33,null,"КПСР",1,1,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-10--СЧ-1,6-1-150-У","КПСР 1-1-40-10-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-10-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,3,16,150,40,0.74,null,"КПСР",1,1,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-10--СЧ-1,6-1-150-У","КПСР 1-1-40-10-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-10-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,3,16,150,40,1.1499999999999999,null,"КПСР",1,1,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-10--СЧ-1,6-1-150-У","КПСР 1-1-40-10-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-10-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,3,16,150,40,1.29,null,"КПСР",1,1,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6,"КПСР 1-1-40-10--СЧ-1,6-1-150-У","КПСР 1-1-40-10-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У",0.5,"КПСР 1-1-40-10-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-40-10--СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,1,16,150,50,0.05,null,"КПСР",1,1,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-40-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-40--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-40-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-40-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,1,16,150,50,0.15,null,"КПСР",1,1,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-40-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-40--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-40-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-40-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,1,16,150,50,0.19,null,"КПСР",1,1,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-40-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-40--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-40-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-40-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,1,16,150,50,0.19,null,"КПСР",1,1,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-40-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-40--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-40-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-40-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,1,16,150,50,0.44,null,"КПСР",1,1,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-40-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-40--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-40-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-40-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,1,16,150,50,0.69,null,"КПСР",1,1,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-40-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-40--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-40-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-40-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,1,16,150,50,0.78,null,"КПСР",1,1,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-40-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-40--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-40-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-40-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,2,16,150,50,0.05,null,"КПСР",1,1,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-25-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-25--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-25-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-25-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,2,16,150,50,0.15,null,"КПСР",1,1,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-25-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-25--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-25-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-25-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,2,16,150,50,0.19,null,"КПСР",1,1,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-25-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-25--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-25-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-25-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,2,16,150,50,0.19,null,"КПСР",1,1,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-25-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-25--СЧ-1,6-1-150-У",0.8,{"$f":"M137&\" \"&N137&\"-\"&O137&\"-\"&P137&\"-\"&Q137&\"-\"&U137&\"-\"&Y137&\"-\"&Z137&\"-\"&AA137&\"-\"&AB137&\"-\"&AC137","v":"КПСР 1-1-50-25-1.1100-СЧ-1,6-1-150-У"},"КПСР 1-1-50-25-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,2,16,150,50,0.44,null,"КПСР",1,1,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-25-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-25--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-25-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-25-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,2,16,150,50,0.69,null,"КПСР",1,1,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-25-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-25--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-25-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-25-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,2,16,150,50,0.78,null,"КПСР",1,1,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-25-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-25--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-25-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-25-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,1,3,16,150,50,0.05,null,"КПСР",1,1,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-16--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-16-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ERE",4,3,1,3,16,150,50,0.15,null,"КПСР",1,1,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-16--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-16-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,3,16,150,50,0.19,null,"КПСР",1,1,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-16--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-16-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,3,16,150,50,0.19,null,"КПСР",1,1,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-16--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-16-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ERA",4,3,1,3,16,150,50,0.44,null,"КПСР",1,1,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-16--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-16-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ENA",4,3,1,3,16,150,50,0.69,null,"КПСР",1,1,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-16--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-16-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"ERB",4,3,1,3,16,150,50,0.78,null,"КПСР",1,1,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6,null,"КПСР 1-1-50-16-1.3501-СЧ-1,6-1-150-У","КПСР 1-1-50-16--СЧ-1,6-1-150-У",0.8,"КПСР 1-1-50-16-1.1100-СЧ-1,6-1-150-У","КПСР 1-1-50-16-1.1200-СЧ-1,6-1-150-У"]
["RV",103,"END",4,3,2,1,16,150,15,0.81,null,"КПСР",1,2,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERE",4,3,2,1,16,150,15,1.6,null,"КПСР",1,2,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERA",4,3,2,1,16,150,15,1.6,null,"КПСР",1,2,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ENA",4,3,2,1,16,150,15,1.6,null,"КПСР",1,2,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERA",4,3,2,1,16,150,15,1.6,null,"КПСР",1,2,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ENA",4,3,2,1,16,150,15,1.6,null,"КПСР",1,2,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERB",4,3,2,1,16,150,15,1.6,null,"КПСР",1,2,15,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"END",4,3,2,2,16,150,15,0.81,null,"КПСР",1,2,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERE",4,3,2,2,16,150,15,1.6,null,"КПСР",1,2,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERA",4,3,2,2,16,150,15,1.6,null,"КПСР",1,2,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ENA",4,3,2,2,16,150,15,1.6,null,"КПСР",1,2,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERA",4,3,2,2,16,150,15,1.6,null,"КПСР",1,2,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ENA",4,3,2,2,16,150,15,1.6,null,"КПСР",1,2,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERB",4,3,2,2,16,150,15,1.6,null,"КПСР",1,2,15,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"END",4,3,2,3,16,150,15,0.81,null,"КПСР",1,2,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERE",4,3,2,3,16,150,15,1.6,null,"КПСР",1,2,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERA",4,3,2,3,16,150,15,1.6,null,"КПСР",1,2,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ENA",4,3,2,3,16,150,15,1.6,null,"КПСР",1,2,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERA",4,3,2,3,16,150,15,1.6,null,"КПСР",1,2,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ENA",4,3,2,3,16,150,15,1.6,null,"КПСР",1,2,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERB",4,3,2,3,16,150,15,1.6,null,"КПСР",1,2,15,1.6,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"END",4,3,2,4,16,150,15,0.81,null,"КПСР",1,2,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERE",4,3,2,4,16,150,15,1.6,null,"КПСР",1,2,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERA",4,3,2,4,16,150,15,1.6,null,"КПСР",1,2,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ENA",4,3,2,4,16,150,15,1.6,null,"КПСР",1,2,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERA",4,3,2,4,16,150,15,1.6,null,"КПСР",1,2,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ENA",4,3,2,4,16,150,15,1.6,null,"КПСР",1,2,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERB",4,3,2,4,16,150,15,1.6,null,"КПСР",1,2,15,1,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"END",4,3,2,5,16,150,15,0.81,null,"КПСР",1,2,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERE",4,3,2,5,16,150,15,1.6,null,"КПСР",1,2,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERA",4,3,2,5,16,150,15,1.6,null,"КПСР",1,2,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ENA",4,3,2,5,16,150,15,1.6,null,"КПСР",1,2,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERA",4,3,2,5,16,150,15,1.6,null,"КПСР",1,2,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ENA",4,3,2,5,16,150,15,1.6,null,"КПСР",1,2,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"ERB",4,3,2,5,16,150,15,1.6,null,"КПСР",1,2,15,0.63,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.5,1.6]
["RV",103,"END",4,3,2,1,16,150,20,0.45,null,"КПСР",1,2,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ERE",4,3,2,1,16,150,20,1.07,null,"КПСР",1,2,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ERA",4,3,2,1,16,150,20,1.32,null,"КПСР",1,2,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ENA",4,3,2,1,16,150,20,1.32,null,"КПСР",1,2,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ERA",4,3,2,1,16,150,20,1.6,null,"КПСР",1,2,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ENA",4,3,2,1,16,150,20,1.6,null,"КПСР",1,2,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ERB",4,3,2,1,16,150,20,1.6,null,"КПСР",1,2,20,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"END",4,3,2,2,16,150,20,0.45,null,"КПСР",1,2,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ERE",4,3,2,2,16,150,20,1.07,null,"КПСР",1,2,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ERA",4,3,2,2,16,150,20,1.32,null,"КПСР",1,2,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ENA",4,3,2,2,16,150,20,1.32,null,"КПСР",1,2,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ERA",4,3,2,2,16,150,20,1.6,null,"КПСР",1,2,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ENA",4,3,2,2,16,150,20,1.6,null,"КПСР",1,2,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ERB",4,3,2,2,16,150,20,1.6,null,"КПСР",1,2,20,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"END",4,3,2,3,16,150,20,0.45,null,"КПСР",1,2,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ERE",4,3,2,3,16,150,20,1.07,null,"КПСР",1,2,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ERA",4,3,2,3,16,150,20,1.32,null,"КПСР",1,2,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ENA",4,3,2,3,16,150,20,1.32,null,"КПСР",1,2,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ERA",4,3,2,3,16,150,20,1.6,null,"КПСР",1,2,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ENA",4,3,2,3,16,150,20,1.6,null,"КПСР",1,2,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"ERB",4,3,2,3,16,150,20,1.6,null,"КПСР",1,2,20,2.5,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",1.2,1.6]
["RV",103,"END",4,3,2,1,16,150,25,0.28000000000000003,null,"КПСР",1,2,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ERE",4,3,2,1,16,150,25,0.69,null,"КПСР",1,2,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ERA",4,3,2,1,16,150,25,0.85,null,"КПСР",1,2,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ENA",4,3,2,1,16,150,25,0.85,null,"КПСР",1,2,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ERA",4,3,2,1,16,150,25,1.6,null,"КПСР",1,2,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ENA",4,3,2,1,16,150,25,1.6,null,"КПСР",1,2,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ERB",4,3,2,1,16,150,25,1.6,null,"КПСР",1,2,25,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"END",4,3,2,2,16,150,25,0.28000000000000003,null,"КПСР",1,2,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ERE",4,3,2,2,16,150,25,0.69,null,"КПСР",1,2,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ERA",4,3,2,2,16,150,25,0.85,null,"КПСР",1,2,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ENA",4,3,2,2,16,150,25,0.85,null,"КПСР",1,2,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ERA",4,3,2,2,16,150,25,1.6,null,"КПСР",1,2,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ENA",4,3,2,2,16,150,25,1.6,null,"КПСР",1,2,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ERB",4,3,2,2,16,150,25,1.6,null,"КПСР",1,2,25,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"END",4,3,2,3,16,150,25,0.28000000000000003,null,"КПСР",1,2,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ERE",4,3,2,3,16,150,25,0.69,null,"КПСР",1,2,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ERA",4,3,2,3,16,150,25,0.85,null,"КПСР",1,2,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ENA",4,3,2,3,16,150,25,0.85,null,"КПСР",1,2,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ERA",4,3,2,3,16,150,25,1.6,null,"КПСР",1,2,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ENA",4,3,2,3,16,150,25,1.6,null,"КПСР",1,2,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"ERB",4,3,2,3,16,150,25,1.6,null,"КПСР",1,2,25,4,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.74,1.6]
["RV",103,"END",4,3,2,1,16,150,32,0.16,null,"КПСР",1,2,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ERE",4,3,2,1,16,150,32,0.42,null,"КПСР",1,2,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ERA",4,3,2,1,16,150,32,0.52,null,"КПСР",1,2,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ENA",4,3,2,1,16,150,32,0.52,null,"КПСР",1,2,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ERA",4,3,2,1,16,150,32,1.1399999999999999,null,"КПСР",1,2,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ENA",4,3,2,1,16,150,32,1.6,null,"КПСР",1,2,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ERB",4,3,2,1,16,150,32,1.6,null,"КПСР",1,2,32,16,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"END",4,3,2,2,16,150,32,0.16,null,"КПСР",1,2,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ERE",4,3,2,2,16,150,32,0.42,null,"КПСР",1,2,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ERA",4,3,2,2,16,150,32,0.52,null,"КПСР",1,2,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ENA",4,3,2,2,16,150,32,0.52,null,"КПСР",1,2,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ERA",4,3,2,2,16,150,32,1.1399999999999999,null,"КПСР",1,2,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ENA",4,3,2,2,16,150,32,1.6,null,"КПСР",1,2,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ERB",4,3,2,2,16,150,32,1.6,null,"КПСР",1,2,32,10,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"END",4,3,2,3,16,150,32,0.16,null,"КПСР",1,2,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ERE",4,3,2,3,16,150,32,0.42,null,"КПСР",1,2,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ERA",4,3,2,3,16,150,32,0.52,null,"КПСР",1,2,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ENA",4,3,2,3,16,150,32,0.52,null,"КПСР",1,2,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ERA",4,3,2,3,16,150,32,1.1399999999999999,null,"КПСР",1,2,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ENA",4,3,2,3,16,150,32,1.6,null,"КПСР",1,2,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"ERB",4,3,2,3,16,150,32,1.6,null,"КПСР",1,2,32,6.3,"1.3500",null,null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.68,1.6]
["RV",103,"END",4,3,2,1,16,150,40,0.1,null,"КПСР",1,2,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ERE",4,3,2,1,16,150,40,0.27,null,"КПСР",1,2,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ERA",4,3,2,1,16,150,40,0.33,null,"КПСР",1,2,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ENA",4,3,2,1,16,150,40,0.33,null,"КПСР",1,2,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ERA",4,3,2,1,16,150,40,0.74,null,"КПСР",1,2,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ENA",4,3,2,1,16,150,40,1.1499999999999999,null,"КПСР",1,2,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ERB",4,3,2,1,16,150,40,1.29,null,"КПСР",1,2,40,25,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"END",4,3,2,2,16,150,40,0.1,null,"КПСР",1,2,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ERE",4,3,2,2,16,150,40,0.27,null,"КПСР",1,2,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ERA",4,3,2,2,16,150,40,0.33,null,"КПСР",1,2,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ENA",4,3,2,2,16,150,40,0.33,null,"КПСР",1,2,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ERA",4,3,2,2,16,150,40,0.74,null,"КПСР",1,2,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ENA",4,3,2,2,16,150,40,1.1499999999999999,null,"КПСР",1,2,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ERB",4,3,2,2,16,150,40,1.29,null,"КПСР",1,2,40,16,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"END",4,3,2,3,16,150,40,0.1,null,"КПСР",1,2,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ERE",4,3,2,3,16,150,40,0.27,null,"КПСР",1,2,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ERA",4,3,2,3,16,150,40,0.33,null,"КПСР",1,2,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ENA",4,3,2,3,16,150,40,0.33,null,"КПСР",1,2,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ERA",4,3,2,3,16,150,40,0.74,null,"КПСР",1,2,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ENA",4,3,2,3,16,150,40,1.1499999999999999,null,"КПСР",1,2,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"ERB",4,3,2,3,16,150,40,1.29,null,"КПСР",1,2,40,10,null,"1.3501",null,"1.1100",null,null,null,"СЧ",1.6,1,150,"У",0.5,1.6]
["RV",103,"END",4,3,2,1,16,150,50,0.05,null,"КПСР",1,2,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ERE",4,3,2,1,16,150,50,0.15,null,"КПСР",1,2,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ERA",4,3,2,1,16,150,50,0.19,null,"КПСР",1,2,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ENA",4,3,2,1,16,150,50,0.19,null,"КПСР",1,2,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ERA",4,3,2,1,16,150,50,0.44,null,"КПСР",1,2,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ENA",4,3,2,1,16,150,50,0.69,null,"КПСР",1,2,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ERB",4,3,2,1,16,150,50,0.78,null,"КПСР",1,2,50,40,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"END",4,3,2,2,16,150,50,0.05,null,"КПСР",1,2,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ERE",4,3,2,2,16,150,50,0.15,null,"КПСР",1,2,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ERA",4,3,2,2,16,150,50,0.19,null,"КПСР",1,2,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ENA",4,3,2,2,16,150,50,0.19,null,"КПСР",1,2,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ERA",4,3,2,2,16,150,50,0.44,null,"КПСР",1,2,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ENA",4,3,2,2,16,150,50,0.69,null,"КПСР",1,2,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ERB",4,3,2,2,16,150,50,0.78,null,"КПСР",1,2,50,25,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"END",4,3,2,3,16,150,50,0.05,null,"КПСР",1,2,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ERE",4,3,2,3,16,150,50,0.15,null,"КПСР",1,2,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ERA",4,3,2,3,16,150,50,0.19,null,"КПСР",1,2,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ENA",4,3,2,3,16,150,50,0.19,null,"КПСР",1,2,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ERA",4,3,2,3,16,150,50,0.44,null,"КПСР",1,2,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ENA",4,3,2,3,16,150,50,0.69,null,"КПСР",1,2,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",103,"ERB",4,3,2,3,16,150,50,0.78,null,"КПСР",1,2,50,16,null,"1.3501",null,"1.1100","1.1200",null,null,"СЧ",1.6,1,150,"У","0,25  0,8",1.6]
["RV",111,"R",2,3,1,1,16,150,15,null,null,"КПСР",1,1,15,4,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,1,2,16,150,15,null,null,"КПСР",1,1,15,2.5,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,1,3,16,150,15,null,null,"КПСР",1,1,15,1.6,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,1,4,16,150,15,null,null,"КПСР",1,1,15,1,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,1,5,16,150,15,null,null,"КПСР",1,1,15,0.63,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,1,6,16,150,15,null,null,"КПСР",1,1,15,0.4,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,1,7,16,150,15,null,null,"КПСР",1,1,15,0.25,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,1,8,16,150,15,null,null,"КПСР",1,1,15,0.16,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,1,1,16,150,20,null,null,"КПСР",1,1,20,6.3,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,1,1,16,150,25,null,null,"КПСР",1,1,25,10,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,1,1,16,150,32,null,null,"КПСР",1,1,32,16,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,1,1,16,150,40,null,null,"КПСР",1,1,40,25,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,2,1,16,150,15,null,null,"КПСР",1,2,15,4,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,2,2,16,150,15,null,null,"КПСР",1,2,15,2.5,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,2,3,16,150,15,null,null,"КПСР",1,2,15,1.6,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,2,4,16,150,15,null,null,"КПСР",1,2,15,1,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,2,5,16,150,15,null,null,"КПСР",1,2,15,0.63,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,2,6,16,150,15,null,null,"КПСР",1,2,15,0.4,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,2,7,16,150,15,null,null,"КПСР",1,2,15,0.25,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,2,8,16,150,15,null,null,"КПСР",1,2,15,0.16,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,2,1,16,150,20,null,null,"КПСР",1,2,20,6.3,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,2,1,16,150,25,null,null,"КПСР",1,2,25,10,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,2,1,16,150,32,null,null,"КПСР",1,2,32,16,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"R",2,3,2,1,16,150,40,null,null,"КПСР",1,2,40,25,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,1,1,16,150,15,null,null,"КПСР",1,1,15,4,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,1,2,16,150,15,null,null,"КПСР",1,1,15,2.5,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,1,3,16,150,15,null,null,"КПСР",1,1,15,1.6,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,1,4,16,150,15,null,null,"КПСР",1,1,15,1,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,1,5,16,150,15,null,null,"КПСР",1,1,15,0.63,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,1,6,16,150,15,null,null,"КПСР",1,1,15,0.4,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,1,7,16,150,15,null,null,"КПСР",1,1,15,0.25,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,1,8,16,150,15,null,null,"КПСР",1,1,15,0.16,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,1,1,16,150,20,null,null,"КПСР",1,1,20,6.3,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,1,1,16,150,25,null,null,"КПСР",1,1,25,10,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,1,1,16,150,32,null,null,"КПСР",1,1,32,16,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,1,1,16,150,40,null,null,"КПСР",1,1,40,25,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,2,1,16,150,15,null,null,"КПСР",1,2,15,4,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,2,2,16,150,15,null,null,"КПСР",1,2,15,2.5,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,2,3,16,150,15,null,null,"КПСР",1,2,15,1.6,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,2,4,16,150,15,null,null,"КПСР",1,2,15,1,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,2,5,16,150,15,null,null,"КПСР",1,2,15,0.63,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,2,6,16,150,15,null,null,"КПСР",1,2,15,0.4,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,2,7,16,150,15,null,null,"КПСР",1,2,15,0.25,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,2,8,16,150,15,null,null,"КПСР",1,2,15,0.16,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,2,1,16,150,20,null,null,"КПСР",1,2,20,6.3,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,2,1,16,150,25,null,null,"КПСР",1,2,25,10,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,2,1,16,150,32,null,null,"КПСР",1,2,32,16,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV",111,"S",2,3,2,1,16,150,40,null,null,"КПСР",1,2,40,25,null,null,null,null,null,null,null,"СЧ",1.6,1,150,"У"]
["RV","113 R",null,4,3,3,1,16,150,50,1.6,null,"КПСР",1,1,50,40,null,null,"1.3600",null,"1.1200",null,null,"СЧ",1.6,1,150,"У","0,7  0,8"]
["RV","113 R",null,4,3,3,1,16,150,65,1.6,null,"КПСР",1,1,65,63,null,null,"1.3600",null,"1.1200",null,null,"СЧ",1.6,1,150,"У","1   1,5"]
["RV","113 R",null,4,3,3,1,16,150,80,1.6,null,"КПСР",1,1,80,100,null,null,"1.3600",null,"1.1200",null,null,"СЧ",1.6,1,150,"У","0,8   1"]
["RV","113 R",null,4,3,3,1,16,150,100,1.6,null,"КПСР",1,1,100,160,null,null,null,null,"1.1200",null,null,"СЧ",1.6,1,150,"У",0.8]
["RV","113 R",null,4,3,3,1,16,150,125,1.6,null,"КПСР",1,1,125,250,null,null,null,null,null,"1.1300",null,"СЧ",1.6,1,150,"У",1]
["RV","113 R",null,4,3,3,1,16,150,150,1.6,null,"КПСР",1,1,150,360,null,null,null,null,null,null,"1.1400","СЧ",1.6,1,150,"У",1]

{"sheet":"Подбор RD","index":36,"n_rows":102,"n_cols":31,"rows_kept":102,"cut":false,"hidden":false,"merged":[[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,6,4,6],[3,14,4,14],[3,7,4,7],[3,8,4,8],[3,9,4,9],[3,11,4,11],[3,12,4,12],[3,27,4,27],[3,28,4,28],[3,29,4,29],[3,30,4,30],[3,3,3,4],[3,5,4,5],[3,15,3,18],[3,21,4,21],[3,22,4,22],[3,23,4,23],[3,24,4,24],[3,25,4,25],[3,26,4,26],[3,19,4,19],[3,20,4,20],[3,13,4,13]]}
[]
[]
[]
["Марка","Серия","Тип","Исполнение",null,"Диапазон настройи","Pn, Bar","T","DN",null,null,"Тип изделия","Тип клапана","DN","Kvs, м³/ч","Диапазон настройки, МПа, №",null,null,null,"Pn, МПа","Присоеди-нение к тр-ду","Т","Клим исполн",null,null,"Привод AUMA ES05-11","Привод AUMA ES05-12","Привод AUMA ES06-4","ΔP max. Мпа серия 100","Привод Regada ST mini","Привод Regada ST 0"]
[null,null,null,"с манометром","без манометра",null,null,null,null,null,null,null,null,null,null,"0,01-0,1","0,04-0,16","0,1-0,4","0,3-0,7"]
[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23]
["RD",103,"V",3,null,1,16,140,15,null,null,"РА","А",15,2.5,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L7&\" \"&M7&\"-\"&#REF!&\"-\"&N7&\"-\"&O7&\"-\"&P7&\"-\"&#REF!&\"-\"&T7&\"-\"&U7&\"-\"&V7&\"-\"&W7","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L7&\" \"&M7&\"-\"&#REF!&\"-\"&N7&\"-\"&O7&\"-\"&S7&\"-\"&#REF!&\"-\"&T7&\"-\"&U7&\"-\"&V7&\"-\"&W7","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,1,16,140,15,null,null,"РА","А",15,2.5,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L8&\" \"&M8&\"-\"&#REF!&\"-\"&N8&\"-\"&O8&\"-\"&P8&\"-\"&#REF!&\"-\"&T8&\"-\"&U8&\"-\"&V8&\"-\"&#REF!","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L8&\" \"&M8&\"-\"&#REF!&\"-\"&N8&\"-\"&O8&\"-\"&S8&\"-\"&#REF!&\"-\"&T8&\"-\"&U8&\"-\"&V8&\"-\"&#REF!","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,2,16,140,15,null,null,"РА","А",15,2.5,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L9&\" \"&M9&\"-\"&#REF!&\"-\"&N9&\"-\"&O9&\"-\"&P9&\"-\"&#REF!&\"-\"&T9&\"-\"&U9&\"-\"&V9&\"-\"&W9","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L9&\" \"&M9&\"-\"&#REF!&\"-\"&N9&\"-\"&O9&\"-\"&S9&\"-\"&#REF!&\"-\"&T9&\"-\"&U9&\"-\"&V9&\"-\"&W9","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,2,16,140,15,null,null,"РА","А",15,2.5,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L10&\" \"&M10&\"-\"&#REF!&\"-\"&N10&\"-\"&O10&\"-\"&P10&\"-\"&#REF!&\"-\"&T10&\"-\"&U10&\"-\"&V10&\"-\"&W10","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L10&\" \"&M10&\"-\"&#REF!&\"-\"&N10&\"-\"&O10&\"-\"&S10&\"-\"&#REF!&\"-\"&T10&\"-\"&U10&\"-\"&V10&\"-\"&W10","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,3,16,140,15,null,null,"РА","А",15,2.5,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L11&\" \"&M11&\"-\"&#REF!&\"-\"&N11&\"-\"&O11&\"-\"&P11&\"-\"&#REF!&\"-\"&T11&\"-\"&U11&\"-\"&V11&\"-\"&W11","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L11&\" \"&M11&\"-\"&#REF!&\"-\"&N11&\"-\"&O11&\"-\"&S11&\"-\"&#REF!&\"-\"&T11&\"-\"&U11&\"-\"&V11&\"-\"&W11","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,3,16,140,15,null,null,"РА","А",15,2.5,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L12&\" \"&M12&\"-\"&#REF!&\"-\"&N12&\"-\"&O12&\"-\"&P12&\"-\"&#REF!&\"-\"&T12&\"-\"&U12&\"-\"&V12&\"-\"&W12","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L12&\" \"&M12&\"-\"&#REF!&\"-\"&N12&\"-\"&O12&\"-\"&S12&\"-\"&#REF!&\"-\"&T12&\"-\"&U12&\"-\"&V12&\"-\"&W12","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,4,16,140,15,null,null,"РА","А",15,2.5,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L13&\" \"&M13&\"-\"&#REF!&\"-\"&N13&\"-\"&O13&\"-\"&P13&\"-\"&#REF!&\"-\"&T13&\"-\"&U13&\"-\"&V13&\"-\"&W13","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L13&\" \"&M13&\"-\"&#REF!&\"-\"&N13&\"-\"&O13&\"-\"&S13&\"-\"&#REF!&\"-\"&T13&\"-\"&U13&\"-\"&V13&\"-\"&W13","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,4,16,140,15,null,null,"РА","А",15,2.5,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L14&\" \"&M14&\"-\"&#REF!&\"-\"&N14&\"-\"&O14&\"-\"&P14&\"-\"&#REF!&\"-\"&T14&\"-\"&U14&\"-\"&V14&\"-\"&W14","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L14&\" \"&M14&\"-\"&#REF!&\"-\"&N14&\"-\"&O14&\"-\"&S14&\"-\"&#REF!&\"-\"&T14&\"-\"&U14&\"-\"&V14&\"-\"&W14","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,1,16,140,20,null,null,"РА","А",20,4,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L15&\" \"&M15&\"-\"&#REF!&\"-\"&N15&\"-\"&O15&\"-\"&P15&\"-\"&#REF!&\"-\"&T15&\"-\"&U15&\"-\"&V15&\"-\"&W15","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L15&\" \"&M15&\"-\"&#REF!&\"-\"&N15&\"-\"&O15&\"-\"&S15&\"-\"&#REF!&\"-\"&T15&\"-\"&U15&\"-\"&V15&\"-\"&W15","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,1,16,140,20,null,null,"РА","А",20,4,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L16&\" \"&M16&\"-\"&#REF!&\"-\"&N16&\"-\"&O16&\"-\"&P16&\"-\"&#REF!&\"-\"&T16&\"-\"&U16&\"-\"&V16&\"-\"&W16","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L16&\" \"&M16&\"-\"&#REF!&\"-\"&N16&\"-\"&O16&\"-\"&S16&\"-\"&#REF!&\"-\"&T16&\"-\"&U16&\"-\"&V16&\"-\"&W16","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,2,16,140,20,null,null,"РА","А",20,4,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L17&\" \"&M17&\"-\"&#REF!&\"-\"&N17&\"-\"&O17&\"-\"&P17&\"-\"&#REF!&\"-\"&T17&\"-\"&U17&\"-\"&V17&\"-\"&W17","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L17&\" \"&M17&\"-\"&#REF!&\"-\"&N17&\"-\"&O17&\"-\"&S17&\"-\"&#REF!&\"-\"&T17&\"-\"&U17&\"-\"&V17&\"-\"&W17","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,2,16,140,20,null,null,"РА","А",20,4,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L18&\" \"&M18&\"-\"&#REF!&\"-\"&N18&\"-\"&O18&\"-\"&P18&\"-\"&#REF!&\"-\"&T18&\"-\"&U18&\"-\"&V18&\"-\"&W18","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L18&\" \"&M18&\"-\"&#REF!&\"-\"&N18&\"-\"&O18&\"-\"&S18&\"-\"&#REF!&\"-\"&T18&\"-\"&U18&\"-\"&V18&\"-\"&W18","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,3,16,140,20,null,null,"РА","А",20,4,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L19&\" \"&M19&\"-\"&#REF!&\"-\"&N19&\"-\"&O19&\"-\"&P19&\"-\"&#REF!&\"-\"&T19&\"-\"&U19&\"-\"&V19&\"-\"&W19","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L19&\" \"&M19&\"-\"&#REF!&\"-\"&N19&\"-\"&O19&\"-\"&S19&\"-\"&#REF!&\"-\"&T19&\"-\"&U19&\"-\"&V19&\"-\"&W19","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,3,16,140,20,null,null,"РА","А",20,4,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L20&\" \"&M20&\"-\"&#REF!&\"-\"&N20&\"-\"&O20&\"-\"&P20&\"-\"&#REF!&\"-\"&T20&\"-\"&U20&\"-\"&V20&\"-\"&W20","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L20&\" \"&M20&\"-\"&#REF!&\"-\"&N20&\"-\"&O20&\"-\"&S20&\"-\"&#REF!&\"-\"&T20&\"-\"&U20&\"-\"&V20&\"-\"&W20","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,4,16,140,20,null,null,"РА","А",20,4,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L21&\" \"&M21&\"-\"&#REF!&\"-\"&N21&\"-\"&O21&\"-\"&P21&\"-\"&#REF!&\"-\"&T21&\"-\"&U21&\"-\"&V21&\"-\"&W21","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L21&\" \"&M21&\"-\"&#REF!&\"-\"&N21&\"-\"&O21&\"-\"&S21&\"-\"&#REF!&\"-\"&T21&\"-\"&U21&\"-\"&V21&\"-\"&W21","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,4,16,140,20,null,null,"РА","А",20,4,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L22&\" \"&M22&\"-\"&#REF!&\"-\"&N22&\"-\"&O22&\"-\"&P22&\"-\"&#REF!&\"-\"&T22&\"-\"&U22&\"-\"&V22&\"-\"&W22","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L22&\" \"&M22&\"-\"&#REF!&\"-\"&N22&\"-\"&O22&\"-\"&S22&\"-\"&#REF!&\"-\"&T22&\"-\"&U22&\"-\"&V22&\"-\"&W22","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,1,16,140,25,null,null,"РА","А",25,6.3,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L23&\" \"&M23&\"-\"&#REF!&\"-\"&N23&\"-\"&O23&\"-\"&P23&\"-\"&#REF!&\"-\"&T23&\"-\"&U23&\"-\"&V23&\"-\"&W23","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L23&\" \"&M23&\"-\"&#REF!&\"-\"&N23&\"-\"&O23&\"-\"&S23&\"-\"&#REF!&\"-\"&T23&\"-\"&U23&\"-\"&V23&\"-\"&W23","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,1,16,140,25,null,null,"РА","А",25,6.3,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L24&\" \"&M24&\"-\"&#REF!&\"-\"&N24&\"-\"&O24&\"-\"&P24&\"-\"&#REF!&\"-\"&T24&\"-\"&U24&\"-\"&V24&\"-\"&W24","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L24&\" \"&M24&\"-\"&#REF!&\"-\"&N24&\"-\"&O24&\"-\"&S24&\"-\"&#REF!&\"-\"&T24&\"-\"&U24&\"-\"&V24&\"-\"&W24","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,2,16,140,25,null,null,"РА","А",25,6.3,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L25&\" \"&M25&\"-\"&#REF!&\"-\"&N25&\"-\"&O25&\"-\"&P25&\"-\"&#REF!&\"-\"&T25&\"-\"&U25&\"-\"&V25&\"-\"&W25","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L25&\" \"&M25&\"-\"&#REF!&\"-\"&N25&\"-\"&O25&\"-\"&S25&\"-\"&#REF!&\"-\"&T25&\"-\"&U25&\"-\"&V25&\"-\"&W25","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,2,16,140,25,null,null,"РА","А",25,6.3,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L26&\" \"&M26&\"-\"&#REF!&\"-\"&N26&\"-\"&O26&\"-\"&P26&\"-\"&#REF!&\"-\"&T26&\"-\"&U26&\"-\"&V26&\"-\"&W26","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L26&\" \"&M26&\"-\"&#REF!&\"-\"&N26&\"-\"&O26&\"-\"&S26&\"-\"&#REF!&\"-\"&T26&\"-\"&U26&\"-\"&V26&\"-\"&W26","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,3,16,140,25,null,null,"РА","А",25,6.3,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L27&\" \"&M27&\"-\"&#REF!&\"-\"&N27&\"-\"&O27&\"-\"&P27&\"-\"&#REF!&\"-\"&T27&\"-\"&U27&\"-\"&V27&\"-\"&W27","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L27&\" \"&M27&\"-\"&#REF!&\"-\"&N27&\"-\"&O27&\"-\"&S27&\"-\"&#REF!&\"-\"&T27&\"-\"&U27&\"-\"&V27&\"-\"&W27","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,3,16,140,25,null,null,"РА","А",25,6.3,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L28&\" \"&M28&\"-\"&#REF!&\"-\"&N28&\"-\"&O28&\"-\"&P28&\"-\"&#REF!&\"-\"&T28&\"-\"&U28&\"-\"&V28&\"-\"&W28","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L28&\" \"&M28&\"-\"&#REF!&\"-\"&N28&\"-\"&O28&\"-\"&S28&\"-\"&#REF!&\"-\"&T28&\"-\"&U28&\"-\"&V28&\"-\"&W28","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,4,16,140,25,null,null,"РА","А",25,6.3,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L29&\" \"&M29&\"-\"&#REF!&\"-\"&N29&\"-\"&O29&\"-\"&P29&\"-\"&#REF!&\"-\"&T29&\"-\"&U29&\"-\"&V29&\"-\"&W29","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L29&\" \"&M29&\"-\"&#REF!&\"-\"&N29&\"-\"&O29&\"-\"&S29&\"-\"&#REF!&\"-\"&T29&\"-\"&U29&\"-\"&V29&\"-\"&W29","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,4,16,140,25,null,null,"РА","А",25,6.3,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L30&\" \"&M30&\"-\"&#REF!&\"-\"&N30&\"-\"&O30&\"-\"&P30&\"-\"&#REF!&\"-\"&T30&\"-\"&U30&\"-\"&V30&\"-\"&W30","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L30&\" \"&M30&\"-\"&#REF!&\"-\"&N30&\"-\"&O30&\"-\"&S30&\"-\"&#REF!&\"-\"&T30&\"-\"&U30&\"-\"&V30&\"-\"&W30","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,1,16,140,32,null,null,"РА","А",32,10,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L31&\" \"&M31&\"-\"&#REF!&\"-\"&N31&\"-\"&O31&\"-\"&P31&\"-\"&#REF!&\"-\"&T31&\"-\"&U31&\"-\"&V31&\"-\"&W31","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L31&\" \"&M31&\"-\"&#REF!&\"-\"&N31&\"-\"&O31&\"-\"&S31&\"-\"&#REF!&\"-\"&T31&\"-\"&U31&\"-\"&V31&\"-\"&W31","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,1,16,140,32,null,null,"РА","А",32,10,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L32&\" \"&M32&\"-\"&#REF!&\"-\"&N32&\"-\"&O32&\"-\"&P32&\"-\"&#REF!&\"-\"&T32&\"-\"&U32&\"-\"&V32&\"-\"&W32","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L32&\" \"&M32&\"-\"&#REF!&\"-\"&N32&\"-\"&O32&\"-\"&S32&\"-\"&#REF!&\"-\"&T32&\"-\"&U32&\"-\"&V32&\"-\"&W32","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,2,16,140,32,null,null,"РА","А",32,10,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L33&\" \"&M33&\"-\"&#REF!&\"-\"&N33&\"-\"&O33&\"-\"&P33&\"-\"&#REF!&\"-\"&T33&\"-\"&U33&\"-\"&V33&\"-\"&W33","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L33&\" \"&M33&\"-\"&#REF!&\"-\"&N33&\"-\"&O33&\"-\"&S33&\"-\"&#REF!&\"-\"&T33&\"-\"&U33&\"-\"&V33&\"-\"&W33","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,2,16,140,32,null,null,"РА","А",32,10,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L34&\" \"&M34&\"-\"&#REF!&\"-\"&N34&\"-\"&O34&\"-\"&P34&\"-\"&#REF!&\"-\"&T34&\"-\"&U34&\"-\"&V34&\"-\"&W34","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L34&\" \"&M34&\"-\"&#REF!&\"-\"&N34&\"-\"&O34&\"-\"&S34&\"-\"&#REF!&\"-\"&T34&\"-\"&U34&\"-\"&V34&\"-\"&W34","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,3,16,140,32,null,null,"РА","А",32,10,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L35&\" \"&M35&\"-\"&#REF!&\"-\"&N35&\"-\"&O35&\"-\"&P35&\"-\"&#REF!&\"-\"&T35&\"-\"&U35&\"-\"&V35&\"-\"&W35","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L35&\" \"&M35&\"-\"&#REF!&\"-\"&N35&\"-\"&O35&\"-\"&S35&\"-\"&#REF!&\"-\"&T35&\"-\"&U35&\"-\"&V35&\"-\"&W35","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,3,16,140,32,null,null,"РА","А",32,10,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L36&\" \"&M36&\"-\"&#REF!&\"-\"&N36&\"-\"&O36&\"-\"&P36&\"-\"&#REF!&\"-\"&T36&\"-\"&U36&\"-\"&V36&\"-\"&W36","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L36&\" \"&M36&\"-\"&#REF!&\"-\"&N36&\"-\"&O36&\"-\"&S36&\"-\"&#REF!&\"-\"&T36&\"-\"&U36&\"-\"&V36&\"-\"&W36","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,4,16,140,32,null,null,"РА","А",32,10,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L37&\" \"&M37&\"-\"&#REF!&\"-\"&N37&\"-\"&O37&\"-\"&P37&\"-\"&#REF!&\"-\"&T37&\"-\"&U37&\"-\"&V37&\"-\"&W37","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L37&\" \"&M37&\"-\"&#REF!&\"-\"&N37&\"-\"&O37&\"-\"&S37&\"-\"&#REF!&\"-\"&T37&\"-\"&U37&\"-\"&V37&\"-\"&W37","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,4,16,140,32,null,null,"РА","А",32,10,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L38&\" \"&M38&\"-\"&#REF!&\"-\"&N38&\"-\"&O38&\"-\"&P38&\"-\"&#REF!&\"-\"&T38&\"-\"&U38&\"-\"&V38&\"-\"&W38","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L38&\" \"&M38&\"-\"&#REF!&\"-\"&N38&\"-\"&O38&\"-\"&S38&\"-\"&#REF!&\"-\"&T38&\"-\"&U38&\"-\"&V38&\"-\"&W38","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,1,16,140,40,null,null,"РА","А",40,16,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L39&\" \"&M39&\"-\"&#REF!&\"-\"&N39&\"-\"&O39&\"-\"&P39&\"-\"&#REF!&\"-\"&T39&\"-\"&U39&\"-\"&V39&\"-\"&W39","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L39&\" \"&M39&\"-\"&#REF!&\"-\"&N39&\"-\"&O39&\"-\"&S39&\"-\"&#REF!&\"-\"&T39&\"-\"&U39&\"-\"&V39&\"-\"&W39","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,1,16,140,40,null,null,"РА","А",40,16,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L40&\" \"&M40&\"-\"&#REF!&\"-\"&N40&\"-\"&O40&\"-\"&P40&\"-\"&#REF!&\"-\"&T40&\"-\"&U40&\"-\"&V40&\"-\"&W40","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L40&\" \"&M40&\"-\"&#REF!&\"-\"&N40&\"-\"&O40&\"-\"&S40&\"-\"&#REF!&\"-\"&T40&\"-\"&U40&\"-\"&V40&\"-\"&W40","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,2,16,140,40,null,null,"РА","А",40,16,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L41&\" \"&M41&\"-\"&#REF!&\"-\"&N41&\"-\"&O41&\"-\"&P41&\"-\"&#REF!&\"-\"&T41&\"-\"&U41&\"-\"&V41&\"-\"&W41","v":{"$error":"#REF!"}},null,null,1.6,{"$f":"L41&\" \"&M41&\"-\"&#REF!&\"-\"&N41&\"-\"&O41&\"-\"&S41&\"-\"&#REF!&\"-\"&T41&\"-\"&U41&\"-\"&V41&\"-\"&W41","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,2,16,140,40,null,null,"РА","А",40,16,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L42&\" \"&M42&\"-\"&#REF!&\"-\"&N42&\"-\"&O42&\"-\"&P42&\"-\"&#REF!&\"-\"&T42&\"-\"&U42&\"-\"&V42&\"-\"&W42","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L42&\" \"&M42&\"-\"&#REF!&\"-\"&N42&\"-\"&O42&\"-\"&S42&\"-\"&#REF!&\"-\"&T42&\"-\"&U42&\"-\"&V42&\"-\"&W42","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,3,16,140,40,null,null,"РА","А",40,16,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L43&\" \"&M43&\"-\"&#REF!&\"-\"&N43&\"-\"&O43&\"-\"&P43&\"-\"&#REF!&\"-\"&T43&\"-\"&U43&\"-\"&V43&\"-\"&W43","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L43&\" \"&M43&\"-\"&#REF!&\"-\"&N43&\"-\"&O43&\"-\"&S43&\"-\"&#REF!&\"-\"&T43&\"-\"&U43&\"-\"&V43&\"-\"&W43","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,3,16,140,40,null,null,"РА","А",40,16,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L44&\" \"&M44&\"-\"&#REF!&\"-\"&N44&\"-\"&O44&\"-\"&P44&\"-\"&#REF!&\"-\"&T44&\"-\"&U44&\"-\"&V44&\"-\"&W44","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L44&\" \"&M44&\"-\"&#REF!&\"-\"&N44&\"-\"&O44&\"-\"&S44&\"-\"&#REF!&\"-\"&T44&\"-\"&U44&\"-\"&V44&\"-\"&W44","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,4,16,140,40,null,null,"РА","А",40,16,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L45&\" \"&M45&\"-\"&#REF!&\"-\"&N45&\"-\"&O45&\"-\"&P45&\"-\"&#REF!&\"-\"&T45&\"-\"&U45&\"-\"&V45&\"-\"&W45","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L45&\" \"&M45&\"-\"&#REF!&\"-\"&N45&\"-\"&O45&\"-\"&S45&\"-\"&#REF!&\"-\"&T45&\"-\"&U45&\"-\"&V45&\"-\"&W45","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,4,16,140,40,null,null,"РА","А",40,16,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L46&\" \"&M46&\"-\"&#REF!&\"-\"&N46&\"-\"&O46&\"-\"&P46&\"-\"&#REF!&\"-\"&T46&\"-\"&U46&\"-\"&V46&\"-\"&W46","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L46&\" \"&M46&\"-\"&#REF!&\"-\"&N46&\"-\"&O46&\"-\"&S46&\"-\"&#REF!&\"-\"&T46&\"-\"&U46&\"-\"&V46&\"-\"&W46","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,1,16,140,50,null,null,"РА","А",50,25,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L47&\" \"&M47&\"-\"&#REF!&\"-\"&N47&\"-\"&O47&\"-\"&P47&\"-\"&#REF!&\"-\"&T47&\"-\"&U47&\"-\"&V47&\"-\"&W47","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L47&\" \"&M47&\"-\"&#REF!&\"-\"&N47&\"-\"&O47&\"-\"&S47&\"-\"&#REF!&\"-\"&T47&\"-\"&U47&\"-\"&V47&\"-\"&W47","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,1,16,140,50,null,null,"РА","А",50,25,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L48&\" \"&M48&\"-\"&#REF!&\"-\"&N48&\"-\"&O48&\"-\"&P48&\"-\"&#REF!&\"-\"&T48&\"-\"&U48&\"-\"&V48&\"-\"&W48","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L48&\" \"&M48&\"-\"&#REF!&\"-\"&N48&\"-\"&O48&\"-\"&S48&\"-\"&#REF!&\"-\"&T48&\"-\"&U48&\"-\"&V48&\"-\"&W48","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,2,16,140,50,null,null,"РА","А",50,25,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L49&\" \"&M49&\"-\"&#REF!&\"-\"&N49&\"-\"&O49&\"-\"&P49&\"-\"&#REF!&\"-\"&T49&\"-\"&U49&\"-\"&V49&\"-\"&W49","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L49&\" \"&M49&\"-\"&#REF!&\"-\"&N49&\"-\"&O49&\"-\"&S49&\"-\"&#REF!&\"-\"&T49&\"-\"&U49&\"-\"&V49&\"-\"&W49","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,2,16,140,50,null,null,"РА","А",50,25,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L50&\" \"&M50&\"-\"&#REF!&\"-\"&N50&\"-\"&O50&\"-\"&P50&\"-\"&#REF!&\"-\"&T50&\"-\"&U50&\"-\"&V50&\"-\"&W50","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L50&\" \"&M50&\"-\"&#REF!&\"-\"&N50&\"-\"&O50&\"-\"&S50&\"-\"&#REF!&\"-\"&T50&\"-\"&U50&\"-\"&V50&\"-\"&W50","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,3,16,140,50,null,null,"РА","А",50,25,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L51&\" \"&M51&\"-\"&#REF!&\"-\"&N51&\"-\"&O51&\"-\"&P51&\"-\"&#REF!&\"-\"&T51&\"-\"&U51&\"-\"&V51&\"-\"&W51","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L51&\" \"&M51&\"-\"&#REF!&\"-\"&N51&\"-\"&O51&\"-\"&S51&\"-\"&#REF!&\"-\"&T51&\"-\"&U51&\"-\"&V51&\"-\"&W51","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,3,16,140,50,null,null,"РА","А",50,25,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L52&\" \"&M52&\"-\"&#REF!&\"-\"&N52&\"-\"&O52&\"-\"&P52&\"-\"&#REF!&\"-\"&T52&\"-\"&U52&\"-\"&V52&\"-\"&W52","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L52&\" \"&M52&\"-\"&#REF!&\"-\"&N52&\"-\"&O52&\"-\"&S52&\"-\"&#REF!&\"-\"&T52&\"-\"&U52&\"-\"&V52&\"-\"&W52","v":{"$error":"#REF!"}}]
["RD",103,"V",3,null,4,16,140,50,null,null,"РА","А",50,25,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L53&\" \"&M53&\"-\"&#REF!&\"-\"&N53&\"-\"&O53&\"-\"&P53&\"-\"&#REF!&\"-\"&T53&\"-\"&U53&\"-\"&V53&\"-\"&W53","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L53&\" \"&M53&\"-\"&#REF!&\"-\"&N53&\"-\"&O53&\"-\"&S53&\"-\"&#REF!&\"-\"&T53&\"-\"&U53&\"-\"&V53&\"-\"&W53","v":{"$error":"#REF!"}}]
["RD",103,"V",null,4,4,16,140,50,null,null,"РА","А",50,25,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L54&\" \"&M54&\"-\"&#REF!&\"-\"&N54&\"-\"&O54&\"-\"&P54&\"-\"&#REF!&\"-\"&T54&\"-\"&U54&\"-\"&V54&\"-\"&W54","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L54&\" \"&M54&\"-\"&#REF!&\"-\"&N54&\"-\"&O54&\"-\"&S54&\"-\"&#REF!&\"-\"&T54&\"-\"&U54&\"-\"&V54&\"-\"&W54","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,1,16,140,15,null,null,"РА","М",15,2.5,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L55&\" \"&M55&\"-\"&#REF!&\"-\"&N55&\"-\"&O55&\"-\"&P55&\"-\"&#REF!&\"-\"&T55&\"-\"&U55&\"-\"&V55&\"-\"&W55","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L55&\" \"&M55&\"-\"&#REF!&\"-\"&N55&\"-\"&O55&\"-\"&S55&\"-\"&#REF!&\"-\"&T55&\"-\"&U55&\"-\"&V55&\"-\"&W55","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,1,16,140,15,null,null,"РА","М",15,2.5,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L56&\" \"&M56&\"-\"&#REF!&\"-\"&N56&\"-\"&O56&\"-\"&P56&\"-\"&#REF!&\"-\"&T56&\"-\"&U56&\"-\"&V56&\"-\"&W56","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L56&\" \"&M56&\"-\"&#REF!&\"-\"&N56&\"-\"&O56&\"-\"&S56&\"-\"&#REF!&\"-\"&T56&\"-\"&U56&\"-\"&V56&\"-\"&W56","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,2,16,140,15,null,null,"РА","М",15,2.5,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L57&\" \"&M57&\"-\"&#REF!&\"-\"&N57&\"-\"&O57&\"-\"&P57&\"-\"&#REF!&\"-\"&T57&\"-\"&U57&\"-\"&V57&\"-\"&W57","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L57&\" \"&M57&\"-\"&#REF!&\"-\"&N57&\"-\"&O57&\"-\"&S57&\"-\"&#REF!&\"-\"&T57&\"-\"&U57&\"-\"&V57&\"-\"&W57","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,2,16,140,15,null,null,"РА","М",15,2.5,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L58&\" \"&M58&\"-\"&#REF!&\"-\"&N58&\"-\"&O58&\"-\"&P58&\"-\"&#REF!&\"-\"&T58&\"-\"&U58&\"-\"&V58&\"-\"&W58","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L58&\" \"&M58&\"-\"&#REF!&\"-\"&N58&\"-\"&O58&\"-\"&S58&\"-\"&#REF!&\"-\"&T58&\"-\"&U58&\"-\"&V58&\"-\"&W58","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,3,16,140,15,null,null,"РА","М",15,2.5,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L59&\" \"&M59&\"-\"&#REF!&\"-\"&N59&\"-\"&O59&\"-\"&P59&\"-\"&#REF!&\"-\"&T59&\"-\"&U59&\"-\"&V59&\"-\"&W59","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L59&\" \"&M59&\"-\"&#REF!&\"-\"&N59&\"-\"&O59&\"-\"&S59&\"-\"&#REF!&\"-\"&T59&\"-\"&U59&\"-\"&V59&\"-\"&W59","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,3,16,140,15,null,null,"РА","М",15,2.5,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L60&\" \"&M60&\"-\"&#REF!&\"-\"&N60&\"-\"&O60&\"-\"&P60&\"-\"&#REF!&\"-\"&T60&\"-\"&U60&\"-\"&V60&\"-\"&W60","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L60&\" \"&M60&\"-\"&#REF!&\"-\"&N60&\"-\"&O60&\"-\"&S60&\"-\"&#REF!&\"-\"&T60&\"-\"&U60&\"-\"&V60&\"-\"&W60","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,4,16,140,15,null,null,"РА","М",15,2.5,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L61&\" \"&M61&\"-\"&#REF!&\"-\"&N61&\"-\"&O61&\"-\"&P61&\"-\"&#REF!&\"-\"&T61&\"-\"&U61&\"-\"&V61&\"-\"&W61","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L61&\" \"&M61&\"-\"&#REF!&\"-\"&N61&\"-\"&O61&\"-\"&S61&\"-\"&#REF!&\"-\"&T61&\"-\"&U61&\"-\"&V61&\"-\"&W61","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,4,16,140,15,null,null,"РА","М",15,2.5,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L62&\" \"&M62&\"-\"&#REF!&\"-\"&N62&\"-\"&O62&\"-\"&P62&\"-\"&#REF!&\"-\"&T62&\"-\"&U62&\"-\"&V62&\"-\"&W62","v":{"$error":"#REF!"}},null,null,1.2,{"$f":"L62&\" \"&M62&\"-\"&#REF!&\"-\"&N62&\"-\"&O62&\"-\"&S62&\"-\"&#REF!&\"-\"&T62&\"-\"&U62&\"-\"&V62&\"-\"&W62","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,1,16,140,20,null,null,"РА","М",20,4,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L63&\" \"&M63&\"-\"&#REF!&\"-\"&N63&\"-\"&O63&\"-\"&P63&\"-\"&#REF!&\"-\"&T63&\"-\"&U63&\"-\"&V63&\"-\"&W63","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L63&\" \"&M63&\"-\"&#REF!&\"-\"&N63&\"-\"&O63&\"-\"&S63&\"-\"&#REF!&\"-\"&T63&\"-\"&U63&\"-\"&V63&\"-\"&W63","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,1,16,140,20,null,null,"РА","М",20,4,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L64&\" \"&M64&\"-\"&#REF!&\"-\"&N64&\"-\"&O64&\"-\"&P64&\"-\"&#REF!&\"-\"&T64&\"-\"&U64&\"-\"&V64&\"-\"&W64","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L64&\" \"&M64&\"-\"&#REF!&\"-\"&N64&\"-\"&O64&\"-\"&S64&\"-\"&#REF!&\"-\"&T64&\"-\"&U64&\"-\"&V64&\"-\"&W64","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,2,16,140,20,null,null,"РА","М",20,4,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L65&\" \"&M65&\"-\"&#REF!&\"-\"&N65&\"-\"&O65&\"-\"&P65&\"-\"&#REF!&\"-\"&T65&\"-\"&U65&\"-\"&V65&\"-\"&W65","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L65&\" \"&M65&\"-\"&#REF!&\"-\"&N65&\"-\"&O65&\"-\"&S65&\"-\"&#REF!&\"-\"&T65&\"-\"&U65&\"-\"&V65&\"-\"&W65","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,2,16,140,20,null,null,"РА","М",20,4,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L66&\" \"&M66&\"-\"&#REF!&\"-\"&N66&\"-\"&O66&\"-\"&P66&\"-\"&#REF!&\"-\"&T66&\"-\"&U66&\"-\"&V66&\"-\"&W66","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L66&\" \"&M66&\"-\"&#REF!&\"-\"&N66&\"-\"&O66&\"-\"&S66&\"-\"&#REF!&\"-\"&T66&\"-\"&U66&\"-\"&V66&\"-\"&W66","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,3,16,140,20,null,null,"РА","М",20,4,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L67&\" \"&M67&\"-\"&#REF!&\"-\"&N67&\"-\"&O67&\"-\"&P67&\"-\"&#REF!&\"-\"&T67&\"-\"&U67&\"-\"&V67&\"-\"&W67","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L67&\" \"&M67&\"-\"&#REF!&\"-\"&N67&\"-\"&O67&\"-\"&S67&\"-\"&#REF!&\"-\"&T67&\"-\"&U67&\"-\"&V67&\"-\"&W67","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,3,16,140,20,null,null,"РА","М",20,4,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L68&\" \"&M68&\"-\"&#REF!&\"-\"&N68&\"-\"&O68&\"-\"&P68&\"-\"&#REF!&\"-\"&T68&\"-\"&U68&\"-\"&V68&\"-\"&W68","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L68&\" \"&M68&\"-\"&#REF!&\"-\"&N68&\"-\"&O68&\"-\"&S68&\"-\"&#REF!&\"-\"&T68&\"-\"&U68&\"-\"&V68&\"-\"&W68","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,4,16,140,20,null,null,"РА","М",20,4,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L69&\" \"&M69&\"-\"&#REF!&\"-\"&N69&\"-\"&O69&\"-\"&P69&\"-\"&#REF!&\"-\"&T69&\"-\"&U69&\"-\"&V69&\"-\"&W69","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L69&\" \"&M69&\"-\"&#REF!&\"-\"&N69&\"-\"&O69&\"-\"&S69&\"-\"&#REF!&\"-\"&T69&\"-\"&U69&\"-\"&V69&\"-\"&W69","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,4,16,140,20,null,null,"РА","М",20,4,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L70&\" \"&M70&\"-\"&#REF!&\"-\"&N70&\"-\"&O70&\"-\"&P70&\"-\"&#REF!&\"-\"&T70&\"-\"&U70&\"-\"&V70&\"-\"&W70","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L70&\" \"&M70&\"-\"&#REF!&\"-\"&N70&\"-\"&O70&\"-\"&S70&\"-\"&#REF!&\"-\"&T70&\"-\"&U70&\"-\"&V70&\"-\"&W70","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,1,16,140,25,null,null,"РА","М",25,6.3,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L71&\" \"&M71&\"-\"&#REF!&\"-\"&N71&\"-\"&O71&\"-\"&P71&\"-\"&#REF!&\"-\"&T71&\"-\"&U71&\"-\"&V71&\"-\"&W71","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L71&\" \"&M71&\"-\"&#REF!&\"-\"&N71&\"-\"&O71&\"-\"&S71&\"-\"&#REF!&\"-\"&T71&\"-\"&U71&\"-\"&V71&\"-\"&W71","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,1,16,140,25,null,null,"РА","М",25,6.3,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L72&\" \"&M72&\"-\"&#REF!&\"-\"&N72&\"-\"&O72&\"-\"&P72&\"-\"&#REF!&\"-\"&T72&\"-\"&U72&\"-\"&V72&\"-\"&W72","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L72&\" \"&M72&\"-\"&#REF!&\"-\"&N72&\"-\"&O72&\"-\"&S72&\"-\"&#REF!&\"-\"&T72&\"-\"&U72&\"-\"&V72&\"-\"&W72","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,2,16,140,25,null,null,"РА","М",25,6.3,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L73&\" \"&M73&\"-\"&#REF!&\"-\"&N73&\"-\"&O73&\"-\"&P73&\"-\"&#REF!&\"-\"&T73&\"-\"&U73&\"-\"&V73&\"-\"&W73","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L73&\" \"&M73&\"-\"&#REF!&\"-\"&N73&\"-\"&O73&\"-\"&S73&\"-\"&#REF!&\"-\"&T73&\"-\"&U73&\"-\"&V73&\"-\"&W73","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,2,16,140,25,null,null,"РА","М",25,6.3,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L74&\" \"&M74&\"-\"&#REF!&\"-\"&N74&\"-\"&O74&\"-\"&P74&\"-\"&#REF!&\"-\"&T74&\"-\"&U74&\"-\"&V74&\"-\"&W74","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L74&\" \"&M74&\"-\"&#REF!&\"-\"&N74&\"-\"&O74&\"-\"&S74&\"-\"&#REF!&\"-\"&T74&\"-\"&U74&\"-\"&V74&\"-\"&W74","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,3,16,140,25,null,null,"РА","М",25,6.3,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L75&\" \"&M75&\"-\"&#REF!&\"-\"&N75&\"-\"&O75&\"-\"&P75&\"-\"&#REF!&\"-\"&T75&\"-\"&U75&\"-\"&V75&\"-\"&W75","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L75&\" \"&M75&\"-\"&#REF!&\"-\"&N75&\"-\"&O75&\"-\"&S75&\"-\"&#REF!&\"-\"&T75&\"-\"&U75&\"-\"&V75&\"-\"&W75","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,3,16,140,25,null,null,"РА","М",25,6.3,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L76&\" \"&M76&\"-\"&#REF!&\"-\"&N76&\"-\"&O76&\"-\"&P76&\"-\"&#REF!&\"-\"&T76&\"-\"&U76&\"-\"&V76&\"-\"&W76","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L76&\" \"&M76&\"-\"&#REF!&\"-\"&N76&\"-\"&O76&\"-\"&S76&\"-\"&#REF!&\"-\"&T76&\"-\"&U76&\"-\"&V76&\"-\"&W76","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,4,16,140,25,null,null,"РА","М",25,6.3,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L77&\" \"&M77&\"-\"&#REF!&\"-\"&N77&\"-\"&O77&\"-\"&P77&\"-\"&#REF!&\"-\"&T77&\"-\"&U77&\"-\"&V77&\"-\"&W77","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L77&\" \"&M77&\"-\"&#REF!&\"-\"&N77&\"-\"&O77&\"-\"&S77&\"-\"&#REF!&\"-\"&T77&\"-\"&U77&\"-\"&V77&\"-\"&W77","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,4,16,140,25,null,null,"РА","М",25,6.3,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L78&\" \"&M78&\"-\"&#REF!&\"-\"&N78&\"-\"&O78&\"-\"&P78&\"-\"&#REF!&\"-\"&T78&\"-\"&U78&\"-\"&V78&\"-\"&W78","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L78&\" \"&M78&\"-\"&#REF!&\"-\"&N78&\"-\"&O78&\"-\"&S78&\"-\"&#REF!&\"-\"&T78&\"-\"&U78&\"-\"&V78&\"-\"&W78","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,1,16,140,32,null,null,"РА","М",32,10,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L79&\" \"&M79&\"-\"&#REF!&\"-\"&N79&\"-\"&O79&\"-\"&P79&\"-\"&#REF!&\"-\"&T79&\"-\"&U79&\"-\"&V79&\"-\"&W79","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L79&\" \"&M79&\"-\"&#REF!&\"-\"&N79&\"-\"&O79&\"-\"&S79&\"-\"&#REF!&\"-\"&T79&\"-\"&U79&\"-\"&V79&\"-\"&W79","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,1,16,140,32,null,null,"РА","М",32,10,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L80&\" \"&M80&\"-\"&#REF!&\"-\"&N80&\"-\"&O80&\"-\"&P80&\"-\"&#REF!&\"-\"&T80&\"-\"&U80&\"-\"&V80&\"-\"&W80","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L80&\" \"&M80&\"-\"&#REF!&\"-\"&N80&\"-\"&O80&\"-\"&S80&\"-\"&#REF!&\"-\"&T80&\"-\"&U80&\"-\"&V80&\"-\"&W80","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,2,16,140,32,null,null,"РА","М",32,10,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L81&\" \"&M81&\"-\"&#REF!&\"-\"&N81&\"-\"&O81&\"-\"&P81&\"-\"&#REF!&\"-\"&T81&\"-\"&U81&\"-\"&V81&\"-\"&W81","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L81&\" \"&M81&\"-\"&#REF!&\"-\"&N81&\"-\"&O81&\"-\"&S81&\"-\"&#REF!&\"-\"&T81&\"-\"&U81&\"-\"&V81&\"-\"&W81","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,2,16,140,32,null,null,"РА","М",32,10,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L82&\" \"&M82&\"-\"&#REF!&\"-\"&N82&\"-\"&O82&\"-\"&P82&\"-\"&#REF!&\"-\"&T82&\"-\"&U82&\"-\"&V82&\"-\"&W82","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L82&\" \"&M82&\"-\"&#REF!&\"-\"&N82&\"-\"&O82&\"-\"&S82&\"-\"&#REF!&\"-\"&T82&\"-\"&U82&\"-\"&V82&\"-\"&W82","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,3,16,140,32,null,null,"РА","М",32,10,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L83&\" \"&M83&\"-\"&#REF!&\"-\"&N83&\"-\"&O83&\"-\"&P83&\"-\"&#REF!&\"-\"&T83&\"-\"&U83&\"-\"&V83&\"-\"&W83","v":{"$error":"#REF!"}},null,null,0.74,{"$f":"L83&\" \"&M83&\"-\"&#REF!&\"-\"&N83&\"-\"&O83&\"-\"&S83&\"-\"&#REF!&\"-\"&T83&\"-\"&U83&\"-\"&V83&\"-\"&W83","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,3,16,140,32,null,null,"РА","М",32,10,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L84&\" \"&M84&\"-\"&#REF!&\"-\"&N84&\"-\"&O84&\"-\"&P84&\"-\"&#REF!&\"-\"&T84&\"-\"&U84&\"-\"&V84&\"-\"&W84","v":{"$error":"#REF!"}},{"$f":"L84&\" \"&M84&\"-\"&#REF!&\"-\"&N84&\"-\"&O84&\"-\"&Q84&\"-\"&#REF!&\"-\"&T84&\"-\"&U84&\"-\"&V84&\"-\"&W84","v":{"$error":"#REF!"}},null,0.68,{"$f":"L84&\" \"&M84&\"-\"&#REF!&\"-\"&N84&\"-\"&O84&\"-\"&S84&\"-\"&#REF!&\"-\"&T84&\"-\"&U84&\"-\"&V84&\"-\"&W84","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,4,16,140,32,null,null,"РА","М",32,10,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L85&\" \"&M85&\"-\"&#REF!&\"-\"&N85&\"-\"&O85&\"-\"&P85&\"-\"&#REF!&\"-\"&T85&\"-\"&U85&\"-\"&V85&\"-\"&W85","v":{"$error":"#REF!"}},{"$f":"L85&\" \"&M85&\"-\"&#REF!&\"-\"&N85&\"-\"&O85&\"-\"&Q85&\"-\"&#REF!&\"-\"&T85&\"-\"&U85&\"-\"&V85&\"-\"&W85","v":{"$error":"#REF!"}},null,0.68,{"$f":"L85&\" \"&M85&\"-\"&#REF!&\"-\"&N85&\"-\"&O85&\"-\"&S85&\"-\"&#REF!&\"-\"&T85&\"-\"&U85&\"-\"&V85&\"-\"&W85","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,4,16,140,32,null,null,"РА","М",32,10,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L86&\" \"&M86&\"-\"&#REF!&\"-\"&N86&\"-\"&O86&\"-\"&P86&\"-\"&#REF!&\"-\"&T86&\"-\"&U86&\"-\"&V86&\"-\"&W86","v":{"$error":"#REF!"}},{"$f":"L86&\" \"&M86&\"-\"&#REF!&\"-\"&N86&\"-\"&O86&\"-\"&Q86&\"-\"&#REF!&\"-\"&T86&\"-\"&U86&\"-\"&V86&\"-\"&W86","v":{"$error":"#REF!"}},null,0.68,{"$f":"L86&\" \"&M86&\"-\"&#REF!&\"-\"&N86&\"-\"&O86&\"-\"&S86&\"-\"&#REF!&\"-\"&T86&\"-\"&U86&\"-\"&V86&\"-\"&W86","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,1,16,140,40,null,null,"РА","М",40,16,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L87&\" \"&M87&\"-\"&#REF!&\"-\"&N87&\"-\"&O87&\"-\"&P87&\"-\"&#REF!&\"-\"&T87&\"-\"&U87&\"-\"&V87&\"-\"&W87","v":{"$error":"#REF!"}},{"$f":"L87&\" \"&M87&\"-\"&#REF!&\"-\"&N87&\"-\"&O87&\"-\"&Q87&\"-\"&#REF!&\"-\"&T87&\"-\"&U87&\"-\"&V87&\"-\"&W87","v":{"$error":"#REF!"}},null,0.68,{"$f":"L87&\" \"&M87&\"-\"&#REF!&\"-\"&N87&\"-\"&O87&\"-\"&S87&\"-\"&#REF!&\"-\"&T87&\"-\"&U87&\"-\"&V87&\"-\"&W87","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,1,16,140,40,null,null,"РА","М",40,16,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L88&\" \"&M88&\"-\"&#REF!&\"-\"&N88&\"-\"&O88&\"-\"&P88&\"-\"&#REF!&\"-\"&T88&\"-\"&U88&\"-\"&V88&\"-\"&W88","v":{"$error":"#REF!"}},{"$f":"L88&\" \"&M88&\"-\"&#REF!&\"-\"&N88&\"-\"&O88&\"-\"&Q88&\"-\"&#REF!&\"-\"&T88&\"-\"&U88&\"-\"&V88&\"-\"&W88","v":{"$error":"#REF!"}},null,0.68,{"$f":"L88&\" \"&M88&\"-\"&#REF!&\"-\"&N88&\"-\"&O88&\"-\"&S88&\"-\"&#REF!&\"-\"&T88&\"-\"&U88&\"-\"&V88&\"-\"&W88","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,2,16,140,40,null,null,"РА","М",40,16,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L89&\" \"&M89&\"-\"&#REF!&\"-\"&N89&\"-\"&O89&\"-\"&P89&\"-\"&#REF!&\"-\"&T89&\"-\"&U89&\"-\"&V89&\"-\"&W89","v":{"$error":"#REF!"}},{"$f":"L89&\" \"&M89&\"-\"&#REF!&\"-\"&N89&\"-\"&O89&\"-\"&Q89&\"-\"&#REF!&\"-\"&T89&\"-\"&U89&\"-\"&V89&\"-\"&W89","v":{"$error":"#REF!"}},null,0.68,{"$f":"L89&\" \"&M89&\"-\"&#REF!&\"-\"&N89&\"-\"&O89&\"-\"&S89&\"-\"&#REF!&\"-\"&T89&\"-\"&U89&\"-\"&V89&\"-\"&W89","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,2,16,140,40,null,null,"РА","М",40,16,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L90&\" \"&M90&\"-\"&#REF!&\"-\"&N90&\"-\"&O90&\"-\"&P90&\"-\"&#REF!&\"-\"&T90&\"-\"&U90&\"-\"&V90&\"-\"&W90","v":{"$error":"#REF!"}},{"$f":"L90&\" \"&M90&\"-\"&#REF!&\"-\"&N90&\"-\"&O90&\"-\"&Q90&\"-\"&#REF!&\"-\"&T90&\"-\"&U90&\"-\"&V90&\"-\"&W90","v":{"$error":"#REF!"}},null,0.68,{"$f":"L90&\" \"&M90&\"-\"&#REF!&\"-\"&N90&\"-\"&O90&\"-\"&S90&\"-\"&#REF!&\"-\"&T90&\"-\"&U90&\"-\"&V90&\"-\"&W90","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,3,16,140,40,null,null,"РА","М",40,16,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L91&\" \"&M91&\"-\"&#REF!&\"-\"&N91&\"-\"&O91&\"-\"&P91&\"-\"&#REF!&\"-\"&T91&\"-\"&U91&\"-\"&V91&\"-\"&W91","v":{"$error":"#REF!"}},{"$f":"L91&\" \"&M91&\"-\"&#REF!&\"-\"&N91&\"-\"&O91&\"-\"&Q91&\"-\"&#REF!&\"-\"&T91&\"-\"&U91&\"-\"&V91&\"-\"&W91","v":{"$error":"#REF!"}},null,0.68,{"$f":"L91&\" \"&M91&\"-\"&#REF!&\"-\"&N91&\"-\"&O91&\"-\"&S91&\"-\"&#REF!&\"-\"&T91&\"-\"&U91&\"-\"&V91&\"-\"&W91","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,3,16,140,40,null,null,"РА","М",40,16,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L92&\" \"&M92&\"-\"&#REF!&\"-\"&N92&\"-\"&O92&\"-\"&P92&\"-\"&#REF!&\"-\"&T92&\"-\"&U92&\"-\"&V92&\"-\"&W92","v":{"$error":"#REF!"}},{"$f":"L92&\" \"&M92&\"-\"&#REF!&\"-\"&N92&\"-\"&O92&\"-\"&Q92&\"-\"&#REF!&\"-\"&T92&\"-\"&U92&\"-\"&V92&\"-\"&W92","v":{"$error":"#REF!"}},null,0.68,{"$f":"L92&\" \"&M92&\"-\"&#REF!&\"-\"&N92&\"-\"&O92&\"-\"&S92&\"-\"&#REF!&\"-\"&T92&\"-\"&U92&\"-\"&V92&\"-\"&W92","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,4,16,140,40,null,null,"РА","М",40,16,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L93&\" \"&M93&\"-\"&#REF!&\"-\"&N93&\"-\"&O93&\"-\"&P93&\"-\"&#REF!&\"-\"&T93&\"-\"&U93&\"-\"&V93&\"-\"&W93","v":{"$error":"#REF!"}},{"$f":"L93&\" \"&M93&\"-\"&#REF!&\"-\"&N93&\"-\"&O93&\"-\"&Q93&\"-\"&#REF!&\"-\"&T93&\"-\"&U93&\"-\"&V93&\"-\"&W93","v":{"$error":"#REF!"}},null,0.68,{"$f":"L93&\" \"&M93&\"-\"&#REF!&\"-\"&N93&\"-\"&O93&\"-\"&S93&\"-\"&#REF!&\"-\"&T93&\"-\"&U93&\"-\"&V93&\"-\"&W93","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,4,16,140,40,null,null,"РА","М",40,16,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L94&\" \"&M94&\"-\"&#REF!&\"-\"&N94&\"-\"&O94&\"-\"&P94&\"-\"&#REF!&\"-\"&T94&\"-\"&U94&\"-\"&V94&\"-\"&W94","v":{"$error":"#REF!"}},{"$f":"L94&\" \"&M94&\"-\"&#REF!&\"-\"&N94&\"-\"&O94&\"-\"&Q94&\"-\"&#REF!&\"-\"&T94&\"-\"&U94&\"-\"&V94&\"-\"&W94","v":{"$error":"#REF!"}},null,0.68,{"$f":"L94&\" \"&M94&\"-\"&#REF!&\"-\"&N94&\"-\"&O94&\"-\"&S94&\"-\"&#REF!&\"-\"&T94&\"-\"&U94&\"-\"&V94&\"-\"&W94","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,1,16,140,50,null,null,"РА","М",50,25,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L95&\" \"&M95&\"-\"&#REF!&\"-\"&N95&\"-\"&O95&\"-\"&P95&\"-\"&#REF!&\"-\"&T95&\"-\"&U95&\"-\"&V95&\"-\"&W95","v":{"$error":"#REF!"}},{"$f":"L95&\" \"&M95&\"-\"&#REF!&\"-\"&N95&\"-\"&O95&\"-\"&Q95&\"-\"&#REF!&\"-\"&T95&\"-\"&U95&\"-\"&V95&\"-\"&W95","v":{"$error":"#REF!"}},null,0.68,{"$f":"L95&\" \"&M95&\"-\"&#REF!&\"-\"&N95&\"-\"&O95&\"-\"&S95&\"-\"&#REF!&\"-\"&T95&\"-\"&U95&\"-\"&V95&\"-\"&W95","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,1,16,140,50,null,null,"РА","М",50,25,"0",null,null,null,1.6,1,150,"У1",null,null,{"$f":"L96&\" \"&M96&\"-\"&#REF!&\"-\"&N96&\"-\"&O96&\"-\"&P96&\"-\"&#REF!&\"-\"&T96&\"-\"&U96&\"-\"&V96&\"-\"&W96","v":{"$error":"#REF!"}},{"$f":"L96&\" \"&M96&\"-\"&#REF!&\"-\"&N96&\"-\"&O96&\"-\"&Q96&\"-\"&#REF!&\"-\"&T96&\"-\"&U96&\"-\"&V96&\"-\"&W96","v":{"$error":"#REF!"}},null,0.68,{"$f":"L96&\" \"&M96&\"-\"&#REF!&\"-\"&N96&\"-\"&O96&\"-\"&S96&\"-\"&#REF!&\"-\"&T96&\"-\"&U96&\"-\"&V96&\"-\"&W96","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,2,16,140,50,null,null,"РА","М",50,25,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L97&\" \"&M97&\"-\"&#REF!&\"-\"&N97&\"-\"&O97&\"-\"&P97&\"-\"&#REF!&\"-\"&T97&\"-\"&U97&\"-\"&V97&\"-\"&W97","v":{"$error":"#REF!"}},{"$f":"L97&\" \"&M97&\"-\"&#REF!&\"-\"&N97&\"-\"&O97&\"-\"&Q97&\"-\"&#REF!&\"-\"&T97&\"-\"&U97&\"-\"&V97&\"-\"&W97","v":{"$error":"#REF!"}},null,0.68,{"$f":"L97&\" \"&M97&\"-\"&#REF!&\"-\"&N97&\"-\"&O97&\"-\"&S97&\"-\"&#REF!&\"-\"&T97&\"-\"&U97&\"-\"&V97&\"-\"&W97","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,2,16,140,50,null,null,"РА","М",50,25,null,"1",null,null,1.6,1,150,"У1",null,null,{"$f":"L98&\" \"&M98&\"-\"&#REF!&\"-\"&N98&\"-\"&O98&\"-\"&P98&\"-\"&#REF!&\"-\"&T98&\"-\"&U98&\"-\"&V98&\"-\"&W98","v":{"$error":"#REF!"}},{"$f":"L98&\" \"&M98&\"-\"&#REF!&\"-\"&N98&\"-\"&O98&\"-\"&Q98&\"-\"&#REF!&\"-\"&T98&\"-\"&U98&\"-\"&V98&\"-\"&W98","v":{"$error":"#REF!"}},null,0.68,{"$f":"L98&\" \"&M98&\"-\"&#REF!&\"-\"&N98&\"-\"&O98&\"-\"&S98&\"-\"&#REF!&\"-\"&T98&\"-\"&U98&\"-\"&V98&\"-\"&W98","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,3,16,140,50,null,null,"РА","М",50,25,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L99&\" \"&M99&\"-\"&#REF!&\"-\"&N99&\"-\"&O99&\"-\"&P99&\"-\"&#REF!&\"-\"&T99&\"-\"&U99&\"-\"&V99&\"-\"&W99","v":{"$error":"#REF!"}},{"$f":"L99&\" \"&M99&\"-\"&#REF!&\"-\"&N99&\"-\"&O99&\"-\"&Q99&\"-\"&#REF!&\"-\"&T99&\"-\"&U99&\"-\"&V99&\"-\"&W99","v":{"$error":"#REF!"}},null,0.68,{"$f":"L99&\" \"&M99&\"-\"&#REF!&\"-\"&N99&\"-\"&O99&\"-\"&S99&\"-\"&#REF!&\"-\"&T99&\"-\"&U99&\"-\"&V99&\"-\"&W99","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,3,16,140,50,null,null,"РА","М",50,25,null,null,"2",null,1.6,1,150,"У1",null,null,{"$f":"L100&\" \"&M100&\"-\"&#REF!&\"-\"&N100&\"-\"&O100&\"-\"&P100&\"-\"&#REF!&\"-\"&T100&\"-\"&U100&\"-\"&V100&\"-\"&W100","v":{"$error":"#REF!"}},{"$f":"L100&\" \"&M100&\"-\"&#REF!&\"-\"&N100&\"-\"&O100&\"-\"&Q100&\"-\"&#REF!&\"-\"&T100&\"-\"&U100&\"-\"&V100&\"-\"&W100","v":{"$error":"#REF!"}},null,0.68,{"$f":"L100&\" \"&M100&\"-\"&#REF!&\"-\"&N100&\"-\"&O100&\"-\"&S100&\"-\"&#REF!&\"-\"&T100&\"-\"&U100&\"-\"&V100&\"-\"&W100","v":{"$error":"#REF!"}}]
["RD",103,"D",3,null,4,16,140,50,null,null,"РА","М",50,25,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L101&\" \"&M101&\"-\"&#REF!&\"-\"&N101&\"-\"&O101&\"-\"&P101&\"-\"&#REF!&\"-\"&T101&\"-\"&U101&\"-\"&V101&\"-\"&W101","v":{"$error":"#REF!"}},{"$f":"L101&\" \"&M101&\"-\"&#REF!&\"-\"&N101&\"-\"&O101&\"-\"&Q101&\"-\"&#REF!&\"-\"&T101&\"-\"&U101&\"-\"&V101&\"-\"&W101","v":{"$error":"#REF!"}},null,0.68,{"$f":"L101&\" \"&M101&\"-\"&#REF!&\"-\"&N101&\"-\"&O101&\"-\"&S101&\"-\"&#REF!&\"-\"&T101&\"-\"&U101&\"-\"&V101&\"-\"&W101","v":{"$error":"#REF!"}}]
["RD",103,"D",null,4,4,16,140,50,null,null,"РА","М",50,25,null,null,null,3,1.6,1,150,"У1",null,null,{"$f":"L102&\" \"&M102&\"-\"&#REF!&\"-\"&N102&\"-\"&O102&\"-\"&P102&\"-\"&#REF!&\"-\"&T102&\"-\"&U102&\"-\"&V102&\"-\"&W102","v":{"$error":"#REF!"}},{"$f":"L102&\" \"&M102&\"-\"&#REF!&\"-\"&N102&\"-\"&O102&\"-\"&Q102&\"-\"&#REF!&\"-\"&T102&\"-\"&U102&\"-\"&V102&\"-\"&W102","v":{"$error":"#REF!"}},null,0.68,{"$f":"L102&\" \"&M102&\"-\"&#REF!&\"-\"&N102&\"-\"&O102&\"-\"&S102&\"-\"&#REF!&\"-\"&T102&\"-\"&U102&\"-\"&V102&\"-\"&W102","v":{"$error":"#REF!"}}]

{"sheet":"Привода","index":37,"n_rows":36,"n_cols":25,"rows_kept":36,"cut":false,"hidden":false,"merged":[[11,0,11,1],[11,2,11,9],[11,10,11,12],[11,13,11,24],[12,0,12,1],[12,13,12,15],[12,16,12,19],[12,20,12,21],[12,22,12,23],[13,0,14,0],[15,0,17,0],[18,2,18,5],[18,6,18,7],[18,8,18,9],[18,13,18,15],[18,16,18,19],[18,20,18,21],[18,22,18,23],[19,2,19,5],[19,6,19,7],[19,8,19,9],[19,11,19,12],[19,13,19,15],[19,16,19,17],[18,11,18,12],[29,0,29,1],[19,18,19,19],[19,20,19,21],[19,22,19,23],[21,0,21,1],[22,0,22,1],[23,0,23,1],[24,0,24,1],[25,0,25,1],[26,0,26,1],[27,0,27,1],[28,0,28,1],[35,0,35,1],[34,0,34,1],[33,0,33,1],[32,0,32,1],[30,0,30,1],[31,0,31,1]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Производитель",null,"AUMA",null,null,null,null,null,null,null,"SAUTER",null,null,"REGADA"]
["Тип привода",null,"ES 05-11","ES 05-11/E","ES 05-12","ES 05-12/E","ES 06-4","ES06-4/E","ES 08","ES 08/E","AVM 322","AVM 234","AVF 234","ST mini",null,null,"ST 0",null,null,null,"ST 0,1",null,"ST 1",null,"ST 2"]
["Тип управления","трехточечный","+",null,"+",null,"+",null,"+",null,"+","+","+","+","+","+","+","+","+","+","+","+","+","+","+"]
[null,"аналоговый",null,"+",null,"+",null,"+",null,"+","+","+","+"]
["Обратная связь","0-100 Ом",null,null,null,null,null,null,null,null,null,null,null,null,"+",null,null,null,"+",null,"+",null,"+",null,"+"]
[null,"0-10 В",null,"+",null,"+",null,"+",null,"+"]
[null,"4-20 мА",null,null,null,null,null,null,null,"+","+","+","+",null,null,"+",null,null,null,"+",null,"+",null,"+"]
[null,"Скорость, мм/мин","8 / 10",null,null,null,"8 / 10 / 13,2",null,"15/40",null,"10","10/15/30",null,"15",null,null,"16",null,null,null,"16",null,"32",null,"40"]
[null,"Ход штока","30",null,null,null,"40",null,"40/75",null,"20","50",null,"25",null,null,"40",null,"28",null,"50",null,"80",null,"80"]
["DN, мм","Код привода","1.3500","1.3502","1.3501","1.3503","1.3600","1.3601","1.3700","1.3701","1.2300","1.2100","1.2200","1.1100","1.1114","1.1109","1.1200","1.1204","1.1212","1.1213","1.1300","1.1309","1.1400","1.1409","1.1500"]
[15,null,"●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
[20,null,"●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
[25,null,"●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
[32,null,"●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
[40,null,"●","●","●","●","●","●","●","●",null,"●","●","●","●","●","●","●","●","●","●","●"]
[50,null,"●","●","●","●","●","●","●","●",null,"●","●","●","●","●","●","●","●","●","●","●"]
[65,null,null,null,"●","●","●","●","●","●",null,"●","●","●","●","●","●","●","●","●","●","●"]
[80,null,null,null,null,null,"●","●","●","●",null,"●","●",null,null,null,"●","●",null,null,"●","●","●","●"]
[100,null,null,null,null,null,null,null,"●","●",null,"●","●",null,null,null,"●","●",null,null,"●","●","●","●"]
[125,null,null,null,null,null,null,null,"●","●",null,"●","●",null,null,null,null,null,null,null,"●","●","●","●","●"]
[150,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●"]
[200,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●"]
[250,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●"]
[300,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[400,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]

{"sheet":"KVs","index":38,"n_rows":20,"n_cols":43,"rows_kept":20,"cut":false,"hidden":false,"merged":[[18,7,19,42],[1,2,1,6],[1,7,2,42],[2,2,2,6],[4,1,5,1],[4,3,4,6],[5,3,6,6],[7,3,8,6],[8,2,10,2],[9,3,11,6],[11,2,19,2],[12,3,12,6],[13,3,14,6],[15,3,17,6],[18,3,18,6],[19,3,19,6]]}
[]
[null,null,"Ход штока",null,null,null,null,"Условная пропускная способность, Kvу, м³/ч"]
[null,null,"Серия"]
[null,"ДУ, мм",110,100,200,210,220,0.16,0.25,0.4,0.63,1,1.6,2.5,3.2,4,5,6.3,8,10,12.5,16,20,25,32,40,50,63,80,100,125,160,200,250,360,400,450,630,800,1000,1250,1600,2000]
[null,15,5,null,null,null,null,"●","●","●","●","●","●","●","●","●"]
[null,null,null,10,null,null,null,null,null,null,null,null,"●","●",null,"●",null,"●",null,"●"]
[null,20,5,null,null,null,null,null,null,null,null,null,"●","●",null,"●","●","●","●","●"]
[null,25,7,20,null,null,null,null,null,null,null,null,null,null,null,null,null,"●",null,"●",null,"●"]
[null,32,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●",null,"●",null,"●"]
[null,40,null,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●",null,"●","●","●"]
[null,50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●",null,"●","●","●","●","●"]
[null,65,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●",null,null,null,null,null,"●","●","●"]
[null,80,null,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●",null,"●","●","●","●","●"]
[null,100,null,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●",null,"●",null,null,null,null,"●","●","●","●","●"]
[null,125,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●",null,"●","●"]
[null,150,null,75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●",null,"●","●"]
[null,200,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●",null,"●","●","●"]
[null,250,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●"]
[null,300,null,80,null,null,null,"ПО ЗАПРОСУ"]
[null,400,null,100]

{"sheet":"Перепад","index":39,"n_rows":35,"n_cols":19,"rows_kept":35,"cut":false,"hidden":false,"merged":[[24,22,24,28],[25,22,25,23],[25,24,25,28],[26,23,26,28],[33,9,34,9],[33,10,34,10],[33,11,34,11],[27,10,28,10],[27,11,28,11],[27,12,28,12],[33,12,34,12],[33,13,34,13],[27,13,28,13],[27,23,27,28],[28,23,28,24],[28,25,28,28],[29,22,29,24],[29,25,29,28],[29,3,30,3],[33,4,34,5],[33,6,34,6],[33,7,34,7],[33,8,34,8],[27,1,28,1],[27,2,28,2],[27,6,28,6],[27,7,28,7],[27,8,28,8],[23,1,24,1],[23,2,24,2],[23,4,24,4],[23,5,24,5],[23,6,24,6],[25,1,26,1],[25,6,26,6],[25,7,26,7],[25,8,26,8],[25,10,26,10],[20,11,21,11],[20,12,21,12],[23,8,24,8],[23,10,24,10],[25,2,26,2],[23,7,24,7],[25,11,26,11],[25,12,26,12],[11,10,12,10],[17,4,17,5],[17,8,17,9],[16,4,16,9],[18,7,19,7],[18,8,19,8],[11,4,12,4],[11,5,12,5],[11,6,12,6],[11,7,12,7],[11,8,12,8],[11,9,12,9],[4,4,4,7],[10,8,10,9],[5,4,6,4],[5,5,6,5],[5,6,6,6],[5,7,6,7],[16,12,17,12],[16,13,17,13],[22,1,22,18],[31,1,31,18],[32,3,34,3],[20,4,21,5],[20,6,21,6],[20,7,21,7],[18,12,19,12],[20,1,21,1],[20,2,21,2],[16,14,17,14],[20,13,21,13],[20,8,21,8],[20,9,21,9],[20,10,21,10],[16,1,19,1],[16,2,19,2],[3,1,3,18],[4,1,9,1],[4,2,9,2],[6,10,9,10],[6,11,9,11],[10,1,15,1],[10,2,15,2],[12,11,15,11],[5,8,6,8],[5,9,6,9],[16,15,17,15],[16,16,17,16],[16,17,17,17],[16,18,17,18]]}
[]
[null,"Допустимые перепады давления, ΔР, атм"]
[null,"Привод","Усилие, Н","Серия",15,20,25,32,40,50,65,80,100,125,150,200,250,300,400]
[]
[null,"ES05-11 (…/Е)",600,110,16,null,null,null,14,10]
[null,null,null,100,8.5,6.3,4,3.5,1.5]
[null,null,null,220]
[null,null,null,200]
[null,null,null,210]
[null,null,null,220]
[null,"ES05-12 (…/Е)",1000,110,null,null,null,null,16]
[null,null,null,100,14,10.5,6.8,6.2,4,2.8,5]
[null,null,null,220]
[null,null,null,200]
[null,null,null,210]
[null,null,null,220]
[null,"ES06-4 (…/Е)",2000,"110 СЧ",16]
[null,null,null,"110 ВЧ",25,null,20,16,16]
[null,null,null,"100, 200",null,null,13.5,10,9,7,10,8]
[null,null,null,"210, 220",null,null,13,null,null,16,12,10]
[null,"ES08 (…/Е)",4000,"100, 200",30,null,20,12,10,8,18,10,8,6]
[null,null,null,"210, 220"]
[]
[null,"ST mini",1100,"100, 200",15.5,11.6,7.4,6.8,5.8,2.5,8]
[null,null,null,"210, 220",null,null,null,null,null,8]
[null,"ST 0",4500,"100, 200",null,null,20,12,10,8,16,10,8]
[null,null,null,"210, 220",null,null,null,null,null,20]
[null,"ST 0,1",7500,"100, 200",null,null,30,25,18,15,21,16,14,10]
[null,null,null,"210, 220",null,null,null,null,null,25]
[null,"ST 1",8700,"100, 200, 210, 220",null,null,null,null,null,null,null,18,16,12,10,9,8]
[null,"ST 2",21500,null,null,null,null,null,null,null,null,null,null,18,16,14,12,6,4.5]
[]
[null,"AVM 322 S",1000,"100 200 210 220",14,8,7.4,6.2]
[null,"AVM 234 S",2000,null,16,null,13,10,9,6.8,12,8,6,5]
[null,"AVF 234 S ",2000,null,null,null,null,null,9,6.8,12,8,6,5]

{"sheet":"КПСР серия 100","index":40,"n_rows":46,"n_cols":24,"rows_kept":46,"cut":false,"hidden":true,"merged":[[39,0,41,0],[19,0,19,7],[20,2,21,2],[37,9,38,9],[35,2,36,2],[35,1,36,1],[30,1,32,1],[30,2,32,2],[27,9,29,9],[30,9,32,9],[27,0,38,0],[33,2,34,2],[33,1,34,1],[37,1,38,1],[37,2,38,2],[35,9,36,9],[16,0,18,0],[16,1,18,1],[16,2,18,2],[27,1,29,1],[27,2,29,2],[22,2,23,2],[24,2,25,2],[20,0,26,0],[6,3,6,4],[16,9,18,9],[22,9,23,9],[24,9,25,9],[33,9,34,9],[16,8,18,8],[16,3,17,4],[16,5,17,7],[16,10,17,23],[1,6,1,11],[2,6,2,11],[24,5,25,5],[24,7,25,7],[3,6,3,11],[20,9,21,9],[19,10,19,23]]}
[]
[null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Маркировка изделия"]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Клапан КПСР 1- Х - ХХ - Х.ХХХХ - СЧ - 1,6 - 1 - 150 - У"]
[]
["Серия 100",null,null,null,null,null,null,null,null,null,null,"Диаметр изделия",null,null,null,"Код привода"]
["Материал корпуса: Серый чугун (EN-JS 1040)"]
["Рабочее давление: 1,6 МПа (16 атм)",null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность"]
["Рабочая температура: max +150°С"]
[null,null,null,null,null,null,null,null,null,null,"Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[]
[]
["Производитель привода","Марка привода","Макс. усилие, Н","Управление",null,"Обратная связь ②",null,null,"Код привода","ход штока привода","Dn, мм"]
[]
[null,null,null,"трехточечное","аналоговое","1-100 Ω","0-10 v","4-20 mA",null,null,15,20,25,32,40,50,65,80,100,125,150,200,250,300]
[null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
["AUMA","ES 05-11",600,"+",null,null,null,null,"1.3500",30]
[null,"ES 05-11/E",null,null,"+",null,"+",null,"1.3502"]
[null,"ES 05-12",1000,"+",null,null,null,null,"1.3501",30]
[null,"ES 05-12/E",null,null,"+",null,"+",null,"1.3503",null,0.16]
[null,"ES 06-4",2000,"+",null,"②",null,"②","1.3600",35]
[null,"ES 06-4/E",null,null,"+",null,"+",null,"1.3601",null,0.25,null,1.6]
[null,"ES 08",4500,"+",null,null,null,null,"1.3700",null,null,null,null,null,null,10,null,null,63]
["REGADA","ST mini",1100,"+",null,null,null,null,"1.1100",25,0.4,1.6,2.5,null,10,null,25,40,null,100,null,250,400]
[null,null,null,"+",null,"+",null,null,"1.1114",null,null,null,null,6.3,null,16,null,null,80,null,160,null,null,1000]
[null,null,null,"+",null,null,null,"+","1.1109",null,0.63,2.5,4,null,16,null,32,63,null,125,null,360,630]
[null,"ST 0",4500,"+",null,null,null,null,"1.1200",40,null,null,null,10,null,25,null,null,100,null,280,null,null,1250]
[null,null,null,"+",null,"+",null,null,"1.1213",null,1,4,6.3,null,20,null,40,80,null,160,null,450,800]
[null,null,null,"+",null,null,null,"+","1.1212",null,null,null,null,16,null,32,null,null,125,null,360,null,null,1600]
[null,"ST 0.1",7500,"+",null,"+",null,null,"1.1300",50,1.6,6.3,8,null,25,null,63,100,null,250,null,630,1000]
[null,null,null,"+",null,null,null,"+","1.1309",null,null,null,null,null,null,40,null,null,160]
[null,"ST 1",8700,"+",null,"+",null,null,"1.1400",80,2.5,null,10]
[null,null,null,"+",null,null,"+",null,"1.1409"]
[null,"ST 2",21500,"+",null,"+",null,null,"1.1500",80,3.2]
[null,null,null,"+",null,null,"+",null,"1.1509"]
["SAUTER","AVM 322 ",1000,"+","+",null,null,"+","1.2300","20",4]
[null,"AVM 234",2000,"+","+",null,null,"+","1.2100","50"]
[null,"AVF 234 ③",2000,"+","+",null,null,"+","1.2200","50"]
[]
["① - стоимость на изделия Dn>100 предоставляется по запросу и после обработки опросного листа"]
["② - привода ES 06-4 и ES 06-4/E могут комплектоваться датчиками обратной связи 1-100 Ω и 4-20 mA по запросу"]
["③ - привод SAUTER AVF 234 имеет встроенную функцию безопасности при отключении питания (НЗ или НО) "]

{"sheet":"КПСР серия 110","index":41,"n_rows":31,"n_cols":21,"rows_kept":31,"cut":false,"hidden":true,"merged":[[27,6,28,6],[27,8,28,8],[27,9,28,9],[20,3,21,3],[20,4,21,4],[20,5,21,5],[20,6,21,6],[20,7,21,7],[20,8,21,8],[20,9,22,9],[27,7,28,7],[19,10,19,15],[20,0,28,0],[20,2,22,2],[27,1,28,1],[20,1,21,1],[25,5,26,5],[25,7,26,7],[25,9,26,9],[19,0,19,7],[23,2,24,2],[23,9,24,9],[25,2,26,2],[27,2,28,2],[27,3,28,3],[27,4,28,4],[27,5,28,5],[1,6,1,11],[2,6,2,11],[3,6,3,11],[6,3,6,4],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,17,4],[16,5,17,7],[16,8,18,8],[16,10,17,15],[16,9,18,9]]}
[]
[null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Маркировка изделия"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Клапан КПСР 1- Х - ХХ - Х.ХХХХ - СЧ - 1,6 - 1 - 150 - У"]
[]
["Серия 110",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Диаметр изделия",null,null,null,"Код привода"]
["Материал корпуса: Серый чугун (EN-JS 1040), Высокопрочный чугун (EN-JS 1025)"]
["Рабочее давление: 1,6 МПа (16 атм), 2,5 МПа (25 атм)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность"]
["Рабочая температура: +150°С, +220°С"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[]
[]
["Производитель привода","Марка привода","Макс. усилие, Н","Управление",null,"Обратная связь ②",null,null,"Код привода","ход штока привода","Dn, мм"]
[]
[null,null,null,"трехточечное","аналоговое","1-100 Ω","0-10 v","4-20 mA",null,null,15,20,25,32,40,50]
[null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
["AUMA","ES 05-11",600,"+",null,null,null,null,"1.3500",30,0.16]
[null,null,null,null,null,null,null,null,null,null,0.25,null,1.6]
[null,"ES 05-11/E",null,null,"+",null,"+",null,"1.3502",null,0.4,1.6,2.5,null,10,10]
[null,"ES 05-12",1000,"+",null,null,null,null,"1.3501",30,0.63,2.5,4,6.3,16,16]
[null,"ES 05-12/E",null,null,"+",null,"+",null,"1.3503",null,1,4,6.3,10,20,25]
[null,"ES 06-4",2000,"+",null,"②",null,"②","1.3600",35,1.6,6.3,8,16,25,32]
[null,"ES 06-4/E",null,null,"+",null,"+",null,"1.3601",null,2.5,null,10,null,null,40]
[null,"ES 08",4500,"+",null,null,null,null,"1.3700",null,3.2]
[null,null,null,null,null,null,null,null,null,null,4]
[]
["② - привода ES 06-4 и ES 06-4/E могут комплектоваться датчиками обратной связи 1-100 Ω и 4-20 mA по запросу"]

{"sheet":"КПСР серия 200","index":42,"n_rows":46,"n_cols":22,"rows_kept":46,"cut":false,"hidden":true,"merged":[[39,0,41,0],[16,10,17,21],[30,9,32,9],[33,1,34,1],[33,2,34,2],[33,9,34,9],[35,1,36,1],[35,2,36,2],[35,9,36,9],[24,2,25,2],[24,5,25,5],[24,7,25,7],[24,9,25,9],[27,0,38,0],[27,1,29,1],[27,2,29,2],[27,9,29,9],[30,1,32,1],[30,2,32,2],[37,1,38,1],[37,2,38,2],[37,9,38,9],[19,0,19,7],[19,10,19,21],[20,0,26,0],[20,2,21,2],[20,9,21,9],[22,2,23,2],[22,9,23,9],[1,6,1,11],[2,6,2,11],[3,6,3,11],[6,3,6,4],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,17,4],[16,5,17,7],[16,8,18,8],[16,9,18,9]]}
[]
[null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Маркировка изделия"]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Клапан КПСР 1- Х - ХХ - Х.ХХХХ - ВЧ - 2,5 - 1 - 220 - У"]
[]
["Серия 200",null,null,null,null,null,null,null,null,null,null,"Диаметр изделия",null,null,null,"Код привода"]
["Материал корпуса: Высокопрочный чугун (EN-JS 1025)"]
["Рабочее давление: 2,5 МПа (25 атм)",null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность"]
["Рабочая температура: max +220°С"]
[]
[]
[]
["Производитель привода","Марка привода","Макс. усилие, Н","Управление",null,"Обратная связь ②",null,null,"Код привода","ход штока привода","Dn, мм"]
[]
[null,null,null,"трехточечное","аналоговое","1-100 Ω","0-10 v","4-20 mA",null,null,15,20,25,32,40,50,65,80,100,125,150,200]
[null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
["AUMA","ES 05-11",600,"+",null,null,null,null,"1.3500",30]
[null,"ES 05-11/E",null,null,"+",null,"+",null,"1.3502"]
[null,"ES 05-12",1000,"+",null,null,null,null,"1.3501",30]
[null,"ES 05-12/E",null,null,"+",null,"+",null,"1.3503",null,0.16]
[null,"ES 06-4",2000,"+",null,"②",null,"②","1.3600",35]
[null,"ES 06-4/E",null,null,"+",null,"+",null,"1.3601",null,0.25,null,1.6]
[null,"ES 08",4500,"+",null,null,null,null,"1.3700",null,null,null,null,null,null,10,null,null,63]
["REGADA","ST mini",1100,"+",null,null,null,null,"1.1100",25,0.4,1.6,2.5,null,10,null,25,40,null,100,null,250]
[null,null,null,"+",null,"+",null,null,"1.1114",null,null,null,null,6.3,null,16,null,null,80,null,160]
[null,null,null,"+",null,null,null,"+","1.1109",null,0.63,2.5,4,null,16,null,32,63,null,125,null,360]
[null,"ST 0",4500,"+",null,null,null,null,"1.1200",40,null,null,null,10,null,25,null,null,100,null,280]
[null,null,null,"+",null,"+",null,null,"1.1213",null,1,4,6.3,null,20,null,40,80,null,160,null,450]
[null,null,null,"+",null,null,null,"+","1.1212",null,null,null,null,16,null,32,null,null,125,null,360]
[null,"ST 0.1",7500,"+",null,"+",null,null,"1.1300",50,1.6,6.3,8,null,25,null,63,100,null,250,null,630]
[null,null,null,"+",null,null,null,"+","1.1309",null,null,null,null,null,null,40,null,null,160]
[null,"ST 1",8700,"+",null,"+",null,null,"1.1400",80,2.5,null,10]
[null,null,null,"+",null,null,"+",null,"1.1409"]
[null,"ST 2",21500,"+",null,"+",null,null,"1.1500",80,3.2]
[null,null,null,"+",null,null,"+",null,"1.1509"]
["SAUTER","AVM 322 ",1000,"+","+",null,null,"+","1.2300",20,4]
[null,"AVM 234",2000,"+","+",null,null,"+","1.2100",50]
[null,"AVF 234 ③",2000,"+","+",null,null,"+","1.2200",50]
[]
["① - стоимость на изделия Dn>100 предоставляется по запросу и после обработки опросного листа"]
["② - привода ES 06-4 и ES 06-4/E могут комплектоваться датчиками обратной связи 1-100 Ω и 4-20 mA по запросу"]
["③ - привод SAUTER AVF 234 имеет встроенную функцию безопасности при отключении питания (НЗ или НО) "]

{"sheet":"КПСР серия 210","index":43,"n_rows":46,"n_cols":25,"rows_kept":46,"cut":false,"hidden":true,"merged":[[37,1,38,1],[37,2,38,2],[37,9,38,9],[39,0,41,0],[16,10,17,24],[19,10,19,24],[33,1,34,1],[33,2,34,2],[33,9,34,9],[35,1,36,1],[35,2,36,2],[35,9,36,9],[24,5,25,5],[24,7,25,7],[24,9,25,9],[27,0,38,0],[27,1,29,1],[27,2,29,2],[27,9,29,9],[30,1,32,1],[30,2,32,2],[30,9,32,9],[19,0,19,7],[20,0,26,0],[20,2,21,2],[20,9,21,9],[22,2,23,2],[22,9,23,9],[24,2,25,2],[1,6,1,11],[2,6,2,11],[3,6,3,11],[6,3,6,4],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,17,4],[16,5,17,7],[16,8,18,8],[16,9,18,9]]}
[]
[null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Маркировка изделия"]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Клапан КПСР 1- Х - ХХ - Х.ХХХХ - CN - 4,0 - 1 - 260 - У"]
[]
["Серия 200",null,null,null,null,null,null,null,null,null,null,"Диаметр изделия",null,null,null,"Код привода"]
["Материал корпуса: Сталь 20 (GS-C25)"]
["Рабочее давление: 4,0 МПа (40 атм)",null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность"]
["Рабочая температура: max +260°С"]
[]
[]
[]
["Производитель привода","Марка привода","Макс. усилие, Н","Управление",null,"Обратная связь ②",null,null,"Код привода","ход штока привода","Dn, мм"]
[]
[null,null,null,"трехточечное","аналоговое","1-100 Ω","0-10 v","4-20 mA",null,null,15,20,25,32,40,50,65,80,100,125,150,200,250,300,400]
[null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
["AUMA","ES 05-11",600,"+",null,null,null,null,"1.3500",30]
[null,"ES 05-11/E",null,null,"+",null,"+",null,"1.3502"]
[null,"ES 05-12",1000,"+",null,null,null,null,"1.3501",30]
[null,"ES 05-12/E",null,null,"+",null,"+",null,"1.3503",null,0.16]
[null,"ES 06-4",2000,"+",null,"②",null,"②","1.3600",35]
[null,"ES 06-4/E",null,null,"+",null,"+",null,"1.3601",null,0.25,null,1.6]
[null,"ES 08",4500,"+",null,null,null,null,"1.3700",null,null,null,null,null,null,10,null,null,63]
["REGADA","ST mini",1100,"+",null,null,null,null,"1.1100",25,0.4,1.6,2.5,null,10,null,25,40,null,100,null,250,400,null,1250]
[null,null,null,"+",null,"+",null,null,"1.1114",null,null,null,null,6.3,null,16,null,null,80,null,160,null,null,1000]
[null,null,null,"+",null,null,null,"+","1.1109",null,0.63,2.5,4,null,16,null,32,63,null,125,null,360,630,null,1600]
[null,"ST 0",4500,"+",null,null,null,null,"1.1200",40,null,null,null,10,null,25,null,null,100,null,280,null,null,1200]
[null,null,null,"+",null,"+",null,null,"1.1213",null,1,4,6.3,null,20,null,40,80,null,160,null,450,800,null,2000]
[null,null,null,"+",null,null,null,"+","1.1212",null,null,null,null,16,null,32,null,null,125,null,360,null,null,1600]
[null,"ST 0.1",7500,"+",null,"+",null,null,"1.1300",50,1.6,6.3,8,null,25,null,63,100,null,250,null,630,1000,null,2500]
[null,null,null,"+",null,null,null,"+","1.1309",null,null,null,null,null,null,40,null,null,160]
[null,"ST 1",8700,"+",null,"+",null,null,"1.1400",80,2.5,null,10]
[null,null,null,"+",null,null,"+",null,"1.1409"]
[null,"ST 2",21500,"+",null,"+",null,null,"1.1500",80,3.2]
[null,null,null,"+",null,null,"+",null,"1.1509"]
["SAUTER","AVM 322 ",1000,"+","+",null,null,"+","1.2300",20,4]
[null,"AVM 234",2000,"+","+",null,null,"+","1.2100",50]
[null,"AVF 234 ③",2000,"+","+",null,null,"+","1.2200",50]
[]
["① - стоимость на изделия Dn>100 предоставляется по запросу и после обработки опросного листа"]
["② - привода ES 06-4 и ES 06-4/E могут комплектоваться датчиками обратной связи 1-100 Ω и 4-20 mA по запросу"]
["③ - привод SAUTER AVF 234 имеет встроенную функцию безопасности при отключении питания (НЗ или НО) "]

{"sheet":"КССР серия 100","index":44,"n_rows":46,"n_cols":19,"rows_kept":46,"cut":false,"hidden":true,"merged":[[1,6,1,11],[2,6,2,11],[3,6,3,11],[6,3,6,4],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,17,4],[16,5,17,7],[16,8,18,8],[16,9,18,9],[19,0,19,7],[20,0,26,0],[20,2,21,2],[20,9,21,9],[22,2,23,2],[22,9,23,9],[24,2,25,2],[27,1,29,1],[27,2,29,2],[27,9,29,9],[30,1,32,1],[30,2,32,2],[30,9,32,9],[37,1,38,1],[37,2,38,2],[37,9,38,9],[39,0,41,0],[16,10,17,18],[19,10,19,18],[33,1,34,1],[33,2,34,2],[33,9,34,9],[35,1,36,1],[35,2,36,2],[35,9,36,9],[24,5,25,5],[24,7,25,7],[24,9,25,9],[27,0,38,0]]}
[]
[null,null,null,null,null,null,"Номенклатура"]
[null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Маркировка изделия"]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Клапан КССР 1- Х - ХХ - Х.ХХХХ - СЧ - 1,6 - 1 - 150 - У"]
[]
["Серия 100",null,null,null,null,null,null,null,null,null,null,"Диаметр изделия",null,null,null,"Код привода"]
["Материал корпуса: Серый чугун (EN-JS 1040)"]
["Рабочее давление: 1,6 МПа (16 атм)",null,null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность"]
["Рабочая температура: max +150°С"]
[null,null,null,null,null,null,null,null,null,null,"Применяемость приводов к конкретному диаметру уточняйте у сотрудников компании"]
[]
[]
["Производитель привода","Марка привода","Макс. усилие, Н","Управление",null,"Обратная связь ②",null,null,"Код привода","ход штока привода","Dn, мм"]
[]
[null,null,null,"трехточечное","аналоговое","1-100 Ω","0-10 v","4-20 mA",null,null,15,20,25,32,40,50,65,80,100]
[null,null,null,null,null,null,null,null,null,null,"Условная пропускная способность, м³/ч"]
["AUMA","ES 05-11",600,"+",null,null,null,null,"1.3500",30]
[null,"ES 05-11/E",null,null,"+",null,"+",null,"1.3502"]
[null,"ES 05-12",1000,"+",null,null,null,null,"1.3501",30]
[null,"ES 05-12/E",null,null,"+",null,"+",null,"1.3503",null,0.16]
[null,"ES 06-4",2000,"+",null,"②",null,"②","1.3600",35]
[null,"ES 06-4/E",null,null,"+",null,"+",null,"1.3601",null,0.25,null,1.6]
[null,"ES 08",4500,"+",null,null,null,null,"1.3700",null,null,null,null,null,null,10,null,null,63]
["REGADA","ST mini",1100,"+",null,null,null,null,"1.1100",25,0.4,1.6,2.5,null,10,null,25,40]
[null,null,null,"+",null,"+",null,null,"1.1114",null,null,null,null,6.3,null,16,null,null,80]
[null,null,null,"+",null,null,null,"+","1.1109",null,0.63,2.5,4,null,16,null,32,63]
[null,"ST 0",4500,"+",null,null,null,null,"1.1200",40,null,null,null,10,null,25,null,null,100]
[null,null,null,"+",null,"+",null,null,"1.1213",null,1,4,6.3,null,20,null,40,80]
[null,null,null,"+",null,null,null,"+","1.1212",null,null,null,null,16,null,32,null,null,125]
[null,"ST 0.1",7500,"+",null,"+",null,null,"1.1300",50,1.6,6.3,8,null,25,null,63,100]
[null,null,null,"+",null,null,null,"+","1.1309",null,null,null,null,null,null,40,null,null,160]
[null,"ST 1",8700,"+",null,"+",null,null,"1.1400",80,2.5,null,10]
[null,null,null,"+",null,null,"+",null,"1.1409"]
[null,"ST 2",21500,"+",null,"+",null,null,"1.1500",80,3.2]
[null,null,null,"+",null,null,"+",null,"1.1509"]
["SAUTER","AVM 322 ",1000,"+","+",null,null,"+","1.2300","20",4]
[null,"AVM 234",2000,"+","+",null,null,"+","1.2100","50"]
[null,"AVF 234 ③",2000,"+","+",null,null,"+","1.2200","50"]
[]
["① - стоимость на изделия Dn>100 предоставляется по запросу и после обработки опросного листа"]
["② - привода ES 06-4 и ES 06-4/E могут комплектоваться датчиками обратной связи 1-100 Ω и 4-20 mA по запросу"]
["③ - привод SAUTER AVF 234 имеет встроенную функцию безопасности при отключении питания (НЗ или НО) "]

{"sheet":"РА серия 100,200","index":45,"n_rows":36,"n_cols":22,"rows_kept":36,"cut":false,"hidden":true,"merged":[[0,6,0,10],[1,6,1,10],[2,6,2,10],[5,3,5,4],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,18,3],[16,4,18,4],[16,19,18,19],[16,20,18,20],[16,21,18,21],[19,0,35,0],[19,2,35,2],[16,5,17,16],[16,17,18,17],[16,18,18,18],[19,20,35,20],[19,21,35,21],[19,3,35,3],[19,4,35,4],[19,1,35,1],[19,17,35,17],[19,18,35,18],[19,19,35,19]]}
[null,null,null,null,null,null,"ПРАЙС-ЛИСТ "]
[null,null,null,null,null,null,"на продукцию \"КПСР Групп\""]
[null,null,null,null,null,null,"с \"01\" сентября 2016 г."]
[]
[null,null,null,null,null,null,null,null,null,"Маркировка изделия"]
[]
["Регулятор давления",null,null,null,null,null,null,"Регулятор РА - X   DN - KV - Y - XX - T -У"]
["РА",null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура"]
["В комплект поставки входит необходимый \"Монтажный комплект\"",null,null,null,null,null,null,"Тип регулятора"]
["Диапазоны настройки:",null,null,null,null,null,null,null,null,null,null,null,"Материал корпуса "]
[0,"- от 0,01 до 0,1 Мпа (цвет пружины - СЕРЫЙ)",null,null,null,null,null,"Диаметр регулятора"]
[1,"- от 0,04 до 0,16 Мпа (цвет пружины - ЖЕЛТЫЙ)",null,null,null,null,null,null,null,null,null,"Диапазон настройки"]
[2,"- от 0,1 до 0,4 Мпа (цвет пружины - КРАСНЫЙ)",null,null,null,null,null,"Условная пропускная способность"]
[3,"- от 0,3 до 0,7 Мпа (цвет пружины - СИНИЙ)"]
[4,"- от 0,6 до 1,2 Мпа (цвет пружины - ЧЕРНЫЙ)"]
[]
["Серия","Тип регулятора","Метериал корпуса","Рабочее давление, Мпа","Рабочая температура","Dn, мм",null,null,null,null,null,null,null,null,null,null,null,"Рабочая температура","Рабочее давление, Мпа","Метериал корпуса","Тип регулятора","Серия"]
[]
[null,null,null,null,null,15,20,25,32,40,50,65,80,100,125,150,200]
["Серия 100","РА-М          РА-А           РА-В","СЧ",1.6,"+150°С",0.16,null,null,null,null,null,null,null,null,null,null,null,"+220°С",2.5,"ВЧ","РА-А","Серия 200"]
[]
[null,null,null,null,null,0.25,null,1.6]
[null,null,null,null,null,null,null,null,null,null,10,null,null,63]
[null,null,null,null,null,0.4,1.6,2.5,null,10,null,25,40,null,100,null,250]
[null,null,null,null,null,null,null,null,6.3,null,16,null,null,80,null,160]
[null,null,null,null,null,0.63,2.5,4,null,16,null,32,63,null,125,null,360]
[null,null,null,null,null,null,null,null,10,null,25,null,null,100,null,280]
[null,null,null,null,null,1,4,6.3,null,20,null,40,80,null,160,null,450]
[null,null,null,null,null,null,null,null,16,null,32,null,null,125,null,360]
[null,null,null,null,null,1.6,6.3,8,null,25,null,63,100,null,250,null,630]
[null,null,null,null,null,null,null,null,null,null,40,null,null,160]
[null,null,null,null,null,2.5,null,10]
[]
[null,null,null,null,null,3.2]
[]
[null,null,null,null,null,4]